From 3d7de6e870ece5a32153382df9df6fb87613335e Mon Sep 17 00:00:00 2001
From: William Wu <william.wu@rock-chips.com>
Date: Wed, 16 Oct 2024 15:37:13 +0800
Subject: [PATCH] phy: rockchip: inno-usb2: Add usb2 phys support for rk3576

The RK3576 SoC has two independent USB2.0 PHYs, and each PHY has
one port. This adds device specific data for it.

Signed-off-by: William Wu <william.wu@rock-chips.com>
Signed-off-by: Frank Wang <frank.wang@rock-chips.com>
Reviewed-by: Heiko Stuebner <heiko@sntech.de>
Link: https://lore.kernel.org/r/20241016073713.14133-4-frawang.cn@gmail.com
Signed-off-by: Vinod Koul <vkoul@kernel.org>
---
 drivers/phy/rockchip/phy-rockchip-inno-usb2.c | 103 ++++++++++++++++++
 1 file changed, 103 insertions(+)

--- a/drivers/phy/rockchip/phy-rockchip-inno-usb2.c
+++ b/drivers/phy/rockchip/phy-rockchip-inno-usb2.c
@@ -1521,6 +1521,30 @@ static int rk3128_usb2phy_tuning(struct
 				BIT(2) << BIT_WRITEABLE_SHIFT | 0);
 }
 
+static int rk3576_usb2phy_tuning(struct rockchip_usb2phy *rphy)
+{
+	int ret;
+	u32 reg = rphy->phy_cfg->reg;
+
+	/* Deassert SIDDQ to power on analog block */
+	ret = regmap_write(rphy->grf, reg + 0x0010, GENMASK(29, 29) | 0x0000);
+	if (ret)
+		return ret;
+
+	/* Do reset after exit IDDQ mode */
+	ret = rockchip_usb2phy_reset(rphy);
+	if (ret)
+		return ret;
+
+	/* HS DC Voltage Level Adjustment 4'b1001 : +5.89% */
+	ret |= regmap_write(rphy->grf, reg + 0x000c, GENMASK(27, 24) | 0x0900);
+
+	/* HS Transmitter Pre-Emphasis Current Control 2'b10 : 2x */
+	ret |= regmap_write(rphy->grf, reg + 0x0010, GENMASK(20, 19) | 0x0010);
+
+	return ret;
+}
+
 static int rk3588_usb2phy_tuning(struct rockchip_usb2phy *rphy)
 {
 	int ret;
@@ -1949,6 +1973,84 @@ static const struct rockchip_usb2phy_cfg
 	{ /* sentinel */ }
 };
 
+static const struct rockchip_usb2phy_cfg rk3576_phy_cfgs[] = {
+	{
+		.reg = 0x0,
+		.num_ports	= 1,
+		.phy_tuning	= rk3576_usb2phy_tuning,
+		.clkout_ctl	= { 0x0008, 0, 0, 1, 0 },
+		.port_cfgs	= {
+			[USB2PHY_PORT_OTG] = {
+				.phy_sus	= { 0x0000, 8, 0, 0, 0x1d1 },
+				.bvalid_det_en	= { 0x00c0, 1, 1, 0, 1 },
+				.bvalid_det_st	= { 0x00c4, 1, 1, 0, 1 },
+				.bvalid_det_clr = { 0x00c8, 1, 1, 0, 1 },
+				.ls_det_en	= { 0x00c0, 0, 0, 0, 1 },
+				.ls_det_st	= { 0x00c4, 0, 0, 0, 1 },
+				.ls_det_clr	= { 0x00c8, 0, 0, 0, 1 },
+				.disfall_en	= { 0x00c0, 6, 6, 0, 1 },
+				.disfall_st	= { 0x00c4, 6, 6, 0, 1 },
+				.disfall_clr	= { 0x00c8, 6, 6, 0, 1 },
+				.disrise_en	= { 0x00c0, 5, 5, 0, 1 },
+				.disrise_st	= { 0x00c4, 5, 5, 0, 1 },
+				.disrise_clr	= { 0x00c8, 5, 5, 0, 1 },
+				.utmi_avalid	= { 0x0080, 1, 1, 0, 1 },
+				.utmi_bvalid	= { 0x0080, 0, 0, 0, 1 },
+				.utmi_ls	= { 0x0080, 5, 4, 0, 1 },
+			}
+		},
+		.chg_det = {
+			.cp_det		= { 0x0080, 8, 8, 0, 1 },
+			.dcp_det	= { 0x0080, 8, 8, 0, 1 },
+			.dp_det		= { 0x0080, 9, 9, 1, 0 },
+			.idm_sink_en	= { 0x0010, 5, 5, 1, 0 },
+			.idp_sink_en	= { 0x0010, 5, 5, 0, 1 },
+			.idp_src_en	= { 0x0010, 14, 14, 0, 1 },
+			.rdm_pdwn_en	= { 0x0010, 14, 14, 0, 1 },
+			.vdm_src_en	= { 0x0010, 7, 6, 0, 3 },
+			.vdp_src_en	= { 0x0010, 7, 6, 0, 3 },
+		},
+	},
+	{
+		.reg = 0x2000,
+		.num_ports	= 1,
+		.phy_tuning	= rk3576_usb2phy_tuning,
+		.clkout_ctl	= { 0x2008, 0, 0, 1, 0 },
+		.port_cfgs	= {
+			[USB2PHY_PORT_OTG] = {
+				.phy_sus	= { 0x2000, 8, 0, 0, 0x1d1 },
+				.bvalid_det_en	= { 0x20c0, 1, 1, 0, 1 },
+				.bvalid_det_st	= { 0x20c4, 1, 1, 0, 1 },
+				.bvalid_det_clr = { 0x20c8, 1, 1, 0, 1 },
+				.ls_det_en	= { 0x20c0, 0, 0, 0, 1 },
+				.ls_det_st	= { 0x20c4, 0, 0, 0, 1 },
+				.ls_det_clr	= { 0x20c8, 0, 0, 0, 1 },
+				.disfall_en	= { 0x20c0, 6, 6, 0, 1 },
+				.disfall_st	= { 0x20c4, 6, 6, 0, 1 },
+				.disfall_clr	= { 0x20c8, 6, 6, 0, 1 },
+				.disrise_en	= { 0x20c0, 5, 5, 0, 1 },
+				.disrise_st	= { 0x20c4, 5, 5, 0, 1 },
+				.disrise_clr	= { 0x20c8, 5, 5, 0, 1 },
+				.utmi_avalid	= { 0x2080, 1, 1, 0, 1 },
+				.utmi_bvalid	= { 0x2080, 0, 0, 0, 1 },
+				.utmi_ls	= { 0x2080, 5, 4, 0, 1 },
+			}
+		},
+		.chg_det = {
+			.cp_det		= { 0x2080, 8, 8, 0, 1 },
+			.dcp_det	= { 0x2080, 8, 8, 0, 1 },
+			.dp_det		= { 0x2080, 9, 9, 1, 0 },
+			.idm_sink_en	= { 0x2010, 5, 5, 1, 0 },
+			.idp_sink_en	= { 0x2010, 5, 5, 0, 1 },
+			.idp_src_en	= { 0x2010, 14, 14, 0, 1 },
+			.rdm_pdwn_en	= { 0x2010, 14, 14, 0, 1 },
+			.vdm_src_en	= { 0x2010, 7, 6, 0, 3 },
+			.vdp_src_en	= { 0x2010, 7, 6, 0, 3 },
+		},
+	},
+	{ /* sentinel */ }
+};
+
 static const struct rockchip_usb2phy_cfg rk3588_phy_cfgs[] = {
 	{
 		.reg = 0x0000,
@@ -2120,6 +2222,7 @@ static const struct of_device_id rockchi
 	{ .compatible = "rockchip,rk3366-usb2phy", .data = &rk3366_phy_cfgs },
 	{ .compatible = "rockchip,rk3399-usb2phy", .data = &rk3399_phy_cfgs },
 	{ .compatible = "rockchip,rk3568-usb2phy", .data = &rk3568_phy_cfgs },
+	{ .compatible = "rockchip,rk3576-usb2phy", .data = &rk3576_phy_cfgs },
 	{ .compatible = "rockchip,rk3588-usb2phy", .data = &rk3588_phy_cfgs },
 	{ .compatible = "rockchip,rv1108-usb2phy", .data = &rv1108_phy_cfgs },
 	{}
