--- a/arch/arm64/boot/dts/allwinner/sun50i-h616-cpu-opp.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h616-cpu-opp.dtsi
@@ -100,11 +100,9 @@
 
 		opp-1512000000 {
 			opp-hz = /bits/ 64 <1512000000>;
-			opp-microvolt-speed1 = <1100000>;
-			opp-microvolt-speed3 = <1100000>;
-			opp-microvolt-speed5 = <1160000>;
+			opp-microvolt = <1100000>;
 			clock-latency-ns = <244144>; /* 8 32k periods */
-			opp-supported-hw = <0x2a>;
+			opp-supported-hw = <0x2b>;
 		};
 	};
 };
