From 3a92ee5a97f030bdb1e88272a5d277ecb76836d6 Mon Sep 17 00:00:00 2001
From: Zoltan HERPAI <wigyori@uid0.hu>
Date: Sun, 1 Jun 2025 14:03:30 +0000
Subject: [PATCH 7/8] riscv: dts: starfive: visionfive2: add SYSLED support

A SYS LED is available at aongpio-3. Add standard heartbeat
support for it.

Signed-off-by: Zoltan HERPAI <wigyori@uid0.hu>
---
 .../dts/starfive/jh7110-starfive-visionfive-2.dtsi   | 12 ++++++++++++
 1 file changed, 12 insertions(+)

--- a/arch/riscv/boot/dts/starfive/jh7110-starfive-visionfive-2.dtsi
+++ b/arch/riscv/boot/dts/starfive/jh7110-starfive-visionfive-2.dtsi
@@ -21,6 +21,18 @@
 			reg = <0x0 0x6ce00000 0x0 0x1600000>;
 		};
 	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		led-ack {
+			gpios = <&aongpio 3 GPIO_ACTIVE_HIGH>;
+			color = <LED_COLOR_ID_GREEN>;
+			function = LED_FUNCTION_HEARTBEAT;
+			linux,default-trigger = "heartbeat";
+			label = "ack";
+		};
+	};
 };
 
 &gmac0 {
