// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "elecom,wrc-x1800gs", "mediatek,mt7621-soc";
	model = "ELECOM WRC-X1800GS";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_red;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
		label-mac-device = &gmac0;
	};

	chosen {
		bootargs-override = "console=ttyS0,115200n8";
	};

	leds {
		compatible = "gpio-leds";

		/* available on 1st HW rev. */
		led-0 {
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN_2GHZ;
			function-enumerator = <1>;
			linux,default-trigger = "phy0tpt";
		};

		led_power_green: led-1 {
			gpios = <&gpio 3 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_POWER;
		};

		led_power_red: led-2 {
			gpios = <&gpio 4 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_POWER;
		};

		led-3 {
			gpios = <&gpio 5 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_WLAN_2GHZ;
		};

		led-4 {
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_WPS;
		};

		led-5 {
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN_5GHZ;
			linux,default-trigger = "phy1tpt";
		};

		/* available on 2nd HW rev. */
		led-6 {
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN_2GHZ;
			function-enumerator = <2>;
			linux,default-trigger = "phy0tpt";
		};

		led-7 {
			gpios = <&gpio 17 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_WLAN_5GHZ;
		};

	};

	keys {
		compatible = "gpio-keys";

		button-reset {
			label = "reset";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		switch-ap {
			label = "ap";
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
		};

		switch-router {
			label = "router";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_1>;
		};

		button-wps {
			label = "wps";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};
};

&nand {
	status = "okay";
	pinctrl-0 = <&nand_pins>;
	pinctrl-names = "default";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			reg = <0x0 0x100000>;
			label = "u-boot";
			read-only;
		};

		partition@100000 {
			reg = <0x100000 0x100000>;
			label = "u-boot-env";
		};

		partition@200000 {
			reg = <0x200000 0x1c0000>;
			label = "factory";
			read-only;

			nvmem-layout {
				compatible = "fixed-layout";
				#address-cells = <1>;
				#size-cells = <1>;

				eeprom_factory_0: eeprom@0 {
					reg = <0x0 0xe00>;
				};

				precal_factory_e10: precal@e10 {
					reg = <0xe10 0x19c10>;
				};

				macaddr_factory_1fdf4: macaddr@1fdf4 {
					reg = <0x1fdf4 0x6>;
				};

				macaddr_factory_1fdfa: macaddr@1fdfa {
					reg = <0x1fdfa 0x6>;
				};
			};
		};

		/* "RAS1" on stock fw */
		partition@3c0000 {
			compatible = "fixed-partitions";
			reg = <0x3c0000 0x3240000>;
			label = "firmware";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				reg = <0x0 0x800000>;
				label = "kernel";
			};

			partition@800000 {
				reg = <0x800000 0x2a40000>;
				label = "ubi";
			};
		};

		partition@3600000 {
			reg = <0x3600000 0x100000>;
			label = "Config";
			read-only;
		};

		/* "RAS2" on stock fw */
		partition@3700000 {
			reg = <0x3700000 0x3240000>;
			label = "firmware2";
		};

		partition@6940000 {
			reg = <0x6940000 0x100000>;
			label = "Config_2";
			read-only;
		};

		partition@6a40000 {
			reg = <0x6a40000 0x100000>;
			label = "persist";
		};

		partition@6b40000 {
			reg = <0x6b40000 0x100000>;
			label = "mesh";
			read-only;
		};

		partition@6c40000 {
			reg = <0x6c40000 0x1340000>;
			label = "backup";
			read-only;
		};
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_factory_1fdfa>;
	nvmem-cell-names = "mac-address";
};

&gmac1 {
	status = "okay";
	label = "wan";
	phy-handle = <&ethphy0>;

	nvmem-cells = <&macaddr_factory_1fdf4>;
	nvmem-cell-names = "mac-address";
};

&ethphy0 {
	/delete-property/ interrupts;
};

&pcie {
	status = "okay";
};

&pcie1 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&eeprom_factory_0>, <&precal_factory_e10>;
		nvmem-cell-names = "eeprom", "precal";
		mediatek,disable-radar-background;
	};
};

&pcie2 {
	status = "disabled";
};

&switch0 {
	ports {
		port@1 {
			status = "okay";
			label = "lan2";
		};

		port@2 {
			status = "okay";
			label = "lan1";
		};
	};
};

&state_default {
	gpio {
		groups = "i2c", "uart3", "jtag", "wdt";
		function = "gpio";
	};
};
