#include "vr9.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/mips/lantiq_rcu_gphy.h>

/ {
	compatible = "arcadyan,arv7519rw22", "lantiq,xway", "lantiq,vr9";
	model = "Orange Livebox 2.1";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_green;
		led-running = &power_green;
		led-upgrade = &power_green;

		led-dsl = &internet_green;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x8000000>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		reset {
			label = "reset";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
		rfkill {
			label = "rfkill";
			gpios = <&gpio 33 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
		};
		wps {
			label = "wps";
			gpios = <&gpio 37 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";

		lan_green {
			function = LED_FUNCTION_LAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};
		internet_red {
			label = "red:internet";
			gpios = <&gpio 10 GPIO_ACTIVE_LOW>;
		};
		power_green: power_green {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		alarm_blue {
			function = LED_FUNCTION_ALARM;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};
		internet_orange {
			label = "orange:internet";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
		};
		internet_green: internet_green {
			label = "green:internet";
			gpios = <&gpio 28 GPIO_ACTIVE_LOW>;
		};
		voice_green {
			label = "green:voice";
			gpios = <&gpio 29 GPIO_ACTIVE_LOW>;
		};
	};

	usb_vbus: regulator-usb-vbus {
		compatible = "regulator-fixed";

		regulator-name = "USB_VBUS";

		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;

		gpios = <&gpio 32 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};
};

&eth0 {
	nvmem-cells = <&macaddr_boardconfig_16 0>;
	nvmem-cell-names = "mac-address";
};

&ppe {
	nvmem-cells = <&macaddr_boardconfig_16 1>;
	nvmem-cell-names = "mac-address";
};

&gphy0 {
	lantiq,gphy-mode = <GPHY_MODE_FE>;
};

&gphy1 {
	lantiq,gphy-mode = <GPHY_MODE_FE>;
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
		pcie-rst {
			lantiq,pins = "io21";
			lantiq,pull = <0>;
			lantiq,output = <1>;
		};
	};
};

&gswip {
	pinctrl-0 = <&mdio_pins>;
	pinctrl-names = "default";
};

&gswip_mdio {
	phy0: ethernet-phy@0 {
		reg = <0x0>;
	};
	phy11: ethernet-phy@11 {
		reg = <0x11>;
	};
	phy12: ethernet-phy@12 {
		reg = <0x12>;
	};
	phy13: ethernet-phy@13 {
		reg = <0x13>;
	};
	phy14: ethernet-phy@14 {
		reg = <0x14>;
	};
};

&gswip_ports {
	port@0 {
		reg = <0>;
		label = "lan5";
		phy-mode = "rgmii";
		phy-handle = <&phy0>;
	};
	port@2 {
		reg = <2>;
		label = "lan3";
		phy-mode = "internal";
		phy-handle = <&phy11>;
	};
	port@3 {
		reg = <3>;
		label = "lan4";
		phy-mode = "internal";
		phy-handle = <&phy12>;
	};
	port@4 {
		reg = <4>;
		label = "lan1";
		phy-mode = "internal";
		phy-handle = <&phy13>;
	};
	port@5 {
		reg = <5>;
		label = "lan2";
		phy-mode = "internal";
		phy-handle = <&phy14>;
	};
};

&localbus {
	flash@0 {
		compatible = "lantiq,nor";
		bank-width = <2>;
		reg = <0 0x0 0x2000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "uboot";
				reg = <0x0 0x60000>;
				read-only;
			};

			partition@60000 {
				label = "u-boot-env";
				reg = <0x60000 0x20000>;
				read-only;
			};

			partition@80000 {
				label = "firmware";
				reg = <0x80000 0x1f00000>;
			};

			boardconfig: partition@1f80000 {
				label = "boardconfig";
				reg = <0x1f80000 0x80000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_boardconfig_16: macaddr@16 {
						compatible = "mac-base";
						reg = <0x16 0x6>;
						#nvmem-cell-cells = <1>;
					};
				};
			};
		};
	};
};

&pcie0 {
	status = "okay";
	gpio-reset = <&gpio 21 GPIO_ACTIVE_HIGH>;
};

&usb_phy0 {
	status = "okay";
};

&usb_phy1 {
	status = "okay";
};

&usb0 {
	status = "okay";
	vbus-supply = <&usb_vbus>;
};

&usb1 {
	status = "okay";
	vbus-supply = <&usb_vbus>;
};
