From 2795c8b31a686bdb8338f9404d18ef7a154f0d75 Mon Sep 17 00:00:00 2001
From: David Bauer <mail@david-bauer.net>
Date: Sun, 26 Jul 2020 13:32:59 +0200
Subject: [PATCH] arm64: rockchip: add OF node for USB eth on NanoPi R2S

This adds the OF node for the USB3 ethernet adapter on the FriendlyARM
NanoPi R2S. Add the correct value for the RTL8153 LED configuration
register to match the blink behavior of the other port on the device.

Signed-off-by: David Bauer <mail@david-bauer.net>
---
 arch/arm64/boot/dts/rockchip/rk3328-nanopi-r2s.dts | 7 +++++++
 1 file changed, 7 insertions(+)

--- a/arch/arm64/boot/dts/rockchip/rk3328-nanopi-r2c.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3328-nanopi-r2c.dts
@@ -35,6 +35,29 @@
 			reset-assert-us = <10000>;
 			reset-deassert-us = <50000>;
 			reset-gpios = <&gpio1 RK_PC2 GPIO_ACTIVE_LOW>;
+
+			leds {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				led@1 {
+					reg = <1>;
+					color = <LED_COLOR_ID_AMBER>;
+					function = LED_FUNCTION_WAN;
+					default-state = "keep";
+				};
+
+				led@2 {
+					reg = <2>;
+					color = <LED_COLOR_ID_GREEN>;
+					function = LED_FUNCTION_WAN;
+					default-state = "keep";
+				};
+			};
 		};
 	};
 };
+
+&rtl8153 {
+	realtek,led-data = <0x78>;
+};
--- a/arch/arm64/boot/dts/rockchip/rk3328-nanopi-r2s.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3328-nanopi-r2s.dts
@@ -410,9 +410,11 @@
 	#size-cells = <0>;
 
 	/* Second port is for USB 3.0 */
-	rtl8153: device@2 {
-		compatible = "usbbda,8153";
+	rtl8153: usb-eth@2 {
+		compatible = "realtek,rtl8153";
 		reg = <2>;
+
+		realtek,led-data = <0x87>;
 	};
 };
 
--- a/arch/arm64/boot/dts/rockchip/rk3328-orangepi-r1-plus.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3328-orangepi-r1-plus.dts
@@ -363,9 +363,11 @@
 	#size-cells = <0>;
 
 	/* Second port is for USB 3.0 */
-	rtl8153: device@2 {
-		compatible = "usbbda,8153";
+	rtl8153: usb-eth@2 {
+		compatible = "realtek,rtl8153";
 		reg = <2>;
+
+		realtek,led-data = <0x87>;
 	};
 };
 
--- a/arch/arm64/boot/dts/rockchip/rk3328-orangepi-r1-plus-lts.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3328-orangepi-r1-plus-lts.dts
@@ -39,6 +39,29 @@
 			reset-assert-us = <15000>;
 			reset-deassert-us = <50000>;
 			reset-gpios = <&gpio1 RK_PC2 GPIO_ACTIVE_LOW>;
+
+			leds {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				led@1 {
+					reg = <1>;
+					color = <LED_COLOR_ID_AMBER>;
+					function = LED_FUNCTION_WAN;
+					default-state = "keep";
+				};
+
+				led@2 {
+					reg = <2>;
+					color = <LED_COLOR_ID_GREEN>;
+					function = LED_FUNCTION_WAN;
+					default-state = "keep";
+				};
+			};
 		};
 	};
 };
+
+&rtl8153 {
+	realtek,led-data = <0x78>;
+};
--- a/arch/arm64/boot/dts/rockchip/rk3399-nanopi-r4s.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3399-nanopi-r4s.dts
@@ -82,6 +82,19 @@
 &pcie0 {
 	num-lanes = <1>;
 	vpcie3v3-supply = <&vcc3v3_sys>;
+
+	pcie@0 {
+		reg = <0x00000000 0 0 0 0>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		pcie-eth@0,0 {
+			compatible = "pci10ec,8168";
+			reg = <0x000000 0 0 0 0>;
+
+			realtek,led-data = <0x870>;
+		};
+	};
 };
 
 &pinctrl {
--- a/arch/arm64/boot/dts/rockchip/rk3528-radxa-e20c.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3528-radxa-e20c.dts
@@ -259,6 +259,25 @@
 		reset-assert-us = <20000>;
 		reset-deassert-us = <100000>;
 		reset-gpios = <&gpio4 RK_PC2 GPIO_ACTIVE_LOW>;
+
+		leds {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			led@1 {
+				reg = <1>;
+				color = <LED_COLOR_ID_AMBER>;
+				function = LED_FUNCTION_LAN;
+				default-state = "keep";
+			};
+
+			led@2 {
+				reg = <2>;
+				color = <LED_COLOR_ID_GREEN>;
+				function = LED_FUNCTION_LAN;
+				default-state = "keep";
+			};
+		};
 	};
 };
 
@@ -268,6 +287,18 @@
 	reset-gpios = <&gpio1 RK_PA2 GPIO_ACTIVE_HIGH>;
 	vpcie3v3-supply = <&vcc_3v3>;
 	status = "okay";
+
+	pcie@0,0 {
+		reg = <0x000000 0 0 0 0>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		rtl8168: pcie-eth@0,0 {
+			compatible = "pci10ec,8168";
+			reg = <0x000000 0 0 0 0>;
+			realtek,led-data = <0x87>;
+		};
+	};
 };
 
 &pinctrl {
--- a/arch/arm64/boot/dts/rockchip/rk3566-nanopi-r3s.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3566-nanopi-r3s.dts
@@ -417,6 +417,25 @@
 		reset-assert-us = <20000>;
 		reset-deassert-us = <100000>;
 		reset-gpios = <&gpio4 RK_PC2 GPIO_ACTIVE_LOW>;
+
+		leds {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			led@1 {
+				reg = <1>;
+				color = <LED_COLOR_ID_AMBER>;
+				function = LED_FUNCTION_WAN;
+				default-state = "keep";
+			};
+
+			led@2 {
+				reg = <2>;
+				color = <LED_COLOR_ID_GREEN>;
+				function = LED_FUNCTION_WAN;
+				default-state = "keep";
+			};
+		};
 	};
 };
 
@@ -425,6 +444,18 @@
 	pinctrl-0 = <&pcie_reset_h>;
 	reset-gpios = <&gpio4 RK_PC6 GPIO_ACTIVE_HIGH>;
 	status = "okay";
+
+	pcie@0,0 {
+		reg = <0x00000000 0 0 0 0>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		rtl8168: pcie-eth@1,0 {
+			compatible = "pci10ec,8168";
+			reg = <0x000000 0 0 0 0>;
+			realtek,led-data = <0x870>;
+		};
+	};
 };
 
 &pinctrl {
--- a/arch/arm64/boot/dts/rockchip/rk3568-easepi-r1.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3568-easepi-r1.dts
@@ -465,6 +465,25 @@
 		reset-assert-us = <20000>;
 		reset-deassert-us = <100000>;
 		reset-gpios = <&gpio2 RK_PD3 GPIO_ACTIVE_LOW>;
+
+		leds {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			led@0 {
+				reg = <0>;
+				color = <LED_COLOR_ID_AMBER>;
+				function = LED_FUNCTION_WAN;
+				default-state = "keep";
+			};
+
+			led@2 {
+				reg = <2>;
+				color = <LED_COLOR_ID_GREEN>;
+				function = LED_FUNCTION_WAN;
+				default-state = "keep";
+			};
+		};
 	};
 };
 
@@ -477,6 +496,25 @@
 		reset-assert-us = <20000>;
 		reset-deassert-us = <100000>;
 		reset-gpios = <&gpio2 RK_PD1 GPIO_ACTIVE_LOW>;
+
+		leds {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			led@0 {
+				reg = <0>;
+				color = <LED_COLOR_ID_AMBER>;
+				function = LED_FUNCTION_LAN;
+				default-state = "keep";
+			};
+
+			led@2 {
+				reg = <2>;
+				color = <LED_COLOR_ID_GREEN>;
+				function = LED_FUNCTION_LAN;
+				default-state = "keep";
+			};
+		};
 	};
 };
 
@@ -485,6 +523,19 @@
 	reset-gpios = <&gpio3 RK_PA4 GPIO_ACTIVE_HIGH>;
 	vpcie3v3-supply = <&vcc3v3_sys>;
 	status = "okay";
+
+	pcie@0,0 {
+		reg = <0x00000000 0 0 0 0>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		pcie-eth@1,0 {
+			compatible = "pci10ec,8125";
+			reg = <0x000000 0 0 0 0>;
+
+			realtek,led-data = <0x0 0x0 0x200 0x2b>;
+		};
+	};
 };
 
 &pcie30phy {
@@ -498,6 +549,19 @@
 	reset-gpios = <&gpio3 RK_PA3 GPIO_ACTIVE_HIGH>;
 	vpcie3v3-supply = <&vcc3v3_sys>;
 	status = "okay";
+
+	pcie@0,0 {
+		reg = <0x00100000 0 0 0 0>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		pcie-eth@10,0 {
+			compatible = "pci10ec,8125";
+			reg = <0x000000 0 0 0 0>;
+
+			realtek,led-data = <0x0 0x0 0x200 0x2b>;
+		};
+	};
 };
 
 /* M.2 Key for 2280 NVMe */
--- a/arch/arm64/boot/dts/rockchip/rk3568-fastrhino-r66s.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3568-fastrhino-r66s.dtsi
@@ -369,6 +369,19 @@
 	reset-gpios = <&gpio0 RK_PC3 GPIO_ACTIVE_HIGH>;
 	vpcie3v3-supply = <&vcc3v3_pcie>;
 	status = "okay";
+
+	pcie@0,0 {
+		reg = <0x00100000 0 0 0 0>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		rtl8125_1: pcie-eth@10,0 {
+			compatible = "pci10ec,8125";
+			reg = <0x000000 0 0 0 0>;
+
+			realtek,led-data = <0x200 0x2b 0x0 0x0>;
+		};
+	};
 };
 
 &pcie3x2 {
@@ -376,6 +389,19 @@
 	reset-gpios = <&gpio0 RK_PC6 GPIO_ACTIVE_HIGH>;
 	vpcie3v3-supply = <&vcc3v3_pcie>;
 	status = "okay";
+
+	pcie@0,0 {
+		reg = <0x00200000 0 0 0 0>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		rtl8125_2: pcie-eth@20,0 {
+			compatible = "pci10ec,8125";
+			reg = <0x000000 0 0 0 0>;
+
+			realtek,led-data = <0x200 0x2b 0x0 0x0>;
+		};
+ 	};
 };
 
 &pinctrl {
--- a/arch/arm64/boot/dts/rockchip/rk3568-fastrhino-r68s.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3568-fastrhino-r68s.dts
@@ -31,6 +31,7 @@
 	assigned-clock-parents = <&cru SCLK_GMAC0_RGMII_SPEED>;
 	assigned-clock-rates = <0>, <125000000>;
 	clock_in_out = "output";
+	label = "eth0";
 	phy-handle = <&rgmii_phy0>;
 	phy-mode = "rgmii-id";
 	pinctrl-names = "default";
@@ -47,6 +48,7 @@
 	assigned-clock-parents = <&cru SCLK_GMAC1_RGMII_SPEED>;
 	assigned-clock-rates = <0>, <125000000>;
 	clock_in_out = "output";
+	label = "eth1";
 	phy-handle = <&rgmii_phy1>;
 	phy-mode = "rgmii-id";
 	pinctrl-names = "default";
@@ -67,6 +69,25 @@
 		reset-assert-us = <20000>;
 		reset-deassert-us = <100000>;
 		reset-gpios = <&gpio1 RK_PB0 GPIO_ACTIVE_LOW>;
+
+		leds {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			led@1 {
+				reg = <1>;
+				color = <LED_COLOR_ID_GREEN>;
+				function = LED_FUNCTION_LAN;
+				default-state = "keep";
+			};
+
+			led@2 {
+				reg = <2>;
+				color = <LED_COLOR_ID_AMBER>;
+				function = LED_FUNCTION_LAN;
+				default-state = "keep";
+			};
+		};
 	};
 };
 
@@ -79,6 +100,25 @@
 		reset-assert-us = <20000>;
 		reset-deassert-us = <100000>;
 		reset-gpios = <&gpio1 RK_PB1 GPIO_ACTIVE_LOW>;
+
+		leds {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			led@1 {
+				reg = <1>;
+				color = <LED_COLOR_ID_GREEN>;
+				function = LED_FUNCTION_LAN;
+				default-state = "keep";
+			};
+
+			led@2 {
+				reg = <2>;
+				color = <LED_COLOR_ID_AMBER>;
+				function = LED_FUNCTION_LAN;
+				default-state = "keep";
+			};
+		};
 	};
 };
 
@@ -100,6 +140,14 @@
 	vccio3-supply = <&vcc_3v3>;
 };
 
+&rtl8125_1 {
+	label = "eth3";
+};
+
+&rtl8125_2 {
+	label = "eth2";
+};
+
 &sdhci {
 	bus-width = <8>;
 	max-frequency = <200000000>;
--- a/arch/arm64/boot/dts/rockchip/rk3568-nanopi-r5c.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3568-nanopi-r5c.dts
@@ -69,6 +69,19 @@
 	reset-gpios = <&gpio0 RK_PA0 GPIO_ACTIVE_HIGH>;
 	vpcie3v3-supply = <&vcc3v3_pcie>;
 	status = "okay";
+
+	pcie@0,0 {
+		reg = <0x00100000 0 0 0 0>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		rtl8125_1: pcie-eth@10,0 {
+			compatible = "pci10ec,8125";
+			reg = <0x000000 0 0 0 0>;
+
+			realtek,led-data = <0x0 0x0 0x2b 0x200>;
+		};
+ 	};
 };
 
 &pcie3x2 {
@@ -76,6 +89,19 @@
 	reset-gpios = <&gpio0 RK_PB6 GPIO_ACTIVE_HIGH>;
 	vpcie3v3-supply = <&vcc3v3_pcie>;
 	status = "okay";
+
+	pcie@0,0 {
+		reg = <0x00200000 0 0 0 0>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		rtl8125_2: pcie-eth@20,0 {
+			compatible = "pci10ec,8125";
+			reg = <0x000000 0 0 0 0>;
+
+			realtek,led-data = <0x0 0x0 0x2b 0x200>;
+		};
+ 	};
 };
 
 &pinctrl {
--- a/arch/arm64/boot/dts/rockchip/rk3568-nanopi-r5s.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3568-nanopi-r5s.dts
@@ -78,6 +78,25 @@
 		reg = <1>;
 		pinctrl-0 = <&eth_phy0_reset_pin>;
 		pinctrl-names = "default";
+
+		leds {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			led@1 {
+				reg = <1>;
+				color = <LED_COLOR_ID_AMBER>;
+				function = LED_FUNCTION_LAN;
+				default-state = "keep";
+			};
+
+			led@2 {
+				reg = <2>;
+				color = <LED_COLOR_ID_GREEN>;
+				function = LED_FUNCTION_LAN;
+				default-state = "keep";
+			};
+		};
 	};
 };
 
@@ -85,6 +104,19 @@
 	num-lanes = <1>;
 	reset-gpios = <&gpio0 RK_PB6 GPIO_ACTIVE_HIGH>;
 	status = "okay";
+
+	pcie@0,0 {
+		reg = <0x00000000 0 0 0 0>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		rtl8125_1: pcie-eth@1,0 {
+			compatible = "pci10ec,8125";
+			reg = <0x000000 0 0 0 0>;
+
+			realtek,led-data = <0x0 0x0 0x2b 0x200>;
+		};
+	};
 };
 
 &pcie30phy {
@@ -97,6 +129,19 @@
 	reset-gpios = <&gpio0 RK_PA0 GPIO_ACTIVE_HIGH>;
 	vpcie3v3-supply = <&vcc3v3_pcie>;
 	status = "okay";
+
+	pcie@0,0 {
+		reg = <0x00100000 0 0 0 0>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		rtl8125_2: pcie-eth@10,0 {
+			compatible = "pci10ec,8125";
+			reg = <0x000000 0 0 0 0>;
+
+			realtek,led-data = <0x0 0x0 0x2b 0x200>;
+		};
+	};
 };
 
 &pcie3x2 {
--- a/arch/arm64/boot/dts/rockchip/rk3568-photonicat.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3568-photonicat.dts
@@ -3,6 +3,7 @@
 /dts-v1/;
 
 #include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/leds/common.h>
 #include <dt-bindings/pinctrl/rockchip.h>
 #include <dt-bindings/soc/rockchip,vop2.h>
 #include "rk3568.dtsi"
@@ -287,6 +288,7 @@
 &gmac0 {
 	assigned-clocks = <&cru SCLK_GMAC0_RX_TX>;
 	assigned-clock-parents = <&gmac0_xpcsclk>;
+	label = "eth1";
 	power-domains = <&power RK3568_PD_PIPE>;
 	phys = <&combphy2 PHY_TYPE_SGMII>;
 	phy-handle = <&sgmii_phy>;
@@ -305,6 +307,7 @@
 	assigned-clock-parents = <&cru SCLK_GMAC1_RGMII_SPEED>;
 	assigned-clock-rates = <0>, <125000000>;
 	clock_in_out = "output";
+	label = "eth0";
 	phy-handle = <&rgmii_phy>;
 	phy-mode = "rgmii-id";
 	phy-supply = <&vcc_3v3>;
@@ -386,6 +389,25 @@
 		reset-assert-us = <20000>;
 		reset-deassert-us = <100000>;
 		reset-gpios = <&gpio3 RK_PC6 GPIO_ACTIVE_LOW>;
+
+		leds {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			led@1 {
+				reg = <1>;
+				color = <LED_COLOR_ID_AMBER>;
+				function = LED_FUNCTION_LAN;
+				default-state = "keep";
+			};
+
+			led@2 {
+				reg = <2>;
+				color = <LED_COLOR_ID_GREEN>;
+				function = LED_FUNCTION_LAN;
+				default-state = "keep";
+			};
+		};
 	};
 };
 
@@ -398,6 +420,25 @@
 		reset-gpios = <&gpio4 RK_PC0 GPIO_ACTIVE_LOW>;
 		rx-internal-delay-ps = <1500>;
 		tx-internal-delay-ps = <1500>;
+
+		leds {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			led@1 {
+				reg = <1>;
+				color = <LED_COLOR_ID_AMBER>;
+				function = LED_FUNCTION_WAN;
+				default-state = "keep";
+			};
+
+			led@2 {
+				reg = <2>;
+				color = <LED_COLOR_ID_GREEN>;
+				function = LED_FUNCTION_WAN;
+				default-state = "keep";
+			};
+		};
 	};
 };
 
--- a/arch/arm64/boot/dts/rockchip/rk3568-rock-3a.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3568-rock-3a.dts
@@ -591,6 +591,25 @@
 		reset-assert-us = <20000>;
 		reset-deassert-us = <100000>;
 		reset-gpios = <&gpio3 RK_PB0 GPIO_ACTIVE_LOW>;
+
+		leds {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			led@1 {
+				reg = <1>;
+				color = <LED_COLOR_ID_AMBER>;
+				function = LED_FUNCTION_LAN;
+				default-state = "keep";
+			};
+
+			led@2 {
+				reg = <2>;
+				color = <LED_COLOR_ID_GREEN>;
+				function = LED_FUNCTION_LAN;
+				default-state = "keep";
+			};
+		};
 	};
 };
 
--- a/arch/arm64/boot/dts/rockchip/rk3576-nanopi-r76s.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3576-nanopi-r76s.dts
@@ -663,6 +663,22 @@
 	reset-gpios = <&gpio2 RK_PB4 GPIO_ACTIVE_HIGH>;
 	vpcie3v3-supply = <&vcc_3v3_s3>;
 	status = "okay";
+
+	pcie@0,0 {
+		reg = <0x00000000 0 0 0 0>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+		ranges;
+		device_type = "pci";
+
+		pcie-eth@0,0 {
+			compatible = "pci10ec,8125";
+			reg = <0x000000 0 0 0 0>;
+
+			realtek,led-data = <0x0 0x0 0x200 0x2b>;
+			label = "eth0";
+		};
+	};
 };
 
 &pcie1 {
@@ -671,6 +687,22 @@
 	reset-gpios = <&gpio0 RK_PC7 GPIO_ACTIVE_HIGH>;
 	vpcie3v3-supply = <&vcc_3v3_s3>;
 	status = "okay";
+
+	pcie@0,0 {
+		reg = <0x00200000 0 0 0 0>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+		ranges;
+		device_type = "pci";
+
+		pcie-eth@0,0 {
+			compatible = "pci10ec,8125";
+			reg = <0x000000 0 0 0 0>;
+
+			realtek,led-data = <0x0 0x0 0x200 0x2b>;
+			label = "eth1";
+		};
+	};
 };
 
 &pinctrl {
--- a/arch/arm64/boot/dts/rockchip/rk3588-armsom-sige7.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3588-armsom-sige7.dts
@@ -267,6 +267,19 @@
 &pcie2x1l0 {
 	reset-gpios = <&gpio4 RK_PA5 GPIO_ACTIVE_HIGH>;
 	status = "okay";
+
+	pcie@0,0 {
+		reg = <0x00200000 0 0 0 0>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		rtl8125_1: pcie-eth@20,0 {
+			compatible = "pci10ec,8125";
+			reg = <0x000000 0 0 0 0>;
+
+			realtek,led-data = <0x0 0x2b 0x200 0x0>;
+		};
+	};
 };
 
 /* phy2 - WiFi */
@@ -297,6 +310,19 @@
 &pcie2x1l2 {
 	reset-gpios = <&gpio3 RK_PB0 GPIO_ACTIVE_HIGH>;
 	status = "okay";
+
+	pcie@0,0 {
+		reg = <0x00400000 0 0 0 0>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		rtl8125_2: pcie-eth@40,0 {
+			compatible = "pci10ec,8125";
+			reg = <0x000000 0 0 0 0>;
+
+			realtek,led-data = <0x0 0x2b 0x200 0x0>;
+		};
+	};
 };
 
 &pcie30phy {
--- a/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dtsi
@@ -600,6 +600,20 @@
 	pinctrl-names = "default";
 	pinctrl-0 = <&pcie2_0_rst>;
 	status = "okay";
+
+	pcie@0,0 {
+		reg = <0x00200000 0 0 0 0>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		rtl8125_1: pcie-eth@20,0 {
+			compatible = "pci10ec,8125";
+			reg = <0x000000 0 0 0 0>;
+
+			realtek,led-data = <0x0 0x0 0x2b 0x200>;
+			label = "eth2";
+		};
+	};
 };
 
 &pcie2x1l1 {
@@ -616,6 +630,20 @@
 	pinctrl-names = "default";
 	pinctrl-0 = <&pcie2_2_rst>;
 	status = "okay";
+
+	pcie@0,0 {
+		reg = <0x00400000 0 0 0 0>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		rtl8125_2: pcie-eth@40,0 {
+			compatible = "pci10ec,8125";
+			reg = <0x000000 0 0 0 0>;
+
+			realtek,led-data = <0x0 0x0 0x2b 0x200>;
+			label = "eth1";
+		};
+	};
 };
 
 &pcie30phy {
--- a/arch/arm64/boot/dts/rockchip/rk3588s-rock-5c.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3588s-rock-5c.dts
@@ -417,6 +417,25 @@
 		reset-assert-us = <20000>;
 		reset-deassert-us = <100000>;
 		reset-gpios = <&gpio3 RK_PB7 GPIO_ACTIVE_LOW>;
+
+		leds {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			led@0 {
+				reg = <0>;
+				color = <LED_COLOR_ID_AMBER>;
+				function = LED_FUNCTION_LAN;
+				default-state = "keep";
+			};
+
+			led@1 {
+				reg = <1>;
+				color = <LED_COLOR_ID_GREEN>;
+				function = LED_FUNCTION_LAN;
+				default-state = "keep";
+			};
+		};
 	};
 };
 
