From 7fee88882704a5ed7657f467ecb44e39b20f42aa Mon Sep 17 00:00:00 2001
From: Tianling Shen <cnsztl@gmail.com>
Date: Sat, 27 Sep 2025 17:23:10 +0800
Subject: [PATCH] arm64: dts: rockchip: Add devicetree for the FriendlyElec
 NanoPi R76S

The NanoPi R76S (as "R76S") is an open-sourced mini IoT gateway
device with two 2.5G, designed and developed by FriendlyElec.

Specification:
- Rockchip RK3576
- 2/4GB LPDDR4X RAM
- 2x 2500Base-T (PCIe, rtl8125b)
- 3x LEDs (Power, LAN, WAN)
- 32GB eMMC
- MicroSD Slot
- MDMI 1.4/2.0 OUT
- M.2 E-Key SDIO slot
- USB 3.0 Port
- USB Type-C 5V Power

Signed-off-by: Tianling Shen <cnsztl@gmail.com>
Signed-off-by: Heiko Stuebner <heiko@sntech.de>
---
 arch/arm64/boot/dts/rockchip/Makefile              |   1 +
 .../arm64/boot/dts/rockchip/rk3576-nanopi-r76s.dts | 860 +++++++++++++++++++++
 2 files changed, 861 insertions(+)
 create mode 100644 arch/arm64/boot/dts/rockchip/rk3576-nanopi-r76s.dts

--- a/arch/arm64/boot/dts/rockchip/Makefile
+++ b/arch/arm64/boot/dts/rockchip/Makefile
@@ -128,6 +128,7 @@ dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3568-ro
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3568-wolfvision-pf5.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3568-wolfvision-pf5-display-vz.dtbo
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3568-wolfvision-pf5-io-expander.dtbo
+dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3576-nanopi-r76s.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3576-rock-4d.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3582-radxa-e52c.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3588-armsom-sige7.dtb
--- /dev/null
+++ b/arch/arm64/boot/dts/rockchip/rk3576-nanopi-r76s.dts
@@ -0,0 +1,860 @@
+// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
+/*
+ * Copyright (c) 2025 FriendlyElec Computer Tech. Co., Ltd.
+ * (http://www.friendlyelec.com)
+ *
+ * Copyright (c) 2025 Tianling Shen <cnsztl@gmail.com>
+ */
+
+/dts-v1/;
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/input/input.h>
+#include <dt-bindings/leds/common.h>
+#include <dt-bindings/pinctrl/rockchip.h>
+#include <dt-bindings/soc/rockchip,vop2.h>
+
+#include "rk3576.dtsi"
+
+/ {
+	model = "FriendlyElec NanoPi R76S";
+	compatible = "friendlyarm,nanopi-r76s", "rockchip,rk3576";
+
+	aliases {
+		mmc0 = &sdhci;
+		mmc1 = &sdmmc;
+		mmc2 = &sdio;
+	};
+
+	chosen {
+		stdout-path = "serial0:1500000n8";
+	};
+
+	gpio-keys {
+		compatible = "gpio-keys";
+		pinctrl-names = "default";
+		pinctrl-0 = <&user_but_pin>;
+
+		button-reset {
+			label = "reset";
+			gpios = <&gpio4 RK_PA2 GPIO_ACTIVE_LOW>;
+			debounce-interval = <50>;
+			linux,code = <KEY_RESTART>;
+			wakeup-source;
+		};
+	};
+
+	gpio-leds {
+		compatible = "gpio-leds";
+		pinctrl-names = "default";
+		pinctrl-0 = <&led1_h>, <&led_sys_h>, <&led2_h>;
+
+		led-0 {
+			color = <LED_COLOR_ID_GREEN>;
+			function = LED_FUNCTION_LAN;
+			gpios = <&gpio2 RK_PB0 GPIO_ACTIVE_HIGH>;
+		};
+
+		led-1 {
+			color = <LED_COLOR_ID_RED>;
+			function = LED_FUNCTION_POWER;
+			gpios = <&gpio2 RK_PB3 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "heartbeat";
+		};
+
+		led-2 {
+			color = <LED_COLOR_ID_GREEN>;
+			function = LED_FUNCTION_WAN;
+			gpios = <&gpio4 RK_PC5 GPIO_ACTIVE_HIGH>;
+		};
+	};
+
+	hdmi-con {
+		compatible = "hdmi-connector";
+		hdmi-pwr-supply = <&vcc5v_hdmi_tx>;
+		type = "a";
+
+		port {
+			hdmi_con_in: endpoint {
+				remote-endpoint = <&hdmi_out_con>;
+			};
+		};
+	};
+
+	sdio_pwrseq: sdio-pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		clocks = <&hym8563>;
+		clock-names = "ext_clock";
+		pinctrl-names = "default";
+		pinctrl-0 = <&wifi_reg_on_h>;
+		post-power-on-delay-ms = <200>;
+		reset-gpios = <&gpio1 RK_PC2 GPIO_ACTIVE_LOW>;
+	};
+
+	vcc3v3_rtc_s5: regulator-vcc3v3-rtc-s5 {
+		compatible = "regulator-fixed";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-name = "vcc3v3_rtc_s5";
+		vin-supply = <&vcc5v0_sys_s5>;
+	};
+
+	vcc5v_dcin: regulator-vcc5v-dcin {
+		compatible = "regulator-fixed";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		regulator-name = "vcc5v_dcin";
+	};
+
+	vcc5v_hdmi_tx: regulator-vcc5v-hdmi-tx {
+		compatible = "regulator-fixed";
+		enable-active-high;
+		gpios = <&gpio4 RK_PC6 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&hdmi_tx_on_h>;
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		regulator-name = "vcc5v_hdmi_tx";
+		vin-supply = <&vcc5v0_sys_s5>;
+	};
+
+	vcc5v0_device_s0: regulator-vcc5v0-device-s0 {
+		compatible = "regulator-fixed";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		regulator-name = "vcc5v0_device_s0";
+		vin-supply = <&vcc5v_dcin>;
+	};
+
+	vcc5v0_sys_s5: regulator-vcc5v0-sys-s5 {
+		compatible = "regulator-fixed";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		regulator-name = "vcc5v0_sys_s5";
+		vin-supply = <&vcc5v_dcin>;
+	};
+
+	vcc5v0_usb_otg0: regulator-vcc5v0-usb-otg0 {
+		compatible = "regulator-fixed";
+		enable-active-high;
+		gpios = <&gpio0 RK_PD1 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&usb_otg0_pwren_h>;
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		regulator-name = "vcc5v0_usb_otg0";
+		vin-supply = <&vcc5v0_sys_s5>;
+	};
+
+	vcc_1v1_nldo_s3: regulator-vcc-1v1-nldo-s3 {
+		compatible = "regulator-fixed";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <1100000>;
+		regulator-max-microvolt = <1100000>;
+		regulator-name = "vcc_1v1_nldo_s3";
+		vin-supply = <&vcc5v0_sys_s5>;
+	};
+
+	vcc_1v8_s0: regulator-vcc-1v8-s0 {
+		compatible = "regulator-fixed";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <1800000>;
+		regulator-name = "vcc_1v8_s0";
+		vin-supply = <&vcc_1v8_s3>;
+	};
+
+	vcc_2v0_pldo_s3: regulator-vcc-2v0-pldo-s3 {
+		compatible = "regulator-fixed";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <2000000>;
+		regulator-max-microvolt = <2000000>;
+		regulator-name = "vcc_2v0_pldo_s3";
+		vin-supply = <&vcc5v0_sys_s5>;
+	};
+
+	vcc_3v3_s0: regulator-vcc-3v3-s0 {
+		compatible = "regulator-fixed";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-name = "vcc_3v3_s0";
+		vin-supply = <&vcc_3v3_s3>;
+	};
+};
+
+&combphy0_ps {
+	status = "okay";
+};
+
+&combphy1_psu {
+	status = "okay";
+};
+
+&cpu_b0 {
+	cpu-supply = <&vdd_cpu_big_s0>;
+};
+
+&cpu_b1 {
+	cpu-supply = <&vdd_cpu_big_s0>;
+};
+
+&cpu_b2 {
+	cpu-supply = <&vdd_cpu_big_s0>;
+};
+
+&cpu_b3 {
+	cpu-supply = <&vdd_cpu_big_s0>;
+};
+
+&cpu_l0 {
+	cpu-supply = <&vdd_cpu_lit_s0>;
+};
+
+&cpu_l1 {
+	cpu-supply = <&vdd_cpu_lit_s0>;
+};
+
+&cpu_l2 {
+	cpu-supply = <&vdd_cpu_lit_s0>;
+};
+
+&cpu_l3 {
+	cpu-supply = <&vdd_cpu_lit_s0>;
+};
+
+&gpu {
+	mali-supply = <&vdd_gpu_s0>;
+	status = "okay";
+};
+
+&hdmi {
+	status = "okay";
+};
+
+&hdmi_in {
+	hdmi_in_vp0: endpoint {
+		remote-endpoint = <&vp0_out_hdmi>;
+	};
+};
+
+&hdmi_out {
+	hdmi_out_con: endpoint {
+		remote-endpoint = <&hdmi_con_in>;
+	};
+};
+
+&hdmi_sound {
+	status = "okay";
+};
+
+&hdptxphy {
+	status = "okay";
+};
+
+&i2c1 {
+	status = "okay";
+
+	pmic@23 {
+		compatible = "rockchip,rk806";
+		reg = <0x23>;
+		#gpio-cells = <2>;
+		gpio-controller;
+		interrupt-parent = <&gpio0>;
+		interrupts = <6 IRQ_TYPE_LEVEL_LOW>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&pmic_pins>, <&rk806_dvs1_null>,
+			    <&rk806_dvs2_null>, <&rk806_dvs3_null>;
+		system-power-controller;
+
+		vcc1-supply = <&vcc5v0_sys_s5>;
+		vcc2-supply = <&vcc5v0_sys_s5>;
+		vcc3-supply = <&vcc5v0_sys_s5>;
+		vcc4-supply = <&vcc5v0_sys_s5>;
+		vcc5-supply = <&vcc5v0_sys_s5>;
+		vcc6-supply = <&vcc5v0_sys_s5>;
+		vcc7-supply = <&vcc5v0_sys_s5>;
+		vcc8-supply = <&vcc5v0_sys_s5>;
+		vcc9-supply = <&vcc5v0_sys_s5>;
+		vcc10-supply = <&vcc5v0_sys_s5>;
+		vcc11-supply = <&vcc_2v0_pldo_s3>;
+		vcc12-supply = <&vcc5v0_sys_s5>;
+		vcc13-supply = <&vcc_1v1_nldo_s3>;
+		vcc14-supply = <&vcc_1v1_nldo_s3>;
+		vcca-supply = <&vcc5v0_sys_s5>;
+
+		rk806_dvs1_null: dvs1-null-pins {
+			pins = "gpio_pwrctrl1";
+			function = "pin_fun0";
+		};
+
+		rk806_dvs1_pwrdn: dvs1-pwrdn-pins {
+			pins = "gpio_pwrctrl1";
+			function = "pin_fun2";
+		};
+
+		rk806_dvs1_rst: dvs1-rst-pins {
+			pins = "gpio_pwrctrl1";
+			function = "pin_fun3";
+		};
+
+		rk806_dvs1_slp: dvs1-slp-pins {
+			pins = "gpio_pwrctrl1";
+			function = "pin_fun1";
+		};
+
+		rk806_dvs2_dvs: dvs2-dvs-pins {
+			pins = "gpio_pwrctrl2";
+			function = "pin_fun4";
+		};
+
+		rk806_dvs2_gpio: dvs2-gpio-pins {
+			pins = "gpio_pwrctrl2";
+			function = "pin_fun5";
+		};
+
+		rk806_dvs2_null: dvs2-null-pins {
+			pins = "gpio_pwrctrl2";
+			function = "pin_fun0";
+		};
+
+		rk806_dvs2_pwrdn: dvs2-pwrdn-pins {
+			pins = "gpio_pwrctrl2";
+			function = "pin_fun2";
+		};
+
+		rk806_dvs2_rst: dvs2-rst-pins {
+			pins = "gpio_pwrctrl2";
+			function = "pin_fun3";
+		};
+
+		rk806_dvs2_slp: dvs2-slp-pins {
+			pins = "gpio_pwrctrl2";
+			function = "pin_fun1";
+		};
+
+		rk806_dvs3_dvs: dvs3-dvs-pins {
+			pins = "gpio_pwrctrl3";
+			function = "pin_fun4";
+		};
+
+		rk806_dvs3_gpio: dvs3-gpio-pins {
+			pins = "gpio_pwrctrl3";
+			function = "pin_fun5";
+		};
+
+		rk806_dvs3_null: dvs3-null-pins {
+			pins = "gpio_pwrctrl3";
+			function = "pin_fun0";
+		};
+
+		rk806_dvs3_pwrdn: dvs3-pwrdn-pins {
+			pins = "gpio_pwrctrl3";
+			function = "pin_fun2";
+		};
+
+		rk806_dvs3_rst: dvs3-rst-pins {
+			pins = "gpio_pwrctrl3";
+			function = "pin_fun3";
+		};
+
+		rk806_dvs3_slp: dvs3-slp-pins {
+			pins = "gpio_pwrctrl3";
+			function = "pin_fun1";
+		};
+
+		regulators {
+			vdd_cpu_big_s0: dcdc-reg1 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-enable-ramp-delay = <400>;
+				regulator-min-microvolt = <550000>;
+				regulator-max-microvolt = <950000>;
+				regulator-name = "vdd_cpu_big_s0";
+				regulator-ramp-delay = <12500>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vdd_npu_s0: dcdc-reg2 {
+				regulator-boot-on;
+				regulator-enable-ramp-delay = <400>;
+				regulator-min-microvolt = <550000>;
+				regulator-max-microvolt = <950000>;
+				regulator-name = "vdd_npu_s0";
+				regulator-ramp-delay = <12500>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vdd_cpu_lit_s0: dcdc-reg3 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <550000>;
+				regulator-max-microvolt = <950000>;
+				regulator-name = "vdd_cpu_lit_s0";
+				regulator-ramp-delay = <12500>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+					regulator-suspend-microvolt = <750000>;
+				};
+			};
+
+			vcc_3v3_s3: dcdc-reg4 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc_3v3_s3";
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <3300000>;
+				};
+			};
+
+			vdd_gpu_s0: dcdc-reg5 {
+				regulator-boot-on;
+				regulator-enable-ramp-delay = <400>;
+				regulator-min-microvolt = <550000>;
+				regulator-max-microvolt = <900000>;
+				regulator-name = "vdd_gpu_s0";
+				regulator-ramp-delay = <12500>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+					regulator-suspend-microvolt = <850000>;
+				};
+			};
+
+			vddq_ddr_s0: dcdc-reg6 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-name = "vddq_ddr_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vdd_logic_s0: dcdc-reg7 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <550000>;
+				regulator-max-microvolt = <800000>;
+				regulator-name = "vdd_logic_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc_1v8_s3: dcdc-reg8 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "vcc_1v8_s3";
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1800000>;
+				};
+			};
+
+			vdd2_ddr_s3: dcdc-reg9 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-name = "vdd2_ddr_s3";
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+				};
+			};
+
+			vdd_ddr_s0: dcdc-reg10 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <550000>;
+				regulator-max-microvolt = <1200000>;
+				regulator-name = "vdd_ddr_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcca_1v8_s0: pldo-reg1 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "vcca_1v8_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcca1v8_pldo2_s0: pldo-reg2 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "vcca1v8_pldo2_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vdda_1v2_s0: pldo-reg3 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1200000>;
+				regulator-max-microvolt = <1200000>;
+				regulator-name = "vdda_1v2_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcca_3v3_s0: pldo-reg4 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcca_3v3_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vccio_sd_s0: pldo-reg5 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vccio_sd_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcca1v8_pldo6_s3: pldo-reg6 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "vcca1v8_pldo6_s3";
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1800000>;
+				};
+			};
+
+			vdd_0v75_s3: nldo-reg1 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <750000>;
+				regulator-max-microvolt = <750000>;
+				regulator-name = "vdd_0v75_s3";
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <750000>;
+				};
+			};
+
+			vdda_ddr_pll_s0: nldo-reg2 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <850000>;
+				regulator-max-microvolt = <850000>;
+				regulator-name = "vdda_ddr_pll_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vdda0v75_hdmi_s0: nldo-reg3 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <837500>;
+				regulator-max-microvolt = <837500>;
+				regulator-name = "vdda0v75_hdmi_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vdda_0v85_s0: nldo-reg4 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <850000>;
+				regulator-max-microvolt = <850000>;
+				regulator-name = "vdda_0v85_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vdda_0v75_s0: nldo-reg5 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <750000>;
+				regulator-max-microvolt = <750000>;
+				regulator-name = "vdda_0v75_s0";
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+		};
+	};
+};
+
+&i2c2 {
+	status = "okay";
+
+	hym8563: rtc@51 {
+		compatible = "haoyu,hym8563";
+		reg = <0x51>;
+		#clock-cells = <0>;
+		clock-output-names = "hym8563";
+		interrupt-parent = <&gpio0>;
+		interrupts = <RK_PA5 IRQ_TYPE_LEVEL_LOW>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&rtc_int_l>;
+		wakeup-source;
+	};
+};
+
+&pcie0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&pcie0_perstn>;
+	reset-gpios = <&gpio2 RK_PB4 GPIO_ACTIVE_HIGH>;
+	vpcie3v3-supply = <&vcc_3v3_s3>;
+	status = "okay";
+};
+
+&pcie1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&pcie1_perstn>;
+	reset-gpios = <&gpio0 RK_PC7 GPIO_ACTIVE_HIGH>;
+	vpcie3v3-supply = <&vcc_3v3_s3>;
+	status = "okay";
+};
+
+&pinctrl {
+	bt {
+		bt_reg_on_h: bt-reg-on-h {
+			rockchip,pins = <3 RK_PC7 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+
+		bt_wake_host_h: bt-wake-host-h {
+			rockchip,pins = <0 RK_PB1 RK_FUNC_GPIO &pcfg_pull_down>;
+		};
+
+		host_wake_bt_h: host-wake-bt-h {
+			rockchip,pins = <3 RK_PD0 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+
+	gpio-keys {
+		user_but_pin: user-but-pin {
+			rockchip,pins = <4 RK_PA2 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+
+	gpio-leds {
+		led_sys_h: led-sys-h {
+			rockchip,pins = <2 RK_PB3 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		led1_h: led1-h {
+			rockchip,pins = <2 RK_PB0 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		led2_h: led2-h {
+			rockchip,pins = <4 RK_PC5 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	hdmi {
+		hdmi_tx_on_h: hdmi-tx-on-h {
+			rockchip,pins = <4 RK_PC6 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	hym8563 {
+		rtc_int_l: rtc-int-l {
+			rockchip,pins = <0 RK_PA5 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+
+	pcie {
+		pcie0_perstn: pcie0-perstn {
+			rockchip,pins = <2 RK_PB4 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+
+		pcie1_perstn: pcie1-perstn {
+			rockchip,pins = <0 RK_PC7 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+
+	usb {
+		usb_otg0_pwren_h: usb-otg0-pwren-h {
+			rockchip,pins = <0 RK_PD1 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	wifi {
+		wifi_wake_host_h: wifi-wake-host-h {
+			rockchip,pins = <0 RK_PB0 RK_FUNC_GPIO &pcfg_pull_down>;
+		};
+
+		wifi_reg_on_h: wifi-reg-on-h {
+			rockchip,pins = <1 RK_PC2 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+};
+
+&sai6 {
+	status = "okay";
+};
+
+&sdmmc {
+	bus-width = <4>;
+	cap-mmc-highspeed;
+	cap-sd-highspeed;
+	disable-wp;
+	no-mmc;
+	no-sdio;
+	sd-uhs-sdr104;
+	vmmc-supply = <&vcc_3v3_s3>;
+	vqmmc-supply = <&vccio_sd_s0>;
+	status = "okay";
+};
+
+&sdio {
+	#address-cells = <1>;
+	#size-cells = <0>;
+	bus-width = <4>;
+	cap-sd-highspeed;
+	cap-sdio-irq;
+	disable-wp;
+	keep-power-in-suspend;
+	mmc-pwrseq = <&sdio_pwrseq>;
+	no-mmc;
+	no-sd;
+	non-removable;
+	sd-uhs-sdr104;
+	vmmc-supply = <&vcc_3v3_s3>;
+	vqmmc-supply = <&vcc_1v8_s3>;
+	wakeup-source;
+	status = "okay";
+
+	rtl8822cs: wifi@1 {
+		reg = <1>;
+		interrupt-parent = <&gpio0>;
+		interrupts = <RK_PB0 IRQ_TYPE_LEVEL_HIGH>;
+		interrupt-names = "host-wake";
+		pinctrl-names = "default";
+		pinctrl-0 = <&wifi_wake_host_h>;
+	};
+};
+
+&sdhci {
+	bus-width = <8>;
+	cap-mmc-highspeed;
+	full-pwr-cycle-in-suspend;
+	mmc-hs400-1_8v;
+	mmc-hs400-enhanced-strobe;
+	no-sdio;
+	no-sd;
+	non-removable;
+	status = "okay";
+};
+
+&saradc {
+	vref-supply = <&vcca_1v8_s0>;
+	status = "okay";
+};
+
+&u2phy0 {
+	status = "okay";
+};
+
+&u2phy0_otg {
+	phy-supply = <&vcc5v0_usb_otg0>;
+	status = "okay";
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&uart5 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart5m0_xfer &uart5m0_ctsn &uart5m0_rtsn>;
+	uart-has-rtscts;
+	status = "okay";
+
+	bluetooth {
+		compatible = "realtek,rtl8822cs-bt";
+		enable-gpios = <&gpio3 RK_PC7 GPIO_ACTIVE_HIGH>;
+		device-wake-gpios = <&gpio3 RK_PD0 GPIO_ACTIVE_HIGH>;
+		host-wake-gpios = <&gpio0 RK_PB1 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&bt_wake_host_h &host_wake_bt_h &bt_reg_on_h>;
+	};
+};
+
+&usbdp_phy {
+	status = "okay";
+};
+
+&usb_drd0_dwc3 {
+	dr_mode = "host";
+	extcon = <&u2phy0>;
+	status = "okay";
+};
+
+&vop {
+	status = "okay";
+};
+
+&vop_mmu {
+	status = "okay";
+};
+
+&vp0 {
+	vp0_out_hdmi: endpoint@ROCKCHIP_VOP2_EP_HDMI0 {
+		reg = <ROCKCHIP_VOP2_EP_HDMI0>;
+		remote-endpoint = <&hdmi_in_vp0>;
+	};
+};
