From 70acfc3433040fa9c26a070d4c2fdaf205e29b03 Mon Sep 17 00:00:00 2001
From: Daniel Golle <daniel@makrotopia.org>
Date: Thu, 26 Mar 2026 05:11:12 +0000
Subject: [PATCH 3/3] clk: mediatek: mt7988: use MUX_CLR_SET for gate-less
 muxes

All 19 muxes in the infra_muxes[] array are pure mux selectors without
a clock gate or update register, yet they were defined using
MUX_GATE_CLR_SET_UPD with gate_shift = -1.

This macro assigns mtk_mux_gate_clr_set_upd_ops, whose
enable/disable/is_enabled callbacks perform BIT(gate_shift). Since
gate_shift is stored as u8, the -1 truncates to 255, causing a
shift-out-of-bounds at runtime:

UBSAN: shift-out-of-bounds in drivers/clk/mediatek/clk-mux.c:76:8
shift exponent 255 is too large for 64-bit type 'long unsigned int'

UBSAN: shift-out-of-bounds in drivers/clk/mediatek/clk-mux.c:102:4
shift exponent 255 is too large for 64-bit type 'long unsigned int'

UBSAN: shift-out-of-bounds in drivers/clk/mediatek/clk-mux.c:122:16
shift exponent 255 is too large for 64-bit type 'long unsigned int'

Switch these definitions to MUX_CLR_SET, which uses
mtk_mux_clr_set_upd_ops (no gate callbacks) and does not require
callers to pass sentinel values for unused update register fields.
The actual clock gating for these peripherals is handled by the
separate GATE_INFRA* definitions further down.

Fixes: 4b4719437d85f ("clk: mediatek: add drivers for MT7988 SoC")
Signed-off-by: Daniel Golle <daniel@makrotopia.org>
Reviewed-by: Chen-Yu Tsai <wenst@chromium.org>
---
 drivers/clk/mediatek/clk-mt7988-infracfg.c | 80 ++++++++++------------
 1 file changed, 38 insertions(+), 42 deletions(-)

--- a/drivers/clk/mediatek/clk-mt7988-infracfg.c
+++ b/drivers/clk/mediatek/clk-mt7988-infracfg.c
@@ -56,49 +56,45 @@ static const char *const infra_pcie_gfmu
 
 static const struct mtk_mux infra_muxes[] = {
 	/* MODULE_CLK_SEL_0 */
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_MUX_UART0_SEL, "infra_mux_uart0_sel",
-			     infra_mux_uart0_parents, 0x0018, 0x0010, 0x0014, 0, 1, -1, -1, -1),
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_MUX_UART1_SEL, "infra_mux_uart1_sel",
-			     infra_mux_uart1_parents, 0x0018, 0x0010, 0x0014, 1, 1, -1, -1, -1),
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_MUX_UART2_SEL, "infra_mux_uart2_sel",
-			     infra_mux_uart2_parents, 0x0018, 0x0010, 0x0014, 2, 1, -1, -1, -1),
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_MUX_SPI0_SEL, "infra_mux_spi0_sel", infra_mux_spi0_parents,
-			     0x0018, 0x0010, 0x0014, 4, 1, -1, -1, -1),
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_MUX_SPI1_SEL, "infra_mux_spi1_sel", infra_mux_spi1_parents,
-			     0x0018, 0x0010, 0x0014, 5, 1, -1, -1, -1),
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_MUX_SPI2_SEL, "infra_mux_spi2_sel", infra_mux_spi0_parents,
-			     0x0018, 0x0010, 0x0014, 6, 1, -1, -1, -1),
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_PWM_SEL, "infra_pwm_sel", infra_pwm_bck_parents, 0x0018,
-			     0x0010, 0x0014, 14, 2, -1, -1, -1),
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_PWM_CK1_SEL, "infra_pwm_ck1_sel", infra_pwm_bck_parents,
-			     0x0018, 0x0010, 0x0014, 16, 2, -1, -1, -1),
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_PWM_CK2_SEL, "infra_pwm_ck2_sel", infra_pwm_bck_parents,
-			     0x0018, 0x0010, 0x0014, 18, 2, -1, -1, -1),
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_PWM_CK3_SEL, "infra_pwm_ck3_sel", infra_pwm_bck_parents,
-			     0x0018, 0x0010, 0x0014, 20, 2, -1, -1, -1),
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_PWM_CK4_SEL, "infra_pwm_ck4_sel", infra_pwm_bck_parents,
-			     0x0018, 0x0010, 0x0014, 22, 2, -1, -1, -1),
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_PWM_CK5_SEL, "infra_pwm_ck5_sel", infra_pwm_bck_parents,
-			     0x0018, 0x0010, 0x0014, 24, 2, -1, -1, -1),
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_PWM_CK6_SEL, "infra_pwm_ck6_sel", infra_pwm_bck_parents,
-			     0x0018, 0x0010, 0x0014, 26, 2, -1, -1, -1),
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_PWM_CK7_SEL, "infra_pwm_ck7_sel", infra_pwm_bck_parents,
-			     0x0018, 0x0010, 0x0014, 28, 2, -1, -1, -1),
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_PWM_CK8_SEL, "infra_pwm_ck8_sel", infra_pwm_bck_parents,
-			     0x0018, 0x0010, 0x0014, 30, 2, -1, -1, -1),
+	MUX_CLR_SET(CLK_INFRA_MUX_UART0_SEL, "infra_mux_uart0_sel",
+		    infra_mux_uart0_parents, 0x0018, 0x0010, 0x0014, 0, 1),
+	MUX_CLR_SET(CLK_INFRA_MUX_UART1_SEL, "infra_mux_uart1_sel",
+		    infra_mux_uart1_parents, 0x0018, 0x0010, 0x0014, 1, 1),
+	MUX_CLR_SET(CLK_INFRA_MUX_UART2_SEL, "infra_mux_uart2_sel",
+		    infra_mux_uart2_parents, 0x0018, 0x0010, 0x0014, 2, 1),
+	MUX_CLR_SET(CLK_INFRA_MUX_SPI0_SEL, "infra_mux_spi0_sel",
+		    infra_mux_spi0_parents, 0x0018, 0x0010, 0x0014, 4, 1),
+	MUX_CLR_SET(CLK_INFRA_MUX_SPI1_SEL, "infra_mux_spi1_sel",
+		    infra_mux_spi1_parents, 0x0018, 0x0010, 0x0014, 5, 1),
+	MUX_CLR_SET(CLK_INFRA_MUX_SPI2_SEL, "infra_mux_spi2_sel",
+		    infra_mux_spi0_parents, 0x0018, 0x0010, 0x0014, 6, 1),
+	MUX_CLR_SET(CLK_INFRA_PWM_SEL, "infra_pwm_sel",
+		    infra_pwm_bck_parents, 0x0018, 0x0010, 0x0014, 14, 2),
+	MUX_CLR_SET(CLK_INFRA_PWM_CK1_SEL, "infra_pwm_ck1_sel",
+		    infra_pwm_bck_parents, 0x0018, 0x0010, 0x0014, 16, 2),
+	MUX_CLR_SET(CLK_INFRA_PWM_CK2_SEL, "infra_pwm_ck2_sel",
+		    infra_pwm_bck_parents, 0x0018, 0x0010, 0x0014, 18, 2),
+	MUX_CLR_SET(CLK_INFRA_PWM_CK3_SEL, "infra_pwm_ck3_sel",
+		    infra_pwm_bck_parents, 0x0018, 0x0010, 0x0014, 20, 2),
+	MUX_CLR_SET(CLK_INFRA_PWM_CK4_SEL, "infra_pwm_ck4_sel",
+		    infra_pwm_bck_parents, 0x0018, 0x0010, 0x0014, 22, 2),
+	MUX_CLR_SET(CLK_INFRA_PWM_CK5_SEL, "infra_pwm_ck5_sel",
+		    infra_pwm_bck_parents, 0x0018, 0x0010, 0x0014, 24, 2),
+	MUX_CLR_SET(CLK_INFRA_PWM_CK6_SEL, "infra_pwm_ck6_sel",
+		    infra_pwm_bck_parents, 0x0018, 0x0010, 0x0014, 26, 2),
+	MUX_CLR_SET(CLK_INFRA_PWM_CK7_SEL, "infra_pwm_ck7_sel",
+		    infra_pwm_bck_parents, 0x0018, 0x0010, 0x0014, 28, 2),
+	MUX_CLR_SET(CLK_INFRA_PWM_CK8_SEL, "infra_pwm_ck8_sel",
+		    infra_pwm_bck_parents, 0x0018, 0x0010, 0x0014, 30, 2),
 	/* MODULE_CLK_SEL_1 */
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_PCIE_GFMUX_TL_O_P0_SEL, "infra_pcie_gfmux_tl_o_p0_sel",
-			     infra_pcie_gfmux_tl_ck_o_p0_parents, 0x0028, 0x0020, 0x0024, 0, 2, -1,
-			     -1, -1),
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_PCIE_GFMUX_TL_O_P1_SEL, "infra_pcie_gfmux_tl_o_p1_sel",
-			     infra_pcie_gfmux_tl_ck_o_p1_parents, 0x0028, 0x0020, 0x0024, 2, 2, -1,
-			     -1, -1),
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_PCIE_GFMUX_TL_O_P2_SEL, "infra_pcie_gfmux_tl_o_p2_sel",
-			     infra_pcie_gfmux_tl_ck_o_p2_parents, 0x0028, 0x0020, 0x0024, 4, 2, -1,
-			     -1, -1),
-	MUX_GATE_CLR_SET_UPD(CLK_INFRA_PCIE_GFMUX_TL_O_P3_SEL, "infra_pcie_gfmux_tl_o_p3_sel",
-			     infra_pcie_gfmux_tl_ck_o_p3_parents, 0x0028, 0x0020, 0x0024, 6, 2, -1,
-			     -1, -1),
+	MUX_CLR_SET(CLK_INFRA_PCIE_GFMUX_TL_O_P0_SEL, "infra_pcie_gfmux_tl_o_p0_sel",
+		    infra_pcie_gfmux_tl_ck_o_p0_parents, 0x0028, 0x0020, 0x0024, 0, 2),
+	MUX_CLR_SET(CLK_INFRA_PCIE_GFMUX_TL_O_P1_SEL, "infra_pcie_gfmux_tl_o_p1_sel",
+		    infra_pcie_gfmux_tl_ck_o_p1_parents, 0x0028, 0x0020, 0x0024, 2, 2),
+	MUX_CLR_SET(CLK_INFRA_PCIE_GFMUX_TL_O_P2_SEL, "infra_pcie_gfmux_tl_o_p2_sel",
+		    infra_pcie_gfmux_tl_ck_o_p2_parents, 0x0028, 0x0020, 0x0024, 4, 2),
+	MUX_CLR_SET(CLK_INFRA_PCIE_GFMUX_TL_O_P3_SEL, "infra_pcie_gfmux_tl_o_p3_sel",
+		    infra_pcie_gfmux_tl_ck_o_p3_parents, 0x0028, 0x0020, 0x0024, 6, 2),
 };
 
 static const struct mtk_gate_regs infra0_cg_regs = {
