From 48afd5124fd6129c46fd12cb06155384b1c4a0c4 Mon Sep 17 00:00:00 2001
From: Chih Kai Hsu <hsu.chih.kai@realtek.com>
Date: Thu, 26 Mar 2026 15:39:23 +0800
Subject: [PATCH] r8152: fix incorrect register write to USB_UPHY_XTAL

The old code used ocp_write_byte() to clear the OOBS_POLLING bit
(BIT(8)) in the USB_UPHY_XTAL register, but this doesn't correctly
clear a bit in the upper byte of the 16-bit register.

Fix this by using ocp_write_word() instead.

Fixes: 195aae321c82 ("r8152: support new chips")
Signed-off-by: Chih Kai Hsu <hsu.chih.kai@realtek.com>
Reviewed-by: Hayes Wang <hayeswang@realtek.com>
Link: https://patch.msgid.link/20260326073925.32976-454-nic_swsd@realtek.com
Signed-off-by: Paolo Abeni <pabeni@redhat.com>
---
 drivers/net/usb/r8152.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/usb/r8152.c
+++ b/drivers/net/usb/r8152.c
@@ -3898,7 +3898,7 @@ static void r8156_ups_en(struct r8152 *t
 		case RTL_VER_15:
 			ocp_data = ocp_read_word(tp, MCU_TYPE_USB, USB_UPHY_XTAL);
 			ocp_data &= ~OOBS_POLLING;
-			ocp_write_byte(tp, MCU_TYPE_USB, USB_UPHY_XTAL, ocp_data);
+			ocp_write_word(tp, MCU_TYPE_USB, USB_UPHY_XTAL, ocp_data);
 			break;
 		default:
 			break;
