From bf919ccfced7d47d14ec2d20ae465e8ae410aee6 Mon Sep 17 00:00:00 2001
From: Robert Marko <robert.marko@sartura.hr>
Date: Mon, 22 Sep 2025 16:27:29 +0200
Subject: [PATCH] reset: sparx5: add LAN969x support

LAN969x uses the same reset configuration as LAN966x, but we need to
allow compiling it when ARCH_LAN969X is selected.

A fallback compatible to LAN966x will be used.

Signed-off-by: Robert Marko <robert.marko@sartura.hr>
Signed-off-by: Philipp Zabel <p.zabel@pengutronix.de>
---
 drivers/reset/Kconfig | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/reset/Kconfig
+++ b/drivers/reset/Kconfig
@@ -170,7 +170,7 @@ config RESET_LPC18XX
 
 config RESET_MCHP_SPARX5
 	tristate "Microchip Sparx5 reset driver"
-	depends on ARCH_SPARX5 || SOC_LAN966 || MCHP_LAN966X_PCI || COMPILE_TEST
+	depends on ARCH_SPARX5 || ARCH_LAN969X || SOC_LAN966 || MCHP_LAN966X_PCI || COMPILE_TEST
 	default y if SPARX5_SWITCH
 	select MFD_SYSCON
 	help
