// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

/dts-v1/;

#include "ipq8074-512m.dtsi"
#include "ipq8074-ac-cpu.dtsi"
#include "ipq8074-ess.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "CMCC RM2-6";
	compatible = "cmcc,rm2-6", "qcom,ipq8074";

	aliases {
		serial0 = &blsp1_uart5;
		serial1 = &blsp1_uart3;
		led-boot = &led_status_red;
		led-failsafe = &led_status_red;
		led-running = &led_status_blue;
		led-upgrade = &led_status_amber;
		/*
		 * Aliases as required by u-boot
		 * to patch MAC addresses
		 */
		ethernet0 = &dp4;
		ethernet1 = &dp2;
		ethernet2 = &dp5;
		label-mac-device = &dp4;
	};

	chosen {
		stdout-path = "serial0:115200n8";
		bootargs-append = " root=/dev/ubiblock0_1";
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&tlmm 27 GPIO_ACTIVE_LOW>;
		};

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&tlmm 30 GPIO_ACTIVE_LOW>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_status_amber: status-amber {
			color = <LED_COLOR_ID_AMBER>;
			function = LED_FUNCTION_STATUS;
			gpios = <&tlmm 25 GPIO_ACTIVE_HIGH>;
		};

		led_status_blue: status-blue {
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_STATUS;
			gpios = <&tlmm 26 GPIO_ACTIVE_HIGH>;
		};

		led_status_red: status-red {
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_STATUS;
			gpios = <&tlmm 31 GPIO_ACTIVE_HIGH>;
		};
	};

	fan: gpio-fan {
		#cooling-cells = <2>;
		compatible = "gpio-fan";
		gpios = <&tlmm 29 GPIO_ACTIVE_HIGH>;
		gpio-fan,speed-map = <0 0>, <1 1>;
	};
};

&tlmm {
	mdio_pins: mdio-pins {
		mdc {
			pins = "gpio68";
			function = "mdc";
			drive-strength = <8>;
			bias-pull-up;
		};

		mdio {
			pins = "gpio69";
			function = "mdio";
			drive-strength = <8>;
			bias-pull-up;
		};
	};
};

&blsp1_uart3 {
	status = "okay";
};

&blsp1_uart5 {
	status = "okay";
};

&cryptobam {
	status = "okay";
};

&crypto {
	status = "okay";
};

&prng {
	status = "okay";
};

&qpic_bam {
	status = "okay";
};

&qpic_nand {
	status = "okay";

	nand@0 {
		reg = <0>;
		nand-ecc-strength = <8>;
		nand-ecc-step-size = <512>;
		nand-bus-width = <8>;

		partitions {
			compatible = "qcom,smem-part";
		};
	};
};

&cpu0_thermal {
	trips {
		cpu0_trip_active: cpu-active {
			temperature = <60000>;
			hysteresis = <2000>;
			type = "active";
		};
	};

	cooling-maps {
		cpu-active {
			cooling-device = <&fan THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
			trip = <&cpu0_trip_active>;
		};
	};
};

&cpu1_thermal {
	trips {
		cpu1_trip_active: cpu-active {
			temperature = <60000>;
			hysteresis = <2000>;
			type = "active";
		};
	};

	cooling-maps {
		cpu-active {
			cooling-device = <&fan THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
			trip = <&cpu1_trip_active>;
		};
	};
};

&cpu2_thermal {
	trips {
		cpu2_trip_active: cpu-active {
			temperature = <60000>;
			hysteresis = <2000>;
			type = "active";
		};
	};

	cooling-maps {
		cpu-active {
			cooling-device = <&fan THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
			trip = <&cpu2_trip_active>;
		};
	};
};

&cpu3_thermal {
	trips {
		cpu3_trip_active: cpu-active {
			temperature = <60000>;
			hysteresis = <2000>;
			type = "active";
		};
	};

	cooling-maps {
		cpu-active {
			cooling-device = <&fan THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
			trip = <&cpu3_trip_active>;
		};
	};
};

&cluster_thermal {
	trips {
		cluster_active: cluster-active {
			temperature = <60000>;
			hysteresis = <2000>;
			type = "active";
		};
	};

	cooling-maps {
		cluster-active {
			cooling-device = <&fan THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
			trip = <&cluster_active>;
		};
	};
};

&mdio {
	status = "okay";

	pinctrl-0 = <&mdio_pins>;
	pinctrl-names = "default";
	reset-gpios = <&tlmm 37 GPIO_ACTIVE_LOW>;

	ethernet-phy-package@0 {
		compatible = "qcom,qca8075-package";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0>;

		qca8075_1: ethernet-phy@1 {
			compatible = "ethernet-phy-ieee802.3-c22";
			reg = <1>;
		};

		qca8075_3: ethernet-phy@3 {
			compatible = "ethernet-phy-ieee802.3-c22";
			reg = <3>;
		};

		qca8075_4: ethernet-phy@4 {
			compatible = "ethernet-phy-ieee802.3-c22";
			reg = <4>;
		};
	};
};

&switch {
	status = "okay";

	switch_lan_bmp = <(ESS_PORT2 | ESS_PORT4)>;
	switch_wan_bmp = <ESS_PORT5>;
	switch_mac_mode = <MAC_MODE_PSGMII>;

	qcom,port_phyinfo {
		port@2 {
			port_id = <2>;
			phy_address = <1>;
		};
		port@4 {
			port_id = <4>;
			phy_address = <3>;
		};
		port@5 {
			port_id = <5>;
			phy_address = <4>;
		};
	};
};

&edma {
	status = "okay";
};

/*
 * Directly connect to the Hi5630
 * PLC (Power Line Communication)
 */
&dp2 {
	status = "okay";
	phy-handle = <&qca8075_1>;
	label = "plc";
};

&dp4 {
	status = "okay";
	phy-handle = <&qca8075_3>;
	label = "lan";
};

&dp5 {
	status = "okay";
	phy-handle = <&qca8075_4>;
	label = "wan";
};

&wifi {
	status = "okay";

	qcom,ath11k-calibration-variant = "CMCC-RM2-6";
	qcom,ath11k-fw-memory-mode = <1>;
};
