From a60d92f6d941bd77bf3aaec724a7c95857c0165b Mon Sep 17 00:00:00 2001
From: Mayank Rana <mayank.rana@oss.qualcomm.com>
Date: Mon, 16 Jun 2025 15:42:56 -0700
Subject: [PATCH] PCI: dwc: Export DWC MSI controller related APIs

Export dw_pcie_msi_host_init(), dw_pcie_msi_init(), and dw_pcie_free_msi()
APIs to allow them to be reused by the upcoming DWC based ECAM driver
implementation. Also, move MSI IRQ related initialization code to
dw_pcie_msi_init(), as this code must be executed before dw_pcie_msi_init()
API can be used with ECAM driver.

Signed-off-by: Mayank Rana <mayank.rana@oss.qualcomm.com>
[mani: commit message rewording]
Signed-off-by: Manivannan Sadhasivam <mani@kernel.org>
Link: https://patch.msgid.link/20250616224259.3549811-2-mayank.rana@oss.qualcomm.com
---
 .../pci/controller/dwc/pcie-designware-host.c | 38 ++++++++++---------
 drivers/pci/controller/dwc/pcie-designware.h  | 14 +++++++
 2 files changed, 34 insertions(+), 18 deletions(-)

--- a/drivers/pci/controller/dwc/pcie-designware-host.c
+++ b/drivers/pci/controller/dwc/pcie-designware-host.c
@@ -250,7 +250,7 @@ int dw_pcie_allocate_domains(struct dw_p
 	return 0;
 }
 
-static void dw_pcie_free_msi(struct dw_pcie_rp *pp)
+void dw_pcie_free_msi(struct dw_pcie_rp *pp)
 {
 	u32 ctrl;
 
@@ -263,19 +263,34 @@ static void dw_pcie_free_msi(struct dw_p
 	irq_domain_remove(pp->msi_domain);
 	irq_domain_remove(pp->irq_domain);
 }
+EXPORT_SYMBOL_GPL(dw_pcie_free_msi);
 
-static void dw_pcie_msi_init(struct dw_pcie_rp *pp)
+void dw_pcie_msi_init(struct dw_pcie_rp *pp)
 {
 	struct dw_pcie *pci = to_dw_pcie_from_pp(pp);
 	u64 msi_target = (u64)pp->msi_data;
+	u32 ctrl, num_ctrls;
 
 	if (!pci_msi_enabled() || !pp->has_msi_ctrl)
 		return;
 
+	num_ctrls = pp->num_vectors / MAX_MSI_IRQS_PER_CTRL;
+
+	/* Initialize IRQ Status array */
+	for (ctrl = 0; ctrl < num_ctrls; ctrl++) {
+		dw_pcie_writel_dbi(pci, PCIE_MSI_INTR0_MASK +
+				    (ctrl * MSI_REG_CTRL_BLOCK_SIZE),
+				    pp->irq_mask[ctrl]);
+		dw_pcie_writel_dbi(pci, PCIE_MSI_INTR0_ENABLE +
+				    (ctrl * MSI_REG_CTRL_BLOCK_SIZE),
+				    ~0);
+	}
+
 	/* Program the msi_data */
 	dw_pcie_writel_dbi(pci, PCIE_MSI_ADDR_LO, lower_32_bits(msi_target));
 	dw_pcie_writel_dbi(pci, PCIE_MSI_ADDR_HI, upper_32_bits(msi_target));
 }
+EXPORT_SYMBOL_GPL(dw_pcie_msi_init);
 
 static int dw_pcie_parse_split_msi_irq(struct dw_pcie_rp *pp)
 {
@@ -317,7 +332,7 @@ static int dw_pcie_parse_split_msi_irq(s
 	return 0;
 }
 
-static int dw_pcie_msi_host_init(struct dw_pcie_rp *pp)
+int dw_pcie_msi_host_init(struct dw_pcie_rp *pp)
 {
 	struct dw_pcie *pci = to_dw_pcie_from_pp(pp);
 	struct device *dev = pci->dev;
@@ -391,6 +406,7 @@ static int dw_pcie_msi_host_init(struct
 
 	return 0;
 }
+EXPORT_SYMBOL_GPL(dw_pcie_msi_host_init);
 
 static void dw_pcie_host_request_msg_tlp_res(struct dw_pcie_rp *pp)
 {
@@ -809,7 +825,7 @@ static int dw_pcie_iatu_setup(struct dw_
 int dw_pcie_setup_rc(struct dw_pcie_rp *pp)
 {
 	struct dw_pcie *pci = to_dw_pcie_from_pp(pp);
-	u32 val, ctrl, num_ctrls;
+	u32 val;
 	int ret;
 
 	/*
@@ -820,20 +836,6 @@ int dw_pcie_setup_rc(struct dw_pcie_rp *
 
 	dw_pcie_setup(pci);
 
-	if (pp->has_msi_ctrl) {
-		num_ctrls = pp->num_vectors / MAX_MSI_IRQS_PER_CTRL;
-
-		/* Initialize IRQ Status array */
-		for (ctrl = 0; ctrl < num_ctrls; ctrl++) {
-			dw_pcie_writel_dbi(pci, PCIE_MSI_INTR0_MASK +
-					    (ctrl * MSI_REG_CTRL_BLOCK_SIZE),
-					    pp->irq_mask[ctrl]);
-			dw_pcie_writel_dbi(pci, PCIE_MSI_INTR0_ENABLE +
-					    (ctrl * MSI_REG_CTRL_BLOCK_SIZE),
-					    ~0);
-		}
-	}
-
 	dw_pcie_msi_init(pp);
 
 	/* Setup RC BARs */
--- a/drivers/pci/controller/dwc/pcie-designware.h
+++ b/drivers/pci/controller/dwc/pcie-designware.h
@@ -678,6 +678,9 @@ static inline enum dw_pcie_ltssm dw_pcie
 int dw_pcie_suspend_noirq(struct dw_pcie *pci);
 int dw_pcie_resume_noirq(struct dw_pcie *pci);
 irqreturn_t dw_handle_msi_irq(struct dw_pcie_rp *pp);
+void dw_pcie_msi_init(struct dw_pcie_rp *pp);
+int dw_pcie_msi_host_init(struct dw_pcie_rp *pp);
+void dw_pcie_free_msi(struct dw_pcie_rp *pp);
 int dw_pcie_setup_rc(struct dw_pcie_rp *pp);
 int dw_pcie_host_init(struct dw_pcie_rp *pp);
 void dw_pcie_host_deinit(struct dw_pcie_rp *pp);
@@ -700,6 +703,17 @@ static inline irqreturn_t dw_handle_msi_
 	return IRQ_NONE;
 }
 
+static inline void dw_pcie_msi_init(struct dw_pcie_rp *pp)
+{ }
+
+static inline int dw_pcie_msi_host_init(struct dw_pcie_rp *pp)
+{
+	return -ENODEV;
+}
+
+static inline void dw_pcie_free_msi(struct dw_pcie_rp *pp)
+{ }
+
 static inline int dw_pcie_setup_rc(struct dw_pcie_rp *pp)
 {
 	return 0;
