// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qcom-ipq4019-whw03.dtsi"

/ {
	model = "Linksys WHW03 V2 (Velop)";
	compatible = "linksys,whw03v2", "qcom,ipq4019";

	// Default bootargs include rootfstype=ext4 and need to be overriden.
	chosen {
		bootargs-append = " root=/dev/ubiblock0_0 rootfstype=squashfs ro";
		stdout-path = &blsp1_uart1;
	};
};

&tlmm {
	i2c_0_pins: i2c-0-pinmux {
		pins = "gpio20", "gpio21";
		function = "blsp_i2c0";
		bias-disable;
	};

	spi_0_pins: spi-0-pinmux {
		mux {
			pins = "gpio13", "gpio14", "gpio15";
			function = "blsp_spi0";
			drive-strength = <12>;
			bias-disable;
		};

		mux-cs {
			pins = "gpio12";
			drive-strength = <2>;
			bias-disable;
			output-high;
		};
	};
};

&spi_1_pins {
	mux-wake {
		pins = "gpio31";
		function = "gpio";
		bias-pull-up;
		output-high;
	};
};

&mdio {
	status = "okay";
	pinctrl-0 = <&mdio_pins>;
	pinctrl-names = "default";

	phy-reset-gpios = <&tlmm 19 GPIO_ACTIVE_LOW>;
};

&ethphy3 {
	reg = <0x1b>;
};

&ethphy4 {
	reg = <0x1c>;
};

&psgmiiphy {
	reg = <0x1d>;
};

&usb3_ss_phy {
	status = "okay";
};

&usb3_hs_phy {
	status = "okay";
};

&usb2_hs_phy {
	status = "okay";
};

&nand {
	status = "okay";

	nand@0 {
		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "SBL1";
				reg = <0x0 0x100000>;
				read-only;
			};

			partition@100000 {
				label = "MIBIB";
				reg = <0x100000 0x100000>;
				read-only;
			};

			partition@200000 {
				label = "QSEE";
				reg = <0x200000 0x100000>;
				read-only;
			};

			partition@300000 {
				label = "CDT";
				reg = <0x300000 0x80000>;
				read-only;
			};

			partition@380000 {
				label = "APPSBL";
				reg = <0x380000 0x200000>;
				read-only;
			};

			partition@580000 {
				label = "ART";
				reg = <0x580000 0x80000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_gmac0: macaddr@0 {
						compatible = "mac-base";
						reg = <0x0 0x6>;
						#nvmem-cell-cells = <1>;
					};

					macaddr_gmac1: macaddr@6 {
						reg = <0x6 0x6>;
					};

					precal_art_1000: precal@1000 {
						reg = <0x1000 0x2f20>;
					};

					precal_art_5000: precal@5000 {
						reg = <0x5000 0x2f20>;
					};

					precal_art_9000: precal@9000 {
						reg = <0x9000 0x2f20>;
					};
				};
			};

			partition@600000 {
				label = "u_env";
				reg = <0x600000 0x80000>;
			};

			partition@680000 {
				label = "s_env";
				reg = <0x680000 0x40000>;
			};

			partition@6c0000 {
				label = "devinfo";
				reg = <0x6c0000 0x40000>;
				read-only;
			};

			partition@700000 {
				label = "kernel";
				reg = <0x700000 0xa100000>;
			};

			partition@d00000 {
				label = "rootfs";
				reg = <0xd00000 0x9b00000>;
			};

			partition@a800000 {
				label = "alt_kernel";
				reg = <0xa800000 0xa100000>;
			};

			partition@ae00000 {
				label = "alt_rootfs";
				reg = <0xae00000 0x9b00000>;
			};

			partition@14900000 {
				label = "sysdiag";
				reg = <0x14900000 0x200000>;
				read-only;
			};

			partition@14b00000 {
				label = "syscfg";
				reg = <0x14b00000 0xb500000>;
				read-only;
			};
		};
	};
};

&qpic_bam {
	status = "okay";
};

&swport4 {
	nvmem-cell-names = "mac-address";
	nvmem-cells = <&macaddr_gmac1>;
};

&swport5 {
	nvmem-cell-names = "mac-address";
	nvmem-cells = <&macaddr_gmac0 0>;
};

&wifi0 {
	qcom,ath10k-calibration-variant = "linksys-whw03v2";

	nvmem-cell-names = "pre-calibration", "mac-address";
	nvmem-cells = <&precal_art_1000>, <&macaddr_gmac0 1>;
};

&wifi1 {
	qcom,ath10k-calibration-variant = "linksys-whw03v2";

	nvmem-cell-names = "pre-calibration", "mac-address";
	nvmem-cells = <&precal_art_5000>, <&macaddr_gmac0 2>;
};

&pcie_bridge0 {
	wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0x00010000 0 0 0 0>;
		ieee80211-freq-limit = <5490000 5835000>;
		nvmem-cell-names = "pre-calibration", "mac-address";
		nvmem-cells = <&precal_art_9000>, <&macaddr_gmac0 3>;
		qcom,ath10k-calibration-variant = "linksys-whw03v2";
	};
};
