From a41519d8b438adc154debd433c3a1436ebb93a10 Mon Sep 17 00:00:00 2001
From: Jonas Karlman <jonas@kwiboo.se>
Date: Wed, 23 Jul 2025 12:23:05 +0000
Subject: [PATCH] arm64: dts: rockchip: Add USB nodes for RK3528

Rockchip RK3528 has one USB 3.0 DWC3 controller, a USB 2.0 EHCI/OHCI
controller and uses a USB2PHY for USB 2.0. The DWC3 controller may also
use the Naneng Combo PHY for USB3.

Add device tree nodes to describe these USB controllers along with the
USB 2.0 PHYs.

Signed-off-by: Jonas Karlman <jonas@kwiboo.se>
---
 arch/arm64/boot/dts/rockchip/rk3528.dtsi | 77 ++++++++++++++++++++++++
 1 file changed, 77 insertions(+)

--- a/arch/arm64/boot/dts/rockchip/rk3528.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3528.dtsi
@@ -336,6 +336,30 @@
 			};
 		};
 
+		usb_host0_xhci: usb@fe500000 {
+			compatible = "rockchip,rk3528-dwc3", "snps,dwc3";
+			reg = <0x0 0xfe500000 0x0 0x400000>;
+			clocks = <&cru CLK_REF_USB3OTG>,
+				 <&cru CLK_SUSPEND_USB3OTG>,
+				 <&cru ACLK_USB3OTG>;
+			clock-names = "ref_clk", "suspend_clk", "bus_clk";
+			interrupts = <GIC_SPI 152 IRQ_TYPE_LEVEL_HIGH>;
+			power-domains = <&power RK3528_PD_VPU>;
+			resets = <&cru SRST_A_USB3OTG>;
+			dr_mode = "otg";
+			phy_type = "utmi_wide";
+			snps,dis_enblslpm_quirk;
+			snps,dis_rxdet_inp3_quirk;
+			snps,dis-del-phy-power-chg-quirk;
+			snps,dis-tx-ipgap-linecheck-quirk;
+			snps,dis-u1-entry-quirk;
+			snps,dis-u2-entry-quirk;
+			snps,dis-u2-freeclk-exists-quirk;
+			snps,parkmode-disable-hs-quirk;
+			snps,parkmode-disable-ss-quirk;
+			status = "disabled";
+		};
+
 		gic: interrupt-controller@fed01000 {
 			compatible = "arm,gic-400";
 			reg = <0x0 0xfed01000 0 0x1000>,
@@ -349,6 +373,30 @@
 			#interrupt-cells = <3>;
 		};
 
+		usb_host0_ehci: usb@ff100000 {
+			compatible = "generic-ehci";
+			reg = <0x0 0xff100000 0x0 0x40000>;
+			clocks = <&cru HCLK_USBHOST>, <&cru HCLK_USBHOST_ARB>,
+				 <&usb2phy>;
+			interrupts = <GIC_SPI 143 IRQ_TYPE_LEVEL_HIGH>;
+			phys = <&usb2phy_host>;
+			phy-names = "usb";
+			power-domains = <&power RK3528_PD_VO>;
+			status = "disabled";
+		};
+
+		usb_host0_ohci: usb@ff140000 {
+			compatible = "generic-ohci";
+			reg = <0x0 0xff140000 0x0 0x40000>;
+			clocks = <&cru HCLK_USBHOST>, <&cru HCLK_USBHOST_ARB>,
+				 <&usb2phy>;
+			interrupts = <GIC_SPI 144 IRQ_TYPE_LEVEL_HIGH>;
+			phys = <&usb2phy_host>;
+			phy-names = "usb";
+			power-domains = <&power RK3528_PD_VO>;
+			status = "disabled";
+		};
+
 		qos_crypto_a: qos@ff200000 {
 			compatible = "rockchip,rk3528-qos", "syscon";
 			reg = <0x0 0xff200000 0x0 0x20>;
@@ -1273,6 +1321,35 @@
 			rockchip,pipe-phy-grf = <&pipe_phy_grf>;
 			status = "disabled";
 		};
+
+		usb2phy: usb2phy@ffdf0000 {
+			compatible = "rockchip,rk3528-usb2phy";
+			reg = <0x0 0xffdf0000 0x0 0x10000>;
+			clocks = <&cru CLK_REF_USBPHY>, <&cru PCLK_USBPHY>;
+			clock-names = "phyclk", "pclk";
+			#clock-cells = <0>;
+			clock-output-names = "clk_usbphy_480m";
+			power-domains = <&power RK3528_PD_VO>;
+			rockchip,usbgrf = <&vo_grf>;
+			status = "disabled";
+
+			usb2phy_otg: otg-port {
+				interrupts = <GIC_SPI 146 IRQ_TYPE_LEVEL_HIGH>,
+					     <GIC_SPI 147 IRQ_TYPE_LEVEL_HIGH>,
+					     <GIC_SPI 148 IRQ_TYPE_LEVEL_HIGH>;
+				interrupt-names = "otg-bvalid", "otg-id",
+						  "linestate";
+				#phy-cells = <0>;
+				status = "disabled";
+			};
+
+			usb2phy_host: host-port {
+				interrupts = <GIC_SPI 150 IRQ_TYPE_LEVEL_HIGH>;
+				interrupt-names = "linestate";
+				#phy-cells = <0>;
+				status = "disabled";
+			};
+		};
 	};
 };
 
