From 2115cbeec8a3ccc69e3b7ecdf97b4472b0829cfc Mon Sep 17 00:00:00 2001
From: Florin Leotescu <florin.leotescu@nxp.com>
Date: Fri, 21 Mar 2025 16:33:08 +0200
Subject: [PATCH] hwmon: emc2305: Use devm_thermal_of_cooling_device_register

Prepare the emc2305 driver to use configuration from Device Tree nodes.
Switch to devm_thermal_of_cooling_device_register to simplify the
cleanup procedure, allowing the removal of emc2305_unset_tz and
emc2305_remove, which are no longer needed.

Signed-off-by: Florin Leotescu <florin.leotescu@nxp.com>
Reviewed-by: Frank Li <Frank.Li@nxp.com>
Link: https://lore.kernel.org/r/20250321143308.4008623-4-florin.leotescu@oss.nxp.com
Signed-off-by: Guenter Roeck <linux@roeck-us.net>
---
 drivers/hwmon/emc2305.c | 33 ++++-----------------------------
 1 file changed, 4 insertions(+), 29 deletions(-)

--- a/drivers/hwmon/emc2305.c
+++ b/drivers/hwmon/emc2305.c
@@ -112,8 +112,6 @@ static char *emc2305_fan_name[] = {
 	"emc2305_fan5",
 };
 
-static void emc2305_unset_tz(struct device *dev);
-
 static int emc2305_get_max_channel(const struct emc2305_data *data)
 {
 	return data->pwm_num;
@@ -293,8 +291,9 @@ static int emc2305_set_single_tz(struct
 	pwm = data->pwm_min[cdev_idx];
 
 	data->cdev_data[cdev_idx].cdev =
-		thermal_cooling_device_register(emc2305_fan_name[idx], data,
-						&emc2305_cooling_ops);
+		devm_thermal_of_cooling_device_register(dev, dev->of_node,
+							emc2305_fan_name[idx], data,
+							&emc2305_cooling_ops);
 
 	if (IS_ERR(data->cdev_data[cdev_idx].cdev)) {
 		dev_err(dev, "Failed to register cooling device %s\n", emc2305_fan_name[idx]);
@@ -338,24 +337,9 @@ static int emc2305_set_tz(struct device
 	for (i = 0; i < data->pwm_num; i++) {
 		ret = emc2305_set_single_tz(dev, i + 1);
 		if (ret)
-			goto thermal_cooling_device_register_fail;
+			return ret;
 	}
 	return 0;
-
-thermal_cooling_device_register_fail:
-	emc2305_unset_tz(dev);
-	return ret;
-}
-
-static void emc2305_unset_tz(struct device *dev)
-{
-	struct emc2305_data *data = dev_get_drvdata(dev);
-	int i;
-
-	/* Unregister cooling device. */
-	for (i = 0; i < EMC2305_PWM_MAX; i++)
-		if (data->cdev_data[i].cdev)
-			thermal_cooling_device_unregister(data->cdev_data[i].cdev);
 }
 
 static umode_t
@@ -605,14 +589,6 @@ static int emc2305_probe(struct i2c_clie
 	return 0;
 }
 
-static void emc2305_remove(struct i2c_client *client)
-{
-	struct device *dev = &client->dev;
-
-	if (IS_REACHABLE(CONFIG_THERMAL))
-		emc2305_unset_tz(dev);
-}
-
 static const struct of_device_id of_emc2305_match_table[] = {
 	{ .compatible = "microchip,emc2305", },
 	{},
@@ -625,7 +601,6 @@ static struct i2c_driver emc2305_driver
 		.of_match_table = of_emc2305_match_table,
 	},
 	.probe = emc2305_probe,
-	.remove	  = emc2305_remove,
 	.id_table = emc2305_ids,
 };
 
