// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

/dts-v1/;

#define STRINGIZE(s) #s
#define LAN_LABEL(p, s) STRINGIZE(p ## s)
#define SWITCH_PORT_LABEL(n) LAN_LABEL(lan, n)

#define PHY_C22(p, n) \
	phy##p: ethernet-phy@n { \
		reg = <##n>; \
		compatible = "ethernet-phy-ieee802.3-c22"; \
	};

#define PHY_C22_SFP(p, n, s) \
	phy##p: ethernet-phy@n { \
		reg = <##n>; \
		compatible = "ethernet-phy-ieee802.3-c22"; \
		sfp = <&sfp##s>; \
	};

#define PHY_C45(p, n) \
	phy##p: ethernet-phy@n { \
		reg = <##n>; \
		compatible = "ethernet-phy-ieee802.3-c45"; \
	};

#define PHY_C45_PAIR_ORDER(p, n, po) \
	phy##p: ethernet-phy@n { \
		reg = <##n>; \
		compatible = "ethernet-phy-ieee802.3-c45"; \
		enet-phy-pair-order = <##po>; \
	};

#define SWITCH_PORT(p, l, m) \
	port##p: port@##p { \
		reg = <##p>; \
		label = SWITCH_PORT_LABEL(l) ; \
		phy-handle = <&phy##p>; \
		phy-mode = #m ; \
	};

#define SWITCH_PORT_SDS(p, l, s, m) \
	port##p: port@##p { \
		reg = <##p>; \
		label = SWITCH_PORT_LABEL(l) ; \
		pcs-handle = <&serdes##s>; \
		phy-handle = <&phy##p>; \
		phy-mode = #m ; \
	};

#define SWITCH_PORT_LED(p, l, s, c, m) \
	port##p: port@##p { \
		reg = <##p>; \
		label = SWITCH_PORT_LABEL(l) ; \
		led-set = <##c>; \
		pcs-handle = <&serdes##s>; \
		phy-handle = <&phy##p>; \
		phy-mode = #m ; \
	};

#define SWITCH_PORT_SFP(p, l, s, c, g) \
	port##p: port@##p { \
		reg = <##p>; \
		label = SWITCH_PORT_LABEL(l) ; \
		led-set = <##c>; \
		pcs-handle = <&serdes##s>; \
		phy-mode = "1000base-x"; \
		sfp = <&sfp##g>; \
		managed = "in-band-status"; \
	};

/* LED Set mode definitions */
#define RTL93XX_LED_SET_NONE        (0)
#define RTL93XX_LED_SET_10G         (1 << 0)
#define RTL93XX_LED_SET_5G          (1 << 1)
#define RTL93XX_LED_SET_2P5G        (1 << 3)
#define RTL93XX_LED_SET_1G          (1 << 5)
#define RTL93XX_LED_SET_100M        (1 << 7)
#define RTL93XX_LED_SET_10M         (1 << 8)
#define RTL93XX_LED_SET_LINK        (1 << 9)
#define RTL93XX_LED_SET_LINK_BLINK  (1 << 10)
#define RTL93XX_LED_SET_ACT         (1 << 11)
#define RTL93XX_LED_SET_RX          (1 << 12)
#define RTL93XX_LED_SET_TX          (1 << 13)
#define RTL93XX_LED_SET_COLLISION   (1 << 14)
#define RTL93XX_LED_SET_DUPLEX      (1 << 15)

/* LED Interface modes */
#define RTL93XX_LED_MODE_SERIAL             1
#define RTL93XX_LED_MODE_SINGLE_COLOR_SCAN  2
#define RTL93XX_LED_MODE_BI_COLOR_SCAN      3
