From 572304faf8c1d30f142060c76a3e731438fc5975 Mon Sep 17 00:00:00 2001
From: Jonas Jelonek <jelonek.jonas@gmail.com>
Date: Thu, 22 Jan 2026 10:59:20 +0000
Subject: [PATCH net-next v6 1/2] net: sfp: apply I2C adapter quirks to limit
 block size

The SFP driver assumes all I2C adapters support reading and writing the
pre-defined block size SFP_EEPROM_BLOCK_SIZE of 16 bytes. This constant
was probably chosen based on good guesses and known limitations of a
range of I2C adapters and SFP modules.

However, I2C adapters may even support less and usually need to specify
this via I2C quirks. Theoretically, such an adapter may provide full
functionality but only support a read and write length of e.g. 8 bytes.
Currently, the SFP driver doesn't account for that.

Add handling for I2C quirks in SFP I2C configuration taking the fields
max_read_len and max_write_len in struct i2c_adapter_quirks into account
to further limit the maximum block size if needed.

Signed-off-by: Jonas Jelonek <jelonek.jonas@gmail.com>
---
 drivers/net/phy/sfp.c | 12 ++++++++++--
 1 file changed, 10 insertions(+), 2 deletions(-)

--- a/drivers/net/phy/sfp.c
+++ b/drivers/net/phy/sfp.c
@@ -809,21 +809,29 @@ static int sfp_smbus_byte_write(struct s
 
 static int sfp_i2c_configure(struct sfp *sfp, struct i2c_adapter *i2c)
 {
+	size_t max_block_size;
+
 	sfp->i2c = i2c;
 
 	if (i2c_check_functionality(i2c, I2C_FUNC_I2C)) {
 		sfp->read = sfp_i2c_read;
 		sfp->write = sfp_i2c_write;
-		sfp->i2c_max_block_size = SFP_EEPROM_BLOCK_SIZE;
+		max_block_size = SFP_EEPROM_BLOCK_SIZE;
 	} else if (i2c_check_functionality(i2c, I2C_FUNC_SMBUS_BYTE_DATA)) {
 		sfp->read = sfp_smbus_byte_read;
 		sfp->write = sfp_smbus_byte_write;
-		sfp->i2c_max_block_size = 1;
+		max_block_size = 1;
 	} else {
 		sfp->i2c = NULL;
 		return -EINVAL;
 	}
 
+	if (i2c->quirks && i2c->quirks->max_read_len)
+		max_block_size = min(max_block_size, i2c->quirks->max_read_len);
+	if (i2c->quirks && i2c->quirks->max_write_len)
+		max_block_size = min(max_block_size, i2c->quirks->max_write_len);
+
+	sfp->i2c_max_block_size = max_block_size;
 	return 0;
 }
 
