--- /dev/null
+++ b/mibs/BGP4-MIB.txt
@@ -0,0 +1,929 @@
+    BGP4-MIB DEFINITIONS ::= BEGIN
+
+        IMPORTS
+            MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,
+            IpAddress, Integer32, Counter32, Gauge32, mib-2
+                FROM SNMPv2-SMI
+            MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
+                FROM SNMPv2-CONF;
+
+        bgp MODULE-IDENTITY
+            LAST-UPDATED "9902100000Z"
+            ORGANIZATION "IETF IDR Working Group"
+            CONTACT-INFO "E-mail:  idr@merit.net
+
+                          Susan Hares  (Editor)
+                          Merit Network
+                          4251 Plymouth Road
+                          Suite C
+                          Ann Arbor, MI 48105-2785
+                          Tel: +1 734 936 2095
+                          Fax: +1 734 647 3185
+                          E-mail: skh@merit.edu
+
+                          Jeff Johnson (Editor)
+                          RedBack Networks, Inc.
+                          1389 Moffett Park Drive
+                          Sunnyvale, CA  94089-1134
+                          Tel: +1 408 548 3516
+                          Fax: +1 408 548 3599
+                          E-mail: jeff@redback.com"
+            DESCRIPTION
+                    "The MIB module for BGP-4."
+            REVISION    "9902100000Z"
+            DESCRIPTION
+                    "Corrected duplicate OBJECT IDENTIFIER
+                     assignment in the conformance information."
+            REVISION    "9601080000Z"
+            DESCRIPTION
+                    "1) Fixed the definitions of the traps to
+                     make them equivalent to their initial
+                     definition in RFC 1269.
+                     2) Added compliance and conformance info."
+            ::= { mib-2 15 }
+
+        bgpVersion OBJECT-TYPE
+            SYNTAX     OCTET STRING (SIZE (1..255))
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "Vector of supported BGP protocol version
+                    numbers.  Each peer negotiates the version
+                    from this vector.  Versions are identified
+                    via the string of bits contained within this
+                    object.  The first octet contains bits 0 to
+                    7, the second octet contains bits 8 to 15,
+                    and so on, with the most significant bit
+                    referring to the lowest bit number in the
+                    octet (e.g., the MSB of the first octet
+                    refers to bit 0).  If a bit, i, is present
+                    and set, then the version (i+1) of the BGP
+                    is supported."
+            ::= { bgp 1 }
+
+        bgpLocalAs OBJECT-TYPE
+            SYNTAX     INTEGER (0..65535)
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The local autonomous system number."
+            ::= { bgp 2 }
+
+
+
+        -- BGP Peer table.  This table contains, one entry per BGP
+        -- peer, information about the BGP peer.
+
+        bgpPeerTable OBJECT-TYPE
+            SYNTAX     SEQUENCE OF BgpPeerEntry
+            MAX-ACCESS not-accessible
+            STATUS     current
+            DESCRIPTION
+                    "BGP peer table.  This table contains,
+                    one entry per BGP peer, information about the
+                    connections with BGP peers."
+            ::= { bgp 3 }
+
+        bgpPeerEntry OBJECT-TYPE
+            SYNTAX     BgpPeerEntry
+            MAX-ACCESS not-accessible
+            STATUS     current
+            DESCRIPTION
+                    "Entry containing information about the
+                    connection with a BGP peer."
+            INDEX { bgpPeerRemoteAddr }
+            ::= { bgpPeerTable 1 }
+
+        BgpPeerEntry ::= SEQUENCE {
+                bgpPeerIdentifier
+                    IpAddress,
+                bgpPeerState
+                    INTEGER,
+                bgpPeerAdminStatus
+                    INTEGER,
+                bgpPeerNegotiatedVersion
+                    Integer32,
+                bgpPeerLocalAddr
+                    IpAddress,
+                bgpPeerLocalPort
+                    INTEGER,
+                bgpPeerRemoteAddr
+                    IpAddress,
+                bgpPeerRemotePort
+                    INTEGER,
+                bgpPeerRemoteAs
+                    INTEGER,
+                bgpPeerInUpdates
+                    Counter32,
+                bgpPeerOutUpdates
+                    Counter32,
+                bgpPeerInTotalMessages
+                    Counter32,
+                bgpPeerOutTotalMessages
+                    Counter32,
+                bgpPeerLastError
+                    OCTET STRING,
+                bgpPeerFsmEstablishedTransitions
+                    Counter32,
+                bgpPeerFsmEstablishedTime
+                    Gauge32,
+                bgpPeerConnectRetryInterval
+                    INTEGER,
+                bgpPeerHoldTime
+                    INTEGER,
+                bgpPeerKeepAlive
+                    INTEGER,
+                bgpPeerHoldTimeConfigured
+                    INTEGER,
+                bgpPeerKeepAliveConfigured
+                    INTEGER,
+                bgpPeerMinASOriginationInterval
+                    INTEGER,
+                bgpPeerMinRouteAdvertisementInterval
+                    INTEGER,
+                bgpPeerInUpdateElapsedTime
+                    Gauge32
+                }
+
+        bgpPeerIdentifier OBJECT-TYPE
+            SYNTAX     IpAddress
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The BGP Identifier of this entry's BGP peer."
+            ::= { bgpPeerEntry 1 }
+
+        bgpPeerState OBJECT-TYPE
+            SYNTAX     INTEGER {
+                                idle(1),
+                                connect(2),
+                                active(3),
+                                opensent(4),
+                                openconfirm(5),
+                                established(6)
+                       }
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The BGP peer connection state."
+            ::= { bgpPeerEntry 2 }
+
+        bgpPeerAdminStatus OBJECT-TYPE
+            SYNTAX     INTEGER {
+                                stop(1),
+                                start(2)
+                       }
+            MAX-ACCESS read-write
+            STATUS     current
+            DESCRIPTION
+                    "The desired state of the BGP connection.  A
+                    transition from 'stop' to 'start' will cause
+                    the BGP Start Event to be generated.  A
+                    transition from 'start' to 'stop' will cause
+                    the BGP Stop Event to be generated.  This
+                    parameter can be used to restart BGP peer
+                    connections.  Care should be used in providing
+                    write access to this object without adequate
+                    authentication."
+            ::= { bgpPeerEntry 3 }
+
+        bgpPeerNegotiatedVersion OBJECT-TYPE
+            SYNTAX     Integer32
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The negotiated version of BGP running between
+                    the two peers."
+            ::= { bgpPeerEntry 4 }
+
+        bgpPeerLocalAddr OBJECT-TYPE
+            SYNTAX     IpAddress
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The local IP address of this entry's BGP
+                    connection."
+            ::= { bgpPeerEntry 5 }
+
+        bgpPeerLocalPort OBJECT-TYPE
+            SYNTAX     INTEGER (0..65535)
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The local port for the TCP connection between
+                    the BGP peers."
+            ::= { bgpPeerEntry 6 }
+
+        bgpPeerRemoteAddr OBJECT-TYPE
+            SYNTAX     IpAddress
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The remote IP address of this entry's BGP
+                    peer."
+            ::= { bgpPeerEntry 7 }
+
+        bgpPeerRemotePort OBJECT-TYPE
+            SYNTAX     INTEGER (0..65535)
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The remote port for the TCP connection between
+                    the BGP peers.  Note that the objects
+                    bgpPeerLocalAddr, bgpPeerLocalPort,
+                    bgpPeerRemoteAddr and bgpPeerRemotePort
+                    provide the appropriate reference to the
+                    standard MIB TCP connection table."
+            ::= { bgpPeerEntry 8 }
+
+        bgpPeerRemoteAs OBJECT-TYPE
+            SYNTAX     INTEGER (0..65535)
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The remote autonomous system number."
+            ::= { bgpPeerEntry 9 }
+
+        bgpPeerInUpdates OBJECT-TYPE
+            SYNTAX     Counter32
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The number of BGP UPDATE messages received on
+                    this connection.  This object should be
+                    initialized to zero (0) when the connection is
+                    established."
+            ::= { bgpPeerEntry 10 }
+
+        bgpPeerOutUpdates OBJECT-TYPE
+            SYNTAX     Counter32
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The number of BGP UPDATE messages transmitted
+                    on this connection.  This object should be
+                    initialized to zero (0) when the connection is
+                    established."
+            ::= { bgpPeerEntry 11 }
+
+        bgpPeerInTotalMessages OBJECT-TYPE
+            SYNTAX     Counter32
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The total number of messages received from the
+                    remote peer on this connection.  This object
+                    should be initialized to zero when the
+                    connection is established."
+            ::= { bgpPeerEntry 12 }
+
+        bgpPeerOutTotalMessages OBJECT-TYPE
+            SYNTAX     Counter32
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The total number of messages transmitted to
+                    the remote peer on this connection.  This object
+                    should be initialized to zero when the
+                    connection is established."
+            ::= { bgpPeerEntry 13 }
+
+        bgpPeerLastError OBJECT-TYPE
+            SYNTAX     OCTET STRING (SIZE (2))
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The last error code and subcode seen by this
+                    peer on this connection.  If no error has
+                    occurred, this field is zero.  Otherwise, the
+                    first byte of this two byte OCTET STRING
+                    contains the error code, and the second byte
+                    contains the subcode."
+            ::= { bgpPeerEntry 14 }
+
+        bgpPeerFsmEstablishedTransitions OBJECT-TYPE
+            SYNTAX     Counter32
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The total number of times the BGP FSM
+                    transitioned into the established state."
+            ::= { bgpPeerEntry 15 }
+
+        bgpPeerFsmEstablishedTime OBJECT-TYPE
+            SYNTAX     Gauge32
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "This timer indicates how long (in seconds) this
+                    peer has been in the Established state or how long
+                    since this peer was last in the Established state.
+                    It is set to zero when a new peer is configured or
+                    the router is booted."
+            ::= { bgpPeerEntry 16 }
+
+        bgpPeerConnectRetryInterval OBJECT-TYPE
+            SYNTAX     INTEGER (1..65535)
+            MAX-ACCESS read-write
+            STATUS     current
+            DESCRIPTION
+                    "Time interval in seconds for the ConnectRetry
+                    timer.  The suggested value for this timer is
+                    120 seconds."
+            ::= { bgpPeerEntry 17 }
+
+        bgpPeerHoldTime OBJECT-TYPE
+            SYNTAX     INTEGER  ( 0 | 3..65535 )
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "Time interval in seconds for the Hold Timer
+                    established with the peer.  The value of this
+                    object is calculated by this BGP speaker by
+                    using the smaller of the value in
+                    bgpPeerHoldTimeConfigured and the Hold Time
+                    received in the OPEN message.  This value
+                    must be at lease three seconds if it is not
+                    zero (0) in which case the Hold Timer has
+                    not been established with the peer, or, the
+                    value of bgpPeerHoldTimeConfigured is zero (0)."
+            ::= { bgpPeerEntry 18 }
+
+        bgpPeerKeepAlive OBJECT-TYPE
+            SYNTAX     INTEGER ( 0 | 1..21845 )
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "Time interval in seconds for the KeepAlive
+                    timer established with the peer.  The value of
+                    this object is calculated by this BGP speaker
+                    such that, when compared with bgpPeerHoldTime,
+                    it has the same proportion as what
+                    bgpPeerKeepAliveConfigured has when compared
+                    with bgpPeerHoldTimeConfigured.  If the value
+                    of this object is zero (0), it indicates that
+                    the KeepAlive timer has not been established
+                    with the peer, or, the value of
+                    bgpPeerKeepAliveConfigured is zero (0)."
+            ::= { bgpPeerEntry 19 }
+
+        bgpPeerHoldTimeConfigured OBJECT-TYPE
+            SYNTAX     INTEGER ( 0 | 3..65535 )
+            MAX-ACCESS read-write
+            STATUS     current
+            DESCRIPTION
+                    "Time interval in seconds for the Hold Time
+                    configured for this BGP speaker with this peer.
+                    This value is placed in an OPEN message sent to
+                    this peer by this BGP speaker, and is compared
+                    with the Hold Time field in an OPEN message
+                    received from the peer when determining the Hold
+                    Time (bgpPeerHoldTime) with the peer.  This value
+                    must not be less than three seconds if it is not
+                    zero (0) in which case the Hold Time is NOT to be
+                    established with the peer.  The suggested value for
+                    this timer is 90 seconds."
+            ::= { bgpPeerEntry 20 }
+
+        bgpPeerKeepAliveConfigured OBJECT-TYPE
+            SYNTAX     INTEGER ( 0 | 1..21845 )
+            MAX-ACCESS read-write
+            STATUS     current
+            DESCRIPTION
+                    "Time interval in seconds for the KeepAlive timer
+                    configured for this BGP speaker with this peer.
+                    The value of this object will only determine the
+                    KEEPALIVE messages' frequency relative to the value
+                    specified in bgpPeerHoldTimeConfigured; the actual
+                    time interval for the KEEPALIVE messages is
+                    indicated by bgpPeerKeepAlive.  A reasonable
+                    maximum value for this timer would be configured to
+                    be one third of that of bgpPeerHoldTimeConfigured.
+                    If the value of this object is zero (0), no
+                    periodical KEEPALIVE messages are sent to the peer
+                    after the BGP connection has been established.  The
+                    suggested value for this timer is 30 seconds."
+            ::= { bgpPeerEntry 21 }
+
+        bgpPeerMinASOriginationInterval OBJECT-TYPE
+            SYNTAX     INTEGER (1..65535)
+            MAX-ACCESS read-write
+            STATUS     current
+            DESCRIPTION
+                    "Time interval in seconds for the
+                    MinASOriginationInterval timer.
+                    The suggested value for this timer is 15 seconds."
+            ::= { bgpPeerEntry 22 }
+
+        bgpPeerMinRouteAdvertisementInterval OBJECT-TYPE
+            SYNTAX     INTEGER (1..65535)
+            MAX-ACCESS read-write
+            STATUS     current
+            DESCRIPTION
+                    "Time interval in seconds for the
+                    MinRouteAdvertisementInterval timer.
+                    The suggested value for this timer is 30 seconds."
+            ::= { bgpPeerEntry 23 }
+
+        bgpPeerInUpdateElapsedTime OBJECT-TYPE
+            SYNTAX     Gauge32
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "Elapsed time in seconds since the last BGP
+                    UPDATE message was received from the peer.
+                    Each time bgpPeerInUpdates is incremented,
+                    the value of this object is set to zero (0)."
+            ::= { bgpPeerEntry 24 }
+
+
+
+        bgpIdentifier OBJECT-TYPE
+            SYNTAX     IpAddress
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The BGP Identifier of local system."
+            ::= { bgp 4 }
+
+
+
+        -- Received Path Attribute Table.  This table contains,
+        -- one entry per path to a network, path attributes
+        -- received from all peers running BGP version 3 or less.
+        -- This table is obsolete, having been replaced in
+        -- functionality with the bgp4PathAttrTable.
+
+        bgpRcvdPathAttrTable OBJECT-TYPE
+            SYNTAX     SEQUENCE OF BgpPathAttrEntry
+            MAX-ACCESS not-accessible
+            STATUS     obsolete
+            DESCRIPTION
+                    "The BGP Received Path Attribute Table contains
+                    information about paths to destination networks
+                    received from all peers running BGP version 3 or
+                    less."
+            ::= { bgp 5 }
+
+        bgpPathAttrEntry OBJECT-TYPE
+            SYNTAX     BgpPathAttrEntry
+            MAX-ACCESS not-accessible
+            STATUS     obsolete
+            DESCRIPTION
+                    "Information about a path to a network."
+            INDEX { bgpPathAttrDestNetwork,
+                    bgpPathAttrPeer        }
+            ::= { bgpRcvdPathAttrTable 1 }
+
+        BgpPathAttrEntry ::= SEQUENCE {
+            bgpPathAttrPeer
+                 IpAddress,
+            bgpPathAttrDestNetwork
+                 IpAddress,
+            bgpPathAttrOrigin
+                 INTEGER,
+            bgpPathAttrASPath
+                 OCTET STRING,
+            bgpPathAttrNextHop
+                 IpAddress,
+            bgpPathAttrInterASMetric
+                 Integer32
+        }
+
+        bgpPathAttrPeer OBJECT-TYPE
+            SYNTAX     IpAddress
+            MAX-ACCESS read-only
+            STATUS     obsolete
+            DESCRIPTION
+                    "The IP address of the peer where the path
+                    information was learned."
+            ::= { bgpPathAttrEntry 1 }
+
+        bgpPathAttrDestNetwork OBJECT-TYPE
+            SYNTAX     IpAddress
+            MAX-ACCESS read-only
+            STATUS     obsolete
+            DESCRIPTION
+                    "The address of the destination network."
+            ::= { bgpPathAttrEntry 2 }
+
+        bgpPathAttrOrigin OBJECT-TYPE
+            SYNTAX     INTEGER {
+                           igp(1),-- networks are interior
+                           egp(2),-- networks learned via EGP
+                           incomplete(3) -- undetermined
+                       }
+            MAX-ACCESS read-only
+            STATUS     obsolete
+            DESCRIPTION
+                 "The ultimate origin of the path information."
+            ::= { bgpPathAttrEntry 3 }
+
+        bgpPathAttrASPath OBJECT-TYPE
+            SYNTAX     OCTET STRING (SIZE (2..255))
+            MAX-ACCESS read-only
+            STATUS     obsolete
+            DESCRIPTION
+                    "The set of ASs that must be traversed to reach
+                    the network.  This object is probably best
+                    represented as SEQUENCE OF INTEGER.  For SMI
+                    compatibility, though, it is represented as
+                    OCTET STRING.  Each AS is represented as a pair
+                    of octets according to the following algorithm:
+
+                        first-byte-of-pair = ASNumber / 256;
+                        second-byte-of-pair = ASNumber & 255;"
+            ::= { bgpPathAttrEntry 4 }
+
+        bgpPathAttrNextHop OBJECT-TYPE
+            SYNTAX     IpAddress
+            MAX-ACCESS read-only
+            STATUS     obsolete
+            DESCRIPTION
+                    "The address of the border router that should
+                    be used for the destination network."
+            ::= { bgpPathAttrEntry 5 }
+
+        bgpPathAttrInterASMetric OBJECT-TYPE
+            SYNTAX     Integer32
+            MAX-ACCESS read-only
+            STATUS     obsolete
+            DESCRIPTION
+                    "The optional inter-AS metric.  If this
+                    attribute has not been provided for this route,
+                    the value for this object is 0."
+            ::= { bgpPathAttrEntry 6 }
+
+
+
+        -- BGP-4 Received Path Attribute Table.  This table contains,
+        -- one entry per path to a network, path attributes
+        -- received from all peers running BGP-4.
+
+        bgp4PathAttrTable OBJECT-TYPE
+            SYNTAX     SEQUENCE OF Bgp4PathAttrEntry
+            MAX-ACCESS not-accessible
+            STATUS     current
+            DESCRIPTION
+                    "The BGP-4 Received Path Attribute Table contains
+                    information about paths to destination networks
+                    received from all BGP4 peers."
+            ::= { bgp 6 }
+
+        bgp4PathAttrEntry OBJECT-TYPE
+            SYNTAX     Bgp4PathAttrEntry
+            MAX-ACCESS not-accessible
+            STATUS     current
+            DESCRIPTION
+                    "Information about a path to a network."
+            INDEX { bgp4PathAttrIpAddrPrefix,
+                    bgp4PathAttrIpAddrPrefixLen,
+                    bgp4PathAttrPeer            }
+            ::= { bgp4PathAttrTable 1 }
+
+        Bgp4PathAttrEntry ::= SEQUENCE {
+            bgp4PathAttrPeer
+                 IpAddress,
+            bgp4PathAttrIpAddrPrefixLen
+                 INTEGER,
+            bgp4PathAttrIpAddrPrefix
+                 IpAddress,
+            bgp4PathAttrOrigin
+                 INTEGER,
+            bgp4PathAttrASPathSegment
+                 OCTET STRING,
+            bgp4PathAttrNextHop
+                 IpAddress,
+            bgp4PathAttrMultiExitDisc
+                 INTEGER,
+            bgp4PathAttrLocalPref
+                 INTEGER,
+            bgp4PathAttrAtomicAggregate
+                 INTEGER,
+            bgp4PathAttrAggregatorAS
+                 INTEGER,
+            bgp4PathAttrAggregatorAddr
+                 IpAddress,
+            bgp4PathAttrCalcLocalPref
+                 INTEGER,
+            bgp4PathAttrBest
+                 INTEGER,
+            bgp4PathAttrUnknown
+                 OCTET STRING
+        }
+
+        bgp4PathAttrPeer OBJECT-TYPE
+            SYNTAX     IpAddress
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The IP address of the peer where the path
+                    information was learned."
+            ::= { bgp4PathAttrEntry 1 }
+        bgp4PathAttrIpAddrPrefixLen OBJECT-TYPE
+            SYNTAX     INTEGER (0..32)
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "Length in bits of the IP address prefix in the
+                    Network Layer Reachability Information field."
+            ::= { bgp4PathAttrEntry 2 }
+
+        bgp4PathAttrIpAddrPrefix OBJECT-TYPE
+            SYNTAX     IpAddress
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "An IP address prefix in the Network Layer
+                    Reachability Information field.  This object
+                    is an IP address containing the prefix with
+                    length specified by bgp4PathAttrIpAddrPrefixLen.
+                    Any bits beyond the length specified by
+                    bgp4PathAttrIpAddrPrefixLen are zeroed."
+            ::= { bgp4PathAttrEntry 3 }
+
+        bgp4PathAttrOrigin OBJECT-TYPE
+            SYNTAX     INTEGER {
+                                 igp(1),-- networks are interior
+                                 egp(2),-- networks learned via EGP
+                                 incomplete(3) -- undetermined
+                               }
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The ultimate origin of the path information."
+            ::= { bgp4PathAttrEntry 4 }
+
+        bgp4PathAttrASPathSegment OBJECT-TYPE
+            SYNTAX     OCTET STRING (SIZE (2..255))
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The sequence of AS path segments.  Each AS
+                    path segment is represented by a triple
+                    <type, length, value>.
+
+                    The type is a 1-octet field which has two
+                    possible values:
+                         1      AS_SET: unordered set of ASs a
+                                     route in the UPDATE message
+                                     has traversed
+                         2      AS_SEQUENCE: ordered set of ASs
+                                     a route in the UPDATE message
+                                     has traversed.
+
+                    The length is a 1-octet field containing the
+                    number of ASs in the value field.
+
+                    The value field contains one or more AS
+                    numbers, each AS is represented in the octet
+                    string as a pair of octets according to the
+                    following algorithm:
+
+                        first-byte-of-pair = ASNumber / 256;
+                        second-byte-of-pair = ASNumber & 255;"
+            ::= { bgp4PathAttrEntry 5 }
+
+        bgp4PathAttrNextHop OBJECT-TYPE
+            SYNTAX     IpAddress
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The address of the border router that should
+                    be used for the destination network."
+            ::= { bgp4PathAttrEntry 6 }
+
+        bgp4PathAttrMultiExitDisc OBJECT-TYPE
+            SYNTAX     INTEGER (-1..2147483647)
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "This metric is used to discriminate between
+                    multiple exit points to an adjacent autonomous
+                    system.  A value of -1 indicates the absence of
+                    this attribute."
+            ::= { bgp4PathAttrEntry 7 }
+
+        bgp4PathAttrLocalPref OBJECT-TYPE
+            SYNTAX     INTEGER (-1..2147483647)
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The originating BGP4 speaker's degree of
+                    preference for an advertised route.  A value of
+                    -1 indicates the absence of this attribute."
+            ::= { bgp4PathAttrEntry 8 }
+
+        bgp4PathAttrAtomicAggregate OBJECT-TYPE
+            SYNTAX     INTEGER {
+                           lessSpecificRrouteNotSelected(1),
+                           lessSpecificRouteSelected(2)
+                       }
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "Whether or not a system has selected
+                    a less specific route without selecting a
+                    more specific route."
+            ::= { bgp4PathAttrEntry 9 }
+
+        bgp4PathAttrAggregatorAS OBJECT-TYPE
+            SYNTAX     INTEGER (0..65535)
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The AS number of the last BGP4 speaker that
+                    performed route aggregation.  A value of zero (0)
+                    indicates the absence of this attribute."
+            ::= { bgp4PathAttrEntry 10 }
+
+        bgp4PathAttrAggregatorAddr OBJECT-TYPE
+            SYNTAX     IpAddress
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The IP address of the last BGP4 speaker that
+                     performed route aggregation.  A value of
+                     0.0.0.0 indicates the absence of this attribute."
+            ::= { bgp4PathAttrEntry 11 }
+
+        bgp4PathAttrCalcLocalPref OBJECT-TYPE
+            SYNTAX     INTEGER (-1..2147483647)
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "The degree of preference calculated by the
+                    receiving BGP4 speaker for an advertised route.
+                    A value of -1 indicates the absence of this
+                    attribute."
+            ::= { bgp4PathAttrEntry 12 }
+
+        bgp4PathAttrBest OBJECT-TYPE
+            SYNTAX     INTEGER {
+                           false(1),-- not chosen as best route
+                           true(2) -- chosen as best route
+                       }
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "An indication of whether or not this route
+                    was chosen as the best BGP4 route."
+            ::= { bgp4PathAttrEntry 13 }
+
+        bgp4PathAttrUnknown OBJECT-TYPE
+            SYNTAX     OCTET STRING (SIZE(0..255))
+            MAX-ACCESS read-only
+            STATUS     current
+            DESCRIPTION
+                    "One or more path attributes not understood
+                     by this BGP4 speaker.  Size zero (0) indicates
+                     the absence of such attribute(s).  Octets
+                     beyond the maximum size, if any, are not
+                     recorded by this object."
+            ::= { bgp4PathAttrEntry 14 }
+
+
+        -- Traps.
+
+        -- note that in RFC 1657, bgpTraps was incorrectly
+        -- assigned a value of { bgp 7 }, and each of the
+        -- traps had the bgpPeerRemoteAddr object inappropriately
+        -- removed from their OBJECTS clause.  The following
+        -- definitions restore the semantics of the traps as
+        -- they were initially defined in RFC 1269.
+
+        -- { bgp 7 } is unused
+
+        bgpTraps          OBJECT IDENTIFIER ::= { bgp 0 }
+
+        bgpEstablished NOTIFICATION-TYPE
+            OBJECTS { bgpPeerRemoteAddr,
+                      bgpPeerLastError,
+                      bgpPeerState      }
+            STATUS  current
+            DESCRIPTION
+                    "The BGP Established event is generated when
+                    the BGP FSM enters the ESTABLISHED state."
+            ::= { bgpTraps 1 }
+
+        bgpBackwardTransition NOTIFICATION-TYPE
+            OBJECTS { bgpPeerRemoteAddr,
+                      bgpPeerLastError,
+                      bgpPeerState      }
+            STATUS  current
+            DESCRIPTION
+                    "The BGPBackwardTransition Event is generated
+                    when the BGP FSM moves from a higher numbered
+                    state to a lower numbered state."
+            ::= { bgpTraps 2 }
+
+        -- conformance information
+
+        bgpMIBConformance OBJECT IDENTIFIER ::= { bgp 8 }
+        bgpMIBCompliances OBJECT IDENTIFIER ::= { bgpMIBConformance 1 }
+        bgpMIBGroups      OBJECT IDENTIFIER ::= { bgpMIBConformance 2 }
+
+        -- compliance statements
+
+        bgpMIBCompliance MODULE-COMPLIANCE
+            STATUS  current
+            DESCRIPTION
+                    "The compliance statement for entities which
+                     implement the BGP4 mib."
+            MODULE  -- this module
+                MANDATORY-GROUPS { bgp4MIBGlobalsGroup,
+                                   bgp4MIBPeerGroup,
+                                   bgp4MIBPathAttrGroup,
+                                   bgp4MIBNotificationGroup }
+            ::= { bgpMIBCompliances 1 }
+
+        -- units of conformance
+
+        bgp4MIBGlobalsGroup OBJECT-GROUP
+            OBJECTS { bgpVersion,
+                      bgpLocalAs,
+                      bgpIdentifier }
+            STATUS  current
+            DESCRIPTION
+                    "A collection of objects providing information
+                     on global BGP state."
+            ::= { bgpMIBGroups 1 }
+
+        bgp4MIBPeerGroup OBJECT-GROUP
+            OBJECTS { bgpPeerIdentifier,
+                      bgpPeerState,
+                      bgpPeerAdminStatus,
+                      bgpPeerNegotiatedVersion,
+                      bgpPeerLocalAddr,
+                      bgpPeerLocalPort,
+                      bgpPeerRemoteAddr,
+                      bgpPeerRemotePort,
+                      bgpPeerRemoteAs,
+                      bgpPeerInUpdates,
+                      bgpPeerOutUpdates,
+                      bgpPeerInTotalMessages,
+                      bgpPeerOutTotalMessages,
+                      bgpPeerLastError,
+                      bgpPeerFsmEstablishedTransitions,
+                      bgpPeerFsmEstablishedTime,
+                      bgpPeerConnectRetryInterval,
+                      bgpPeerHoldTime,
+                      bgpPeerKeepAlive,
+                      bgpPeerHoldTimeConfigured,
+                      bgpPeerKeepAliveConfigured,
+                      bgpPeerMinASOriginationInterval,
+                      bgpPeerMinRouteAdvertisementInterval,
+                      bgpPeerInUpdateElapsedTime }
+            STATUS  current
+            DESCRIPTION
+                    "A collection of objects for managing
+                     BGP peers."
+            ::= { bgpMIBGroups 2 }
+
+        bgp4MIBRcvdPathAttrGroup OBJECT-GROUP
+            OBJECTS { bgpPathAttrPeer,
+                      bgpPathAttrDestNetwork,
+                      bgpPathAttrOrigin,
+                      bgpPathAttrASPath,
+                      bgpPathAttrNextHop,
+                      bgpPathAttrInterASMetric }
+            STATUS  obsolete
+            DESCRIPTION
+                    "A collection of objects for managing BGP
+                     path entries.
+
+                     This conformance group is obsolete,
+                     replaced by bgp4MIBPathAttrGroup."
+            ::= { bgpMIBGroups 3 }
+
+        bgp4MIBPathAttrGroup OBJECT-GROUP
+            OBJECTS { bgp4PathAttrPeer,
+                      bgp4PathAttrIpAddrPrefixLen,
+                      bgp4PathAttrIpAddrPrefix,
+                      bgp4PathAttrOrigin,
+                      bgp4PathAttrASPathSegment,
+                      bgp4PathAttrNextHop,
+                      bgp4PathAttrMultiExitDisc,
+                      bgp4PathAttrLocalPref,
+                      bgp4PathAttrAtomicAggregate,
+                      bgp4PathAttrAggregatorAS,
+                      bgp4PathAttrAggregatorAddr,
+                      bgp4PathAttrCalcLocalPref,
+                      bgp4PathAttrBest,
+                      bgp4PathAttrUnknown }
+            STATUS  current
+            DESCRIPTION
+                    "A collection of objects for managing
+                     BGP path entries."
+            ::= { bgpMIBGroups 4 }
+
+        bgp4MIBNotificationGroup NOTIFICATION-GROUP
+            NOTIFICATIONS { bgpEstablished,
+                            bgpBackwardTransition }
+            STATUS  current
+            DESCRIPTION
+                    "A collection of notifications for signaling
+                    changes in BGP peer relationships."
+            ::= { bgpMIBGroups 5 }
+
+    END
--- /dev/null
+++ b/mibs/GNOME-SMI.txt
@@ -0,0 +1,88 @@
+GNOME-SMI DEFINITIONS ::= BEGIN
+
+IMPORTS
+	MODULE-IDENTITY,
+	OBJECT-IDENTITY,
+	enterprises
+		FROM SNMPv2-SMI;
+
+gnome MODULE-IDENTITY
+	LAST-UPDATED "200709070000Z"
+	ORGANIZATION "GNOME project"
+	CONTACT-INFO
+		"GNU Network Object Model Environment project
+		
+		see http://www.gnome.org for contact persons of a particular
+		area or subproject of GNOME.
+
+		Administrative contact for MIB module:
+
+		Jochen Friedrich
+		Ramsaystr. 9
+		63450 Hanau
+		Germany 
+
+		email: jochen@scram.de"
+	DESCRIPTION
+		"The Structure of GNOME."
+
+	-- revision history
+
+	REVISION "200709070000Z"  -- Sep 07, 2007
+	DESCRIPTION
+		"Fixed wrong enterprise number (how comes this
+		typo was unnoticed for so long?)."
+
+	REVISION "200505070000Z"  -- May 07, 2005
+	DESCRIPTION
+		"Added gnomeLDAP subtree for LDAP definitions."
+
+	REVISION "200312070000Z"  -- December 07, 2003
+	DESCRIPTION
+		"Added gnomeSysadmin subtree for GNOME project system administration.
+		Updated contact info."
+
+	REVISION "9809010000Z"  -- September 01, 1998
+	DESCRIPTION
+		"Initial version."
+
+	::= { enterprises 3319 }	-- assigned by IANA
+
+gnomeProducts OBJECT-IDENTITY
+	STATUS	current
+	DESCRIPTION
+		"gnomeProducts is the root OBJECT IDENTIFIER from
+		which sysObjectID values are assigned."
+	::= { gnome 1 }
+
+gnomeMgmt OBJECT-IDENTITY
+	STATUS  current
+	DESCRIPTION
+		"gnomeMgmt defines the subtree for production GNOME related
+		MIB registrations."
+	::= { gnome 2 }
+
+gnomeTest OBJECT-IDENTITY
+	STATUS  current
+	DESCRIPTION
+		"gnomeTest defines the subtree for testing GNOME related
+		MIB registrations."
+	::= { gnome 3 }
+
+gnomeSysadmin OBJECT-IDENTITY
+	STATUS  current
+	DESCRIPTION
+		"gnomeSysadmin defines the subtree for GNOME related Sysadmin
+		MIB registrations."
+	::= { gnome 4 }
+
+gnomeLDAP OBJECT-IDENTITY
+	STATUS  current
+	DESCRIPTION
+		"gnomeLDAP defines the subtree for GNOME related LDAP
+		registrations."
+	::= { gnome 5 }
+
+-- more to come if necessary.
+
+END
--- /dev/null
+++ b/mibs/OSPF-MIB.txt
@@ -0,0 +1,2723 @@
+OSPF-MIB DEFINITIONS ::= BEGIN
+
+    IMPORTS
+            MODULE-IDENTITY, OBJECT-TYPE, Counter32, Gauge32,
+            Integer32, IpAddress
+                FROM SNMPv2-SMI
+            TEXTUAL-CONVENTION, TruthValue, RowStatus
+                FROM SNMPv2-TC
+            MODULE-COMPLIANCE, OBJECT-GROUP          FROM SNMPv2-CONF
+            mib-2                                    FROM RFC1213-MIB;
+
+--  This MIB module uses the extended OBJECT-TYPE macro as
+--  defined in [9].
+
+ospf MODULE-IDENTITY
+        LAST-UPDATED "9501201225Z" -- Fri Jan 20 12:25:50 PST 1995
+        ORGANIZATION "IETF OSPF Working Group"
+        CONTACT-INFO
+       "       Fred Baker
+       Postal: Cisco Systems
+               519 Lado Drive
+               Santa Barbara, California 93111
+       Tel:    +1 805 681 0115
+       E-Mail: fred@cisco.com
+
+               Rob Coltun
+       Postal: RainbowBridge Communications
+       Tel:    (301) 340-9416
+       E-Mail: rcoltun@rainbow-bridge.com"
+    DESCRIPTION
+       "The MIB module to describe the OSPF Version 2
+       Protocol"
+    ::= { mib-2 14 }
+
+--  The Area ID, in OSPF, has the same format as an IP Address,
+--  but has the function of defining a summarization point for
+--  Link State Advertisements
+
+AreaID ::= TEXTUAL-CONVENTION
+    STATUS      current
+    DESCRIPTION
+       "An OSPF Area Identifier."
+    SYNTAX      IpAddress
+
+
+--  The Router ID, in OSPF, has the same format as an IP Address,
+--  but identifies the router independent of its IP Address.
+
+RouterID ::= TEXTUAL-CONVENTION
+    STATUS      current
+    DESCRIPTION
+       "A OSPF Router Identifier."
+    SYNTAX      IpAddress
+
+
+--  The OSPF Metric is defined as an unsigned value in the range
+
+Metric ::= TEXTUAL-CONVENTION
+    STATUS      current
+    DESCRIPTION
+       "The OSPF Internal Metric."
+    SYNTAX      Integer32 (0..'FFFF'h)
+
+BigMetric ::= TEXTUAL-CONVENTION
+    STATUS      current
+    DESCRIPTION
+       "The OSPF External Metric."
+    SYNTAX      Integer32 (0..'FFFFFF'h)
+
+--  Status Values
+
+Status ::= TEXTUAL-CONVENTION
+    STATUS      current
+    DESCRIPTION
+       "The status of an interface: 'enabled' indicates that
+       it is willing to communicate with other OSPF Routers,
+       while 'disabled' indicates that it is not."
+    SYNTAX      INTEGER { enabled (1), disabled (2) }
+
+--  Time Durations measured in seconds
+
+PositiveInteger ::= TEXTUAL-CONVENTION
+    STATUS      current
+    DESCRIPTION
+       "A positive integer. Values in excess are precluded as
+       unnecessary and prone to interoperability issues."
+    SYNTAX      Integer32 (0..'7FFFFFFF'h)
+
+HelloRange ::= TEXTUAL-CONVENTION
+    STATUS      current
+    DESCRIPTION
+       "The range of intervals on which hello messages are
+       exchanged."
+    SYNTAX      Integer32 (1..'FFFF'h)
+
+UpToMaxAge ::= TEXTUAL-CONVENTION
+    STATUS      current
+    DESCRIPTION
+       "The values that one might find or configure for
+       variables bounded by the maximum age of an LSA."
+    SYNTAX      Integer32 (0..3600)
+
+
+--  The range of ifIndex
+
+InterfaceIndex ::= TEXTUAL-CONVENTION
+    STATUS      current
+    DESCRIPTION
+       "The range of ifIndex."
+    SYNTAX      Integer32
+
+
+--  Potential Priorities for the Designated Router Election
+
+DesignatedRouterPriority ::= TEXTUAL-CONVENTION
+    STATUS      current
+    DESCRIPTION
+       "The values defined for the priority of a system for
+       becoming the designated router."
+    SYNTAX      Integer32 (0..'FF'h)
+
+TOSType ::= TEXTUAL-CONVENTION
+    STATUS      current
+    DESCRIPTION
+       "Type of Service is defined as a mapping to the IP Type of
+       Service Flags as defined in the IP Forwarding Table MIB
+
+       +-----+-----+-----+-----+-----+-----+-----+-----+
+       |                 |                       |     |
+       |   PRECEDENCE    |    TYPE OF SERVICE    |  0  |
+       |                 |                       |     |
+       +-----+-----+-----+-----+-----+-----+-----+-----+
+
+                IP TOS                IP TOS
+           Field     Policy      Field     Policy
+
+           Contents    Code      Contents    Code
+           0 0 0 0  ==>   0      0 0 0 1  ==>   2
+           0 0 1 0  ==>   4      0 0 1 1  ==>   6
+           0 1 0 0  ==>   8      0 1 0 1  ==>  10
+           0 1 1 0  ==>  12      0 1 1 1  ==>  14
+           1 0 0 0  ==>  16      1 0 0 1  ==>  18
+           1 0 1 0  ==>  20      1 0 1 1  ==>  22
+           1 1 0 0  ==>  24      1 1 0 1  ==>  26
+           1 1 1 0  ==>  28      1 1 1 1  ==>  30
+
+       The remaining values are left for future definition."
+    SYNTAX      Integer32 (0..30)
+
+
+--  OSPF General Variables
+
+--      These parameters apply globally to the Router's
+--      OSPF Process.
+
+ospfGeneralGroup OBJECT IDENTIFIER ::= { ospf 1 }
+
+
+    ospfRouterId OBJECT-TYPE
+        SYNTAX   RouterID
+        MAX-ACCESS   read-write
+        STATUS   current
+        DESCRIPTION
+           "A  32-bit  integer  uniquely  identifying  the
+           router in the Autonomous System.
+
+           By  convention,  to  ensure  uniqueness,   this
+           should  default  to  the  value  of  one of the
+           router's IP interface addresses."
+       REFERENCE
+          "OSPF Version 2, C.1 Global parameters"
+      ::= { ospfGeneralGroup 1 }
+
+
+    ospfAdminStat OBJECT-TYPE
+        SYNTAX   Status
+        MAX-ACCESS   read-write
+        STATUS   current
+        DESCRIPTION
+           "The  administrative  status  of  OSPF  in  the
+           router.   The  value 'enabled' denotes that the
+           OSPF Process is active on at least  one  inter-
+           face;  'disabled'  disables  it  on  all inter-
+           faces."
+       ::= { ospfGeneralGroup 2 }
+
+    ospfVersionNumber OBJECT-TYPE
+        SYNTAX   INTEGER    { version2 (2) }
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The current version number of the OSPF  proto-
+           col is 2."
+       REFERENCE
+          "OSPF Version 2, Title"
+      ::= { ospfGeneralGroup 3 }
+
+
+    ospfAreaBdrRtrStatus OBJECT-TYPE
+        SYNTAX   TruthValue
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "A flag to note whether this router is an  area
+           border router."
+       REFERENCE
+          "OSPF Version 2, Section 3 Splitting the AS into
+          Areas"
+      ::= { ospfGeneralGroup 4 }
+
+
+    ospfASBdrRtrStatus OBJECT-TYPE
+        SYNTAX   TruthValue
+        MAX-ACCESS   read-write
+        STATUS   current
+        DESCRIPTION
+           "A flag to note whether this router is  config-
+           ured as an Autonomous System border router."
+       REFERENCE
+          "OSPF Version 2, Section 3.3  Classification  of
+          routers"
+      ::= { ospfGeneralGroup 5 }
+
+    ospfExternLsaCount OBJECT-TYPE
+        SYNTAX   Gauge32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The number of external (LS type 5)  link-state
+           advertisements in the link-state database."
+       REFERENCE
+          "OSPF Version 2, Appendix A.4.5 AS external link
+          advertisements"
+      ::= { ospfGeneralGroup 6 }
+
+
+    ospfExternLsaCksumSum OBJECT-TYPE
+        SYNTAX   Integer32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The 32-bit unsigned sum of the LS checksums of
+           the  external  link-state  advertisements  con-
+           tained in the link-state  database.   This  sum
+           can  be  used  to determine if there has been a
+           change in a router's link state  database,  and
+           to  compare  the  link-state  database  of  two
+           routers."
+       ::= { ospfGeneralGroup 7 }
+
+
+    ospfTOSSupport OBJECT-TYPE
+        SYNTAX   TruthValue
+        MAX-ACCESS   read-write
+        STATUS   current
+        DESCRIPTION
+           "The router's support for type-of-service rout-
+           ing."
+       REFERENCE
+          "OSPF Version 2,  Appendix  F.1.2  Optional  TOS
+          support"
+      ::= { ospfGeneralGroup 8 }
+
+    ospfOriginateNewLsas OBJECT-TYPE
+        SYNTAX   Counter32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The number of  new  link-state  advertisements
+           that  have been originated.  This number is in-
+           cremented each time the router originates a new
+           LSA."
+       ::= { ospfGeneralGroup 9 }
+
+
+    ospfRxNewLsas OBJECT-TYPE
+        SYNTAX   Counter32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The number of  link-state  advertisements  re-
+           ceived  determined  to  be  new instantiations.
+           This number does not include  newer  instantia-
+           tions  of self-originated link-state advertise-
+           ments."
+       ::= { ospfGeneralGroup 10 }
+
+    ospfExtLsdbLimit OBJECT-TYPE
+        SYNTAX   Integer32 (-1..'7FFFFFFF'h)
+        MAX-ACCESS   read-write
+        STATUS   current
+        DESCRIPTION
+           "The  maximum   number   of   non-default   AS-
+           external-LSAs entries that can be stored in the
+           link-state database.  If the value is -1,  then
+           there is no limit.
+
+           When the number of non-default AS-external-LSAs
+           in   a  router's  link-state  database  reaches
+           ospfExtLsdbLimit, the router  enters  Overflow-
+           State.   The   router  never  holds  more  than
+           ospfExtLsdbLimit  non-default  AS-external-LSAs
+           in  its  database. OspfExtLsdbLimit MUST be set
+           identically in all routers attached to the OSPF
+           backbone  and/or  any regular OSPF area. (i.e.,
+           OSPF stub areas and NSSAs are excluded)."
+       DEFVAL { -1 }
+       ::= { ospfGeneralGroup 11 }
+
+    ospfMulticastExtensions OBJECT-TYPE
+        SYNTAX   Integer32
+        MAX-ACCESS   read-write
+        STATUS   current
+        DESCRIPTION
+           "A Bit Mask indicating whether  the  router  is
+           forwarding  IP  multicast  (Class  D) datagrams
+           based on the algorithms defined in  the  Multi-
+           cast Extensions to OSPF.
+
+           Bit 0, if set, indicates that  the  router  can
+           forward  IP multicast datagrams in the router's
+           directly attached areas (called intra-area mul-
+           ticast routing).
+
+           Bit 1, if set, indicates that  the  router  can
+           forward  IP  multicast  datagrams  between OSPF
+           areas (called inter-area multicast routing).
+
+           Bit 2, if set, indicates that  the  router  can
+           forward  IP  multicast  datagrams between Auto-
+           nomous Systems (called inter-AS multicast rout-
+           ing).
+
+           Only certain combinations of bit  settings  are
+           allowed,  namely: 0 (no multicast forwarding is
+           enabled), 1 (intra-area multicasting  only),  3
+           (intra-area  and  inter-area  multicasting),  5
+           (intra-area and inter-AS  multicasting)  and  7
+           (multicasting  everywhere). By default, no mul-
+           ticast forwarding is enabled."
+       DEFVAL { 0 }
+       ::= { ospfGeneralGroup 12 }
+
+    ospfExitOverflowInterval OBJECT-TYPE
+        SYNTAX   PositiveInteger
+        MAX-ACCESS   read-write
+        STATUS   current
+        DESCRIPTION
+           "The number of  seconds  that,  after  entering
+           OverflowState,  a  router will attempt to leave
+           OverflowState. This allows the router to  again
+           originate  non-default  AS-external-LSAs.  When
+           set to 0, the router will not  leave  Overflow-
+           State until restarted."
+       DEFVAL { 0 }
+       ::= { ospfGeneralGroup 13 }
+
+
+    ospfDemandExtensions OBJECT-TYPE
+        SYNTAX   TruthValue
+        MAX-ACCESS   read-write
+        STATUS   current
+        DESCRIPTION
+           "The router's support for demand routing."
+       REFERENCE
+          "OSPF Version 2, Appendix on Demand Routing"
+      ::= { ospfGeneralGroup 14 }
+
+
+--      The OSPF Area Data Structure contains information
+--      regarding the various areas. The interfaces and
+--      virtual links are configured as part of these areas.
+--      Area 0.0.0.0, by definition, is the Backbone Area
+
+
+    ospfAreaTable OBJECT-TYPE
+        SYNTAX   SEQUENCE OF OspfAreaEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "Information describing the configured  parame-
+           ters  and cumulative statistics of the router's
+           attached areas."
+       REFERENCE
+          "OSPF Version 2, Section 6  The Area Data Struc-
+          ture"
+      ::= { ospf 2 }
+
+
+    ospfAreaEntry OBJECT-TYPE
+        SYNTAX   OspfAreaEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "Information describing the configured  parame-
+           ters  and  cumulative  statistics of one of the
+           router's attached areas."
+       INDEX { ospfAreaId }
+       ::= { ospfAreaTable 1 }
+
+OspfAreaEntry ::=
+    SEQUENCE {
+        ospfAreaId
+            AreaID,
+        ospfAuthType
+            Integer32,
+        ospfImportAsExtern
+            INTEGER,
+        ospfSpfRuns
+            Counter32,
+        ospfAreaBdrRtrCount
+            Gauge32,
+        ospfAsBdrRtrCount
+            Gauge32,
+        ospfAreaLsaCount
+            Gauge32,
+        ospfAreaLsaCksumSum
+            Integer32,
+        ospfAreaSummary
+            INTEGER,
+        ospfAreaStatus
+            RowStatus
+              }
+
+    ospfAreaId OBJECT-TYPE
+        SYNTAX   AreaID
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "A 32-bit integer uniquely identifying an area.
+           Area ID 0.0.0.0 is used for the OSPF backbone."
+       REFERENCE
+          "OSPF Version 2, Appendix C.2 Area parameters"
+      ::= { ospfAreaEntry 1 }
+
+
+    ospfAuthType OBJECT-TYPE
+        SYNTAX   Integer32
+                    -- none (0),
+                    -- simplePassword (1)
+                    -- md5 (2)
+                    -- reserved for specification by IANA (> 2)
+        MAX-ACCESS   read-create
+        STATUS   obsolete
+        DESCRIPTION
+           "The authentication type specified for an area.
+           Additional authentication types may be assigned
+           locally on a per Area basis."
+       REFERENCE
+          "OSPF Version 2, Appendix E Authentication"
+      DEFVAL { 0 }        -- no authentication, by default
+      ::= { ospfAreaEntry 2 }
+
+    ospfImportAsExtern OBJECT-TYPE
+        SYNTAX   INTEGER    {
+                    importExternal (1),
+                    importNoExternal (2),
+                    importNssa (3)
+                  }
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The area's support for importing  AS  external
+           link- state advertisements."
+       REFERENCE
+          "OSPF Version 2, Appendix C.2 Area parameters"
+      DEFVAL { importExternal }
+      ::= { ospfAreaEntry 3 }
+
+
+    ospfSpfRuns OBJECT-TYPE
+        SYNTAX   Counter32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The number of times that the intra-area  route
+           table  has  been  calculated  using this area's
+           link-state database.  This  is  typically  done
+           using Dijkstra's algorithm."
+       ::= { ospfAreaEntry 4 }
+
+
+    ospfAreaBdrRtrCount OBJECT-TYPE
+        SYNTAX   Gauge32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The total number of area border routers reach-
+           able within this area.  This is initially zero,
+           and is calculated in each SPF Pass."
+       ::= { ospfAreaEntry 5 }
+
+    ospfAsBdrRtrCount OBJECT-TYPE
+        SYNTAX   Gauge32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The total number of Autonomous  System  border
+           routers  reachable  within  this area.  This is
+           initially zero, and is calculated in  each  SPF
+           Pass."
+       ::= { ospfAreaEntry 6 }
+
+
+    ospfAreaLsaCount OBJECT-TYPE
+        SYNTAX   Gauge32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The total number of link-state  advertisements
+           in  this  area's link-state database, excluding
+           AS External LSA's."
+       ::= { ospfAreaEntry 7 }
+
+
+    ospfAreaLsaCksumSum OBJECT-TYPE
+        SYNTAX   Integer32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The 32-bit unsigned sum of the link-state  ad-
+           vertisements'  LS  checksums  contained in this
+           area's link-state database.  This sum  excludes
+           external (LS type 5) link-state advertisements.
+           The sum can be used to determine if  there  has
+           been  a  change  in a router's link state data-
+           base, and to compare the link-state database of
+           two routers."
+       DEFVAL   { 0 }
+       ::= { ospfAreaEntry 8 }
+
+    ospfAreaSummary OBJECT-TYPE
+        SYNTAX   INTEGER    {
+                    noAreaSummary (1),
+                    sendAreaSummary (2)
+                  }
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The variable ospfAreaSummary controls the  im-
+           port  of  summary LSAs into stub areas.  It has
+           no effect on other areas.
+
+           If it is noAreaSummary, the router will neither
+           originate  nor  propagate summary LSAs into the
+           stub area.  It will rely entirely  on  its  de-
+           fault route.
+
+           If it is sendAreaSummary, the router will  both
+           summarize and propagate summary LSAs."
+       DEFVAL   { noAreaSummary }
+       ::= { ospfAreaEntry 9 }
+
+
+    ospfAreaStatus OBJECT-TYPE
+        SYNTAX   RowStatus
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "This variable displays the status of  the  en-
+           try.  Setting it to 'invalid' has the effect of
+           rendering it inoperative.  The internal  effect
+           (row removal) is implementation dependent."
+       ::= { ospfAreaEntry 10 }
+
+
+--  OSPF Area Default Metric Table
+
+--      The OSPF Area Default Metric Table describes the metrics
+--      that a default Area Border Router will advertise into a
+--      Stub area.
+
+
+    ospfStubAreaTable OBJECT-TYPE
+        SYNTAX   SEQUENCE OF OspfStubAreaEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "The set of metrics that will be advertised  by
+           a default Area Border Router into a stub area."
+       REFERENCE
+          "OSPF Version 2, Appendix C.2, Area Parameters"
+      ::= { ospf 3 }
+
+
+    ospfStubAreaEntry OBJECT-TYPE
+        SYNTAX   OspfStubAreaEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "The metric for a given Type  of  Service  that
+           will  be  advertised  by  a default Area Border
+           Router into a stub area."
+       REFERENCE
+          "OSPF Version 2, Appendix C.2, Area Parameters"
+      INDEX { ospfStubAreaId, ospfStubTOS }
+      ::= { ospfStubAreaTable 1 }
+
+OspfStubAreaEntry ::=
+    SEQUENCE {
+        ospfStubAreaId
+            AreaID,
+        ospfStubTOS
+            TOSType,
+        ospfStubMetric
+            BigMetric,
+        ospfStubStatus
+            RowStatus,
+        ospfStubMetricType
+            INTEGER
+              }
+
+    ospfStubAreaId OBJECT-TYPE
+        SYNTAX   AreaID
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The 32 bit identifier for the Stub  Area.   On
+           creation,  this  can  be  derived  from the in-
+           stance."
+       ::= { ospfStubAreaEntry 1 }
+
+
+    ospfStubTOS OBJECT-TYPE
+        SYNTAX   TOSType
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The  Type  of  Service  associated  with   the
+           metric.   On creation, this can be derived from
+           the instance."
+       ::= { ospfStubAreaEntry 2 }
+
+
+    ospfStubMetric OBJECT-TYPE
+        SYNTAX   BigMetric
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The metric value applied at the indicated type
+           of  service.  By default, this equals the least
+           metric at the type of service among the  inter-
+           faces to other areas."
+       ::= { ospfStubAreaEntry 3 }
+
+
+    ospfStubStatus OBJECT-TYPE
+        SYNTAX   RowStatus
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "This variable displays the status of  the  en-
+           try.  Setting it to 'invalid' has the effect of
+           rendering it inoperative.  The internal  effect
+           (row removal) is implementation dependent."
+       ::= { ospfStubAreaEntry 4 }
+
+    ospfStubMetricType OBJECT-TYPE
+        SYNTAX   INTEGER    {
+                    ospfMetric (1),                -- OSPF Metric
+                    comparableCost (2),        -- external type 1
+                    nonComparable  (3)        -- external type 2
+                  }
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "This variable displays the type of metric  ad-
+           vertised as a default route."
+       DEFVAL   { ospfMetric }
+       ::= { ospfStubAreaEntry 5 }
+
+--  OSPF Link State Database
+
+--      The Link State Database contains the Link State
+--      Advertisements from throughout the areas that the
+--      device is attached to.
+
+
+    ospfLsdbTable OBJECT-TYPE
+        SYNTAX   SEQUENCE OF OspfLsdbEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "The OSPF Process's Link State Database."
+       REFERENCE
+          "OSPF Version 2, Section 12  Link  State  Adver-
+          tisements"
+      ::= { ospf 4 }
+
+
+    ospfLsdbEntry OBJECT-TYPE
+        SYNTAX   OspfLsdbEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "A single Link State Advertisement."
+       INDEX { ospfLsdbAreaId, ospfLsdbType,
+               ospfLsdbLsid, ospfLsdbRouterId }
+       ::= { ospfLsdbTable 1 }
+
+OspfLsdbEntry ::=
+    SEQUENCE {
+        ospfLsdbAreaId
+            AreaID,
+        ospfLsdbType
+            INTEGER,
+        ospfLsdbLsid
+            IpAddress,
+        ospfLsdbRouterId
+            RouterID,
+        ospfLsdbSequence
+            Integer32,
+        ospfLsdbAge
+            Integer32,
+        ospfLsdbChecksum
+            Integer32,
+        ospfLsdbAdvertisement
+            OCTET STRING
+              }
+    ospfLsdbAreaId OBJECT-TYPE
+        SYNTAX   AreaID
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The 32 bit identifier of the Area  from  which
+           the LSA was received."
+       REFERENCE
+          "OSPF Version 2, Appendix C.2 Area parameters"
+      ::= { ospfLsdbEntry 1 }
+
+-- External Link State Advertisements are permitted
+-- for backward compatibility, but should be displayed in
+-- the ospfExtLsdbTable rather than here.
+
+    ospfLsdbType OBJECT-TYPE
+        SYNTAX   INTEGER    {
+                    routerLink (1),
+                    networkLink (2),
+                    summaryLink (3),
+                    asSummaryLink (4),
+                    asExternalLink (5), -- but see ospfExtLsdbTable
+                    multicastLink (6),
+                    nssaExternalLink (7)
+                  }
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The type  of  the  link  state  advertisement.
+           Each  link state type has a separate advertise-
+           ment format."
+       REFERENCE
+          "OSPF Version 2, Appendix A.4.1 The  Link  State
+          Advertisement header"
+      ::= { ospfLsdbEntry 2 }
+
+    ospfLsdbLsid OBJECT-TYPE
+        SYNTAX   IpAddress
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The Link State ID is an LS Type Specific field
+           containing either a Router ID or an IP Address;
+           it identifies the piece of the  routing  domain
+           that is being described by the advertisement."
+       REFERENCE
+          "OSPF Version 2, Section 12.1.4 Link State ID"
+      ::= { ospfLsdbEntry 3 }
+    ospfLsdbRouterId OBJECT-TYPE
+        SYNTAX   RouterID
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The 32 bit number that uniquely identifies the
+           originating router in the Autonomous System."
+       REFERENCE
+          "OSPF Version 2, Appendix C.1 Global parameters"
+      ::= { ospfLsdbEntry 4 }
+
+--  Note that the OSPF Sequence Number is a 32 bit signed
+--  integer.  It starts with the value '80000001'h,
+--  or -'7FFFFFFF'h, and increments until '7FFFFFFF'h
+--  Thus, a typical sequence number will be very negative.
+
+    ospfLsdbSequence OBJECT-TYPE
+        SYNTAX   Integer32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The sequence number field is a  signed  32-bit
+           integer.   It  is used to detect old and dupli-
+           cate link state advertisements.  The  space  of
+           sequence  numbers  is  linearly  ordered.   The
+           larger the sequence number the more recent  the
+           advertisement."
+       REFERENCE
+          "OSPF Version  2,  Section  12.1.6  LS  sequence
+          number"
+      ::= { ospfLsdbEntry 5 }
+
+
+    ospfLsdbAge OBJECT-TYPE
+        SYNTAX   Integer32    -- Should be 0..MaxAge
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "This field is the age of the link state adver-
+           tisement in seconds."
+       REFERENCE
+          "OSPF Version 2, Section 12.1.1 LS age"
+      ::= { ospfLsdbEntry 6 }
+
+    ospfLsdbChecksum OBJECT-TYPE
+        SYNTAX   Integer32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "This field is the  checksum  of  the  complete
+           contents  of  the  advertisement, excepting the
+           age field.  The age field is excepted  so  that
+           an   advertisement's  age  can  be  incremented
+           without updating the  checksum.   The  checksum
+           used  is  the same that is used for ISO connec-
+           tionless datagrams; it is commonly referred  to
+           as the Fletcher checksum."
+       REFERENCE
+          "OSPF Version 2, Section 12.1.7 LS checksum"
+      ::= { ospfLsdbEntry 7 }
+
+
+    ospfLsdbAdvertisement OBJECT-TYPE
+        SYNTAX   OCTET STRING (SIZE (1..65535))
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The entire Link State Advertisement, including
+           its header."
+       REFERENCE
+          "OSPF Version 2, Section 12  Link  State  Adver-
+          tisements"
+      ::= { ospfLsdbEntry 8 }
+
+
+--  Address Range Table
+
+--      The Address Range Table acts as an adjunct to the Area
+--      Table; It describes those Address Range Summaries that
+--      are configured to be propagated from an Area to reduce
+--      the amount of information about it which is known beyond
+--      its borders.
+
+    ospfAreaRangeTable OBJECT-TYPE
+        SYNTAX   SEQUENCE OF OspfAreaRangeEntry
+        MAX-ACCESS   not-accessible
+        STATUS   obsolete
+        DESCRIPTION
+           "A range if IP addresses  specified  by  an  IP
+           address/IP  network  mask  pair.   For example,
+           class B address range of X.X.X.X with a network
+           mask  of  255.255.0.0 includes all IP addresses
+           from X.X.0.0 to X.X.255.255"
+       REFERENCE
+          "OSPF Version 2, Appendix C.2  Area parameters"
+      ::= { ospf 5 }
+    ospfAreaRangeEntry OBJECT-TYPE
+        SYNTAX   OspfAreaRangeEntry
+        MAX-ACCESS   not-accessible
+        STATUS   obsolete
+        DESCRIPTION
+           "A range if IP addresses  specified  by  an  IP
+           address/IP  network  mask  pair.   For example,
+           class B address range of X.X.X.X with a network
+           mask  of  255.255.0.0 includes all IP addresses
+           from X.X.0.0 to X.X.255.255"
+       REFERENCE
+          "OSPF Version 2, Appendix C.2  Area parameters"
+      INDEX { ospfAreaRangeAreaId, ospfAreaRangeNet }
+      ::= { ospfAreaRangeTable 1 }
+
+OspfAreaRangeEntry ::=
+    SEQUENCE {
+        ospfAreaRangeAreaId
+            AreaID,
+        ospfAreaRangeNet
+            IpAddress,
+        ospfAreaRangeMask
+            IpAddress,
+        ospfAreaRangeStatus
+            RowStatus,
+        ospfAreaRangeEffect
+            INTEGER
+              }
+
+    ospfAreaRangeAreaId OBJECT-TYPE
+        SYNTAX   AreaID
+        MAX-ACCESS   read-only
+        STATUS   obsolete
+        DESCRIPTION
+           "The Area the Address  Range  is  to  be  found
+           within."
+       REFERENCE
+          "OSPF Version 2, Appendix C.2 Area parameters"
+      ::= { ospfAreaRangeEntry 1 }
+
+
+    ospfAreaRangeNet OBJECT-TYPE
+        SYNTAX   IpAddress
+        MAX-ACCESS   read-only
+        STATUS   obsolete
+        DESCRIPTION
+           "The IP Address of the Net or Subnet  indicated
+           by the range."
+       REFERENCE
+          "OSPF Version 2, Appendix C.2 Area parameters"
+      ::= { ospfAreaRangeEntry 2 }
+
+
+    ospfAreaRangeMask OBJECT-TYPE
+        SYNTAX   IpAddress
+        MAX-ACCESS   read-create
+        STATUS   obsolete
+        DESCRIPTION
+           "The Subnet Mask that pertains to  the  Net  or
+           Subnet."
+       REFERENCE
+          "OSPF Version 2, Appendix C.2 Area parameters"
+      ::= { ospfAreaRangeEntry 3 }
+
+    ospfAreaRangeStatus OBJECT-TYPE
+        SYNTAX   RowStatus
+        MAX-ACCESS   read-create
+        STATUS   obsolete
+        DESCRIPTION
+           "This variable displays the status of  the  en-
+           try.  Setting it to 'invalid' has the effect of
+           rendering it inoperative.  The internal  effect
+           (row removal) is implementation dependent."
+       ::= { ospfAreaRangeEntry 4 }
+
+
+    ospfAreaRangeEffect OBJECT-TYPE
+        SYNTAX   INTEGER    {
+                    advertiseMatching (1),
+                    doNotAdvertiseMatching (2)
+                  }
+        MAX-ACCESS   read-create
+        STATUS   obsolete
+        DESCRIPTION
+           "Subnets subsumed by ranges either trigger  the
+           advertisement  of the indicated summary (adver-
+           tiseMatching), or result in  the  subnet's  not
+           being advertised at all outside the area."
+       DEFVAL   { advertiseMatching }
+       ::= { ospfAreaRangeEntry 5 }
+
+
+
+--  OSPF Host Table
+
+--      The Host/Metric Table indicates what hosts are directly
+--      attached to the Router, and what metrics and types of
+--      service should be advertised for them.
+
+    ospfHostTable OBJECT-TYPE
+        SYNTAX   SEQUENCE OF OspfHostEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "The list of Hosts, and their metrics, that the
+           router will advertise as host routes."
+       REFERENCE
+          "OSPF Version 2, Appendix C.6  Host route param-
+          eters"
+      ::= { ospf 6 }
+
+
+    ospfHostEntry OBJECT-TYPE
+        SYNTAX   OspfHostEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "A metric to be advertised, for a given type of
+           service, when a given host is reachable."
+       INDEX { ospfHostIpAddress, ospfHostTOS }
+       ::= { ospfHostTable 1 }
+
+OspfHostEntry ::=
+    SEQUENCE {
+        ospfHostIpAddress
+            IpAddress,
+        ospfHostTOS
+            TOSType,
+        ospfHostMetric
+            Metric,
+        ospfHostStatus
+            RowStatus,
+        ospfHostAreaID
+            AreaID
+              }
+
+    ospfHostIpAddress OBJECT-TYPE
+        SYNTAX   IpAddress
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The IP Address of the Host."
+       REFERENCE
+          "OSPF Version 2, Appendix C.6 Host route parame-
+          ters"
+      ::= { ospfHostEntry 1 }
+
+
+    ospfHostTOS OBJECT-TYPE
+        SYNTAX   TOSType
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The Type of Service of the route being config-
+           ured."
+       REFERENCE
+          "OSPF Version 2, Appendix C.6 Host route parame-
+          ters"
+      ::= { ospfHostEntry 2 }
+
+
+    ospfHostMetric OBJECT-TYPE
+        SYNTAX   Metric
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The Metric to be advertised."
+       REFERENCE
+          "OSPF Version 2, Appendix C.6 Host route parame-
+          ters"
+      ::= { ospfHostEntry 3 }
+
+    ospfHostStatus OBJECT-TYPE
+        SYNTAX   RowStatus
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "This variable displays the status of  the  en-
+           try.  Setting it to 'invalid' has the effect of
+           rendering it inoperative.  The internal  effect
+           (row removal) is implementation dependent."
+       ::= { ospfHostEntry 4 }
+
+
+    ospfHostAreaID OBJECT-TYPE
+        SYNTAX   AreaID
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The Area the Host Entry is to be found within.
+           By  default, the area that a subsuming OSPF in-
+           terface is in, or 0.0.0.0"
+       REFERENCE
+          "OSPF Version 2, Appendix C.2 Area parameters"
+      ::= { ospfHostEntry 5 }
+
+
+--  OSPF Interface Table
+
+--      The OSPF Interface Table augments the ipAddrTable
+--             with OSPF specific information.
+
+    ospfIfTable OBJECT-TYPE
+        SYNTAX   SEQUENCE OF OspfIfEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "The OSPF Interface Table describes the  inter-
+           faces from the viewpoint of OSPF."
+       REFERENCE
+          "OSPF Version 2, Appendix C.3  Router  interface
+          parameters"
+      ::= { ospf 7 }
+
+
+    ospfIfEntry OBJECT-TYPE
+        SYNTAX   OspfIfEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "The OSPF Interface Entry describes one  inter-
+           face from the viewpoint of OSPF."
+       INDEX { ospfIfIpAddress, ospfAddressLessIf }
+       ::= { ospfIfTable 1 }
+
+OspfIfEntry ::=
+    SEQUENCE {
+        ospfIfIpAddress
+            IpAddress,
+        ospfAddressLessIf
+            Integer32,
+        ospfIfAreaId
+            AreaID,
+        ospfIfType
+            INTEGER,
+        ospfIfAdminStat
+            Status,
+        ospfIfRtrPriority
+            DesignatedRouterPriority,
+        ospfIfTransitDelay
+            UpToMaxAge,
+        ospfIfRetransInterval
+            UpToMaxAge,
+        ospfIfHelloInterval
+            HelloRange,
+        ospfIfRtrDeadInterval
+            PositiveInteger,
+        ospfIfPollInterval
+            PositiveInteger,
+        ospfIfState
+            INTEGER,
+        ospfIfDesignatedRouter
+            IpAddress,
+        ospfIfBackupDesignatedRouter
+            IpAddress,
+        ospfIfEvents
+            Counter32,
+        ospfIfAuthType
+            INTEGER,
+        ospfIfAuthKey
+            OCTET STRING,
+        ospfIfStatus
+            RowStatus,
+        ospfIfMulticastForwarding
+            INTEGER,
+        ospfIfDemand
+            TruthValue
+              }
+
+    ospfIfIpAddress OBJECT-TYPE
+        SYNTAX   IpAddress
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The IP address of this OSPF interface."
+       ::= { ospfIfEntry 1 }
+
+    ospfAddressLessIf OBJECT-TYPE
+        SYNTAX   Integer32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "For the purpose of easing  the  instancing  of
+           addressed   and  addressless  interfaces;  This
+           variable takes the value 0 on  interfaces  with
+           IP  Addresses,  and  the corresponding value of
+           ifIndex for interfaces having no IP Address."
+       ::= { ospfIfEntry 2 }
+    ospfIfAreaId OBJECT-TYPE
+        SYNTAX   AreaID
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "A 32-bit integer uniquely identifying the area
+           to  which  the  interface  connects.   Area  ID
+           0.0.0.0 is used for the OSPF backbone."
+       DEFVAL   { '00000000'H }    -- 0.0.0.0
+       ::= { ospfIfEntry 3 }
+
+    ospfIfType OBJECT-TYPE
+        SYNTAX   INTEGER    {
+                    broadcast (1),
+                    nbma (2),
+                    pointToPoint (3),
+                    pointToMultipoint (5)
+                  }
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The OSPF interface type.
+
+           By way of a default, this field may be intuited
+           from the corresponding value of ifType.  Broad-
+           cast LANs, such as  Ethernet  and  IEEE  802.5,
+           take  the  value  'broadcast', X.25 and similar
+           technologies take the value 'nbma',  and  links
+           that  are  definitively point to point take the
+           value 'pointToPoint'."
+       ::= { ospfIfEntry 4 }
+
+
+    ospfIfAdminStat OBJECT-TYPE
+        SYNTAX   Status
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The OSPF  interface's  administrative  status.
+           The  value formed on the interface, and the in-
+           terface will be advertised as an internal route
+           to  some  area.   The  value 'disabled' denotes
+           that the interface is external to OSPF."
+       DEFVAL { enabled }
+       ::= { ospfIfEntry 5 }
+
+    ospfIfRtrPriority OBJECT-TYPE
+        SYNTAX   DesignatedRouterPriority
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The  priority  of  this  interface.   Used  in
+           multi-access  networks,  this  field is used in
+           the designated router election algorithm.   The
+           value 0 signifies that the router is not eligi-
+           ble to become the  designated  router  on  this
+           particular  network.   In the event of a tie in
+           this value, routers will use their Router ID as
+           a tie breaker."
+       DEFVAL { 1 }
+       ::= { ospfIfEntry 6 }
+
+
+    ospfIfTransitDelay OBJECT-TYPE
+        SYNTAX   UpToMaxAge
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The estimated number of seconds  it  takes  to
+           transmit  a  link state update packet over this
+           interface."
+       DEFVAL { 1 }
+       ::= { ospfIfEntry 7 }
+
+
+    ospfIfRetransInterval OBJECT-TYPE
+        SYNTAX   UpToMaxAge
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The number of seconds between  link-state  ad-
+           vertisement  retransmissions,  for  adjacencies
+           belonging to this  interface.   This  value  is
+           also used when retransmitting database descrip-
+           tion and link-state request packets."
+       DEFVAL { 5 }
+       ::= { ospfIfEntry 8 }
+
+
+    ospfIfHelloInterval OBJECT-TYPE
+        SYNTAX   HelloRange
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The length of time, in  seconds,  between  the
+           Hello  packets that the router sends on the in-
+           terface.  This value must be the same  for  all
+           routers attached to a common network."
+       DEFVAL { 10 }
+       ::= { ospfIfEntry 9 }
+
+
+    ospfIfRtrDeadInterval OBJECT-TYPE
+        SYNTAX   PositiveInteger
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The number of seconds that  a  router's  Hello
+           packets  have  not been seen before it's neigh-
+           bors declare the router down.  This  should  be
+           some  multiple  of  the  Hello  interval.  This
+           value must be the same for all routers attached
+           to a common network."
+       DEFVAL { 40 }
+       ::= { ospfIfEntry 10 }
+
+
+    ospfIfPollInterval OBJECT-TYPE
+        SYNTAX   PositiveInteger
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The larger time interval, in seconds,  between
+           the  Hello  packets  sent  to  an inactive non-
+           broadcast multi- access neighbor."
+       DEFVAL { 120 }
+       ::= { ospfIfEntry 11 }
+
+
+    ospfIfState OBJECT-TYPE
+        SYNTAX   INTEGER    {
+                    down (1),
+                    loopback (2),
+                    waiting (3),
+                    pointToPoint (4),
+                    designatedRouter (5),
+                    backupDesignatedRouter (6),
+                    otherDesignatedRouter (7)
+                  }
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The OSPF Interface State."
+       DEFVAL { down }
+       ::= { ospfIfEntry 12 }
+
+
+    ospfIfDesignatedRouter OBJECT-TYPE
+        SYNTAX   IpAddress
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The IP Address of the Designated Router."
+       DEFVAL   { '00000000'H }    -- 0.0.0.0
+       ::= { ospfIfEntry 13 }
+
+
+    ospfIfBackupDesignatedRouter OBJECT-TYPE
+        SYNTAX   IpAddress
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The  IP  Address  of  the  Backup   Designated
+           Router."
+       DEFVAL   { '00000000'H }    -- 0.0.0.0
+       ::= { ospfIfEntry 14 }
+
+    ospfIfEvents OBJECT-TYPE
+        SYNTAX   Counter32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The number of times this  OSPF  interface  has
+           changed its state, or an error has occurred."
+       ::= { ospfIfEntry 15 }
+
+
+    ospfIfAuthKey OBJECT-TYPE
+        SYNTAX   OCTET STRING (SIZE (0..256))
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The Authentication Key.  If the Area's Author-
+           ization  Type  is  simplePassword,  and the key
+           length is shorter than 8 octets, the agent will
+           left adjust and zero fill to 8 octets.
+
+           Note that unauthenticated  interfaces  need  no
+           authentication key, and simple password authen-
+           tication cannot use a key of more  than  8  oc-
+           tets.  Larger keys are useful only with authen-
+           tication mechanisms not specified in this docu-
+           ment.
+
+           When read, ospfIfAuthKey always returns an  Oc-
+           tet String of length zero."
+       REFERENCE
+          "OSPF Version 2, Section 9  The  Interface  Data
+          Structure"
+      DEFVAL   { '0000000000000000'H }    -- 0.0.0.0.0.0.0.0
+      ::= { ospfIfEntry 16 }
+
+    ospfIfStatus OBJECT-TYPE
+        SYNTAX   RowStatus
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "This variable displays the status of  the  en-
+           try.  Setting it to 'invalid' has the effect of
+           rendering it inoperative.  The internal  effect
+           (row removal) is implementation dependent."
+       ::= { ospfIfEntry 17 }
+
+
+    ospfIfMulticastForwarding OBJECT-TYPE
+        SYNTAX   INTEGER    {
+                            blocked (1),        -- no multicast forwarding
+                            multicast (2),        -- using multicast address
+                            unicast (3)        -- to each OSPF neighbor
+                  }
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The way multicasts should  forwarded  on  this
+           interface;  not  forwarded,  forwarded  as data
+           link multicasts, or forwarded as data link uni-
+           casts.   Data link multicasting is not meaning-
+           ful on point to point and NBMA interfaces,  and
+           setting ospfMulticastForwarding to 0 effective-
+           ly disables all multicast forwarding."
+       DEFVAL { blocked }
+       ::= { ospfIfEntry 18 }
+
+
+    ospfIfDemand OBJECT-TYPE
+        SYNTAX   TruthValue
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "Indicates whether Demand OSPF procedures (hel-
+           lo supression to FULL neighbors and setting the
+           DoNotAge flag on proogated LSAs) should be per-
+           formed on this interface."
+       DEFVAL { false }
+       ::= { ospfIfEntry 19 }
+
+
+    ospfIfAuthType OBJECT-TYPE
+        SYNTAX   INTEGER (0..255)
+                    -- none (0),
+                    -- simplePassword (1)
+                    -- md5 (2)
+                    -- reserved for specification by IANA (> 2)
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The authentication type specified for  an  in-
+           terface.   Additional  authentication types may
+           be assigned locally."
+       REFERENCE
+          "OSPF Version 2, Appendix E Authentication"
+      DEFVAL { 0 }        -- no authentication, by default
+      ::= { ospfIfEntry 20 }
+
+
+--  OSPF Interface Metric Table
+
+--      The Metric Table describes the metrics to be advertised
+--      for a specified interface at the various types of service.
+--      As such, this table is an adjunct of the OSPF Interface
+--      Table.
+
+-- Types of service, as defined by RFC 791, have the ability
+-- to request low delay, high bandwidth, or reliable linkage.
+
+-- For the purposes of this specification, the measure of
+-- bandwidth
+
+--      Metric = 10^8 / ifSpeed
+
+-- is the default value.  For multiple link interfaces, note
+-- that ifSpeed is the sum of the individual link speeds.
+-- This yields a number having the following typical values:
+
+--      Network Type/bit rate   Metric
+
+--      >= 100 MBPS                 1
+--      Ethernet/802.3             10
+--      E1                         48
+--      T1 (ESF)                   65
+--       64 KBPS                 1562
+--       56 KBPS                 1785
+--       19.2 KBPS               5208
+--        9.6 KBPS              10416
+
+-- Routes that are not specified use the default (TOS 0) metric
+
+    ospfIfMetricTable OBJECT-TYPE
+        SYNTAX   SEQUENCE OF OspfIfMetricEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "The TOS metrics for  a  non-virtual  interface
+           identified by the interface index."
+       REFERENCE
+          "OSPF Version 2, Appendix C.3  Router  interface
+          parameters"
+      ::= { ospf 8 }
+
+    ospfIfMetricEntry OBJECT-TYPE
+        SYNTAX   OspfIfMetricEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "A particular TOS metric for a non-virtual  in-
+           terface identified by the interface index."
+       REFERENCE
+          "OSPF Version 2, Appendix C.3  Router  interface
+          parameters"
+      INDEX { ospfIfMetricIpAddress,
+  ospfIfMetricAddressLessIf,
+  ospfIfMetricTOS }
+      ::= { ospfIfMetricTable 1 }
+
+OspfIfMetricEntry ::=
+    SEQUENCE {
+        ospfIfMetricIpAddress
+            IpAddress,
+        ospfIfMetricAddressLessIf
+            Integer32,
+        ospfIfMetricTOS
+            TOSType,
+        ospfIfMetricValue
+            Metric,
+        ospfIfMetricStatus
+            RowStatus
+              }
+
+    ospfIfMetricIpAddress OBJECT-TYPE
+        SYNTAX   IpAddress
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The IP address of this OSPF interface.  On row
+           creation,  this  can  be  derived  from the in-
+           stance."
+       ::= { ospfIfMetricEntry 1 }
+
+    ospfIfMetricAddressLessIf OBJECT-TYPE
+        SYNTAX   Integer32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "For the purpose of easing  the  instancing  of
+           addressed   and  addressless  interfaces;  This
+           variable takes the value 0 on  interfaces  with
+           IP  Addresses, and the value of ifIndex for in-
+           terfaces having no IP Address.   On  row  crea-
+           tion, this can be derived from the instance."
+       ::= { ospfIfMetricEntry 2 }
+
+
+    ospfIfMetricTOS OBJECT-TYPE
+        SYNTAX   TOSType
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The type of service metric  being  referenced.
+           On  row  creation, this can be derived from the
+           instance."
+       ::= { ospfIfMetricEntry 3 }
+
+
+    ospfIfMetricValue OBJECT-TYPE
+        SYNTAX   Metric
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The metric of using this type  of  service  on
+           this interface.  The default value of the TOS 0
+           Metric is 10^8 / ifSpeed."
+       ::= { ospfIfMetricEntry 4 }
+
+    ospfIfMetricStatus OBJECT-TYPE
+        SYNTAX   RowStatus
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "This variable displays the status of  the  en-
+           try.  Setting it to 'invalid' has the effect of
+           rendering it inoperative.  The internal  effect
+           (row removal) is implementation dependent."
+       ::= { ospfIfMetricEntry 5 }
+
+
+--  OSPF Virtual Interface Table
+
+--      The Virtual Interface Table describes the virtual
+--      links that the OSPF Process is configured to
+--      carry on.
+
+    ospfVirtIfTable OBJECT-TYPE
+        SYNTAX   SEQUENCE OF OspfVirtIfEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "Information about this router's virtual inter-
+           faces."
+       REFERENCE
+          "OSPF Version  2,  Appendix  C.4   Virtual  link
+          parameters"
+      ::= { ospf 9 }
+
+
+    ospfVirtIfEntry OBJECT-TYPE
+        SYNTAX   OspfVirtIfEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "Information about a single Virtual Interface."
+       INDEX { ospfVirtIfAreaId, ospfVirtIfNeighbor }
+       ::= { ospfVirtIfTable 1 }
+
+OspfVirtIfEntry ::=
+    SEQUENCE {
+        ospfVirtIfAreaId
+            AreaID,
+        ospfVirtIfNeighbor
+            RouterID,
+        ospfVirtIfTransitDelay
+            UpToMaxAge,
+        ospfVirtIfRetransInterval
+            UpToMaxAge,
+        ospfVirtIfHelloInterval
+            HelloRange,
+        ospfVirtIfRtrDeadInterval
+            PositiveInteger,
+        ospfVirtIfState
+            INTEGER,
+        ospfVirtIfEvents
+            Counter32,
+        ospfVirtIfAuthType
+            INTEGER,
+        ospfVirtIfAuthKey
+            OCTET STRING,
+        ospfVirtIfStatus
+            RowStatus
+              }
+
+    ospfVirtIfAreaId OBJECT-TYPE
+        SYNTAX   AreaID
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The  Transit  Area  that  the   Virtual   Link
+           traverses.  By definition, this is not 0.0.0.0"
+       ::= { ospfVirtIfEntry 1 }
+
+
+    ospfVirtIfNeighbor OBJECT-TYPE
+        SYNTAX   RouterID
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The Router ID of the Virtual Neighbor."
+       ::= { ospfVirtIfEntry 2 }
+
+
+    ospfVirtIfTransitDelay OBJECT-TYPE
+        SYNTAX   UpToMaxAge
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The estimated number of seconds  it  takes  to
+           transmit  a link- state update packet over this
+           interface."
+       DEFVAL { 1 }
+       ::= { ospfVirtIfEntry 3 }
+
+
+    ospfVirtIfRetransInterval OBJECT-TYPE
+        SYNTAX   UpToMaxAge
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The number of seconds between  link-state  ad-
+           vertisement  retransmissions,  for  adjacencies
+           belonging to this  interface.   This  value  is
+           also used when retransmitting database descrip-
+           tion  and  link-state  request  packets.   This
+           value  should  be well over the expected round-
+           trip time."
+       DEFVAL { 5 }
+       ::= { ospfVirtIfEntry 4 }
+
+
+    ospfVirtIfHelloInterval OBJECT-TYPE
+        SYNTAX   HelloRange
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The length of time, in  seconds,  between  the
+           Hello  packets that the router sends on the in-
+           terface.  This value must be the same  for  the
+           virtual neighbor."
+       DEFVAL { 10 }
+       ::= { ospfVirtIfEntry 5 }
+
+
+    ospfVirtIfRtrDeadInterval OBJECT-TYPE
+        SYNTAX   PositiveInteger
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The number of seconds that  a  router's  Hello
+           packets  have  not been seen before it's neigh-
+           bors declare the router down.  This  should  be
+           some  multiple  of  the  Hello  interval.  This
+           value must be the same for the  virtual  neigh-
+           bor."
+       DEFVAL { 60 }
+       ::= { ospfVirtIfEntry 6 }
+
+
+    ospfVirtIfState OBJECT-TYPE
+        SYNTAX   INTEGER    {
+                    down (1),            -- these use the same encoding
+                    pointToPoint (4)     -- as the ospfIfTable
+                  }
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "OSPF virtual interface states."
+       DEFVAL   { down }
+       ::= { ospfVirtIfEntry 7 }
+
+
+    ospfVirtIfEvents OBJECT-TYPE
+        SYNTAX   Counter32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The number of state changes or error events on
+           this Virtual Link"
+       ::= { ospfVirtIfEntry 8 }
+
+
+    ospfVirtIfAuthKey OBJECT-TYPE
+        SYNTAX   OCTET STRING (SIZE(0..256))
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "If Authentication Type is simplePassword,  the
+           device  will left adjust and zero fill to 8 oc-
+           tets.
+
+           Note that unauthenticated  interfaces  need  no
+           authentication key, and simple password authen-
+           tication cannot use a key of more  than  8  oc-
+           tets.  Larger keys are useful only with authen-
+           tication mechanisms not specified in this docu-
+           ment.
+
+           When  read,  ospfVifAuthKey  always  returns  a
+           string of length zero."
+       REFERENCE
+          "OSPF Version 2, Section 9  The  Interface  Data
+          Structure"
+      DEFVAL   { '0000000000000000'H }    -- 0.0.0.0.0.0.0.0
+      ::= { ospfVirtIfEntry 9 }
+
+
+    ospfVirtIfStatus OBJECT-TYPE
+        SYNTAX   RowStatus
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "This variable displays the status of  the  en-
+           try.  Setting it to 'invalid' has the effect of
+           rendering it inoperative.  The internal  effect
+           (row removal) is implementation dependent."
+       ::= { ospfVirtIfEntry 10 }
+
+
+    ospfVirtIfAuthType OBJECT-TYPE
+        SYNTAX   INTEGER (0..255)
+                    -- none (0),
+                    -- simplePassword (1)
+                    -- md5 (2)
+                    -- reserved for specification by IANA (> 2)
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The authentication type specified for a virtu-
+           al  interface.  Additional authentication types
+           may be assigned locally."
+       REFERENCE
+          "OSPF Version 2, Appendix E Authentication"
+      DEFVAL { 0 }        -- no authentication, by default
+      ::= { ospfVirtIfEntry 11 }
+
+
+--  OSPF Neighbor Table
+
+--      The OSPF Neighbor Table describes all neighbors in
+--      the locality of the subject router.
+
+    ospfNbrTable OBJECT-TYPE
+        SYNTAX   SEQUENCE OF OspfNbrEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "A table of non-virtual neighbor information."
+       REFERENCE
+          "OSPF Version 2, Section 10  The  Neighbor  Data
+          Structure"
+      ::= { ospf 10 }
+
+
+    ospfNbrEntry OBJECT-TYPE
+        SYNTAX   OspfNbrEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "The information regarding a single neighbor."
+       REFERENCE
+          "OSPF Version 2, Section 10  The  Neighbor  Data
+          Structure"
+      INDEX { ospfNbrIpAddr, ospfNbrAddressLessIndex }
+      ::= { ospfNbrTable 1 }
+
+OspfNbrEntry ::=
+    SEQUENCE {
+        ospfNbrIpAddr
+            IpAddress,
+        ospfNbrAddressLessIndex
+            InterfaceIndex,
+        ospfNbrRtrId
+            RouterID,
+        ospfNbrOptions
+            Integer32,
+        ospfNbrPriority
+            DesignatedRouterPriority,
+        ospfNbrState
+            INTEGER,
+        ospfNbrEvents
+            Counter32,
+        ospfNbrLsRetransQLen
+            Gauge32,
+        ospfNbmaNbrStatus
+            RowStatus,
+        ospfNbmaNbrPermanence
+            INTEGER,
+        ospfNbrHelloSuppressed
+            TruthValue
+              }
+
+    ospfNbrIpAddr OBJECT-TYPE
+        SYNTAX   IpAddress
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The IP address this neighbor is using  in  its
+           IP  Source  Address.  Note that, on addressless
+           links, this will not be 0.0.0.0,  but  the  ad-
+           dress of another of the neighbor's interfaces."
+       ::= { ospfNbrEntry 1 }
+
+
+    ospfNbrAddressLessIndex OBJECT-TYPE
+        SYNTAX   InterfaceIndex
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "On an interface having an  IP  Address,  zero.
+           On  addressless  interfaces,  the corresponding
+           value of ifIndex in the Internet Standard  MIB.
+           On  row  creation, this can be derived from the
+           instance."
+       ::= { ospfNbrEntry 2 }
+
+
+    ospfNbrRtrId OBJECT-TYPE
+        SYNTAX   RouterID
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "A 32-bit integer (represented as a type  IpAd-
+           dress)  uniquely  identifying  the  neighboring
+           router in the Autonomous System."
+       DEFVAL   { '00000000'H }    -- 0.0.0.0
+       ::= { ospfNbrEntry 3 }
+
+
+    ospfNbrOptions OBJECT-TYPE
+        SYNTAX   Integer32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "A Bit Mask corresponding to the neighbor's op-
+           tions field.
+
+           Bit 0, if set, indicates that the  system  will
+           operate  on  Type of Service metrics other than
+           TOS 0.  If zero, the neighbor will  ignore  all
+           metrics except the TOS 0 metric.
+
+           Bit 1, if set, indicates  that  the  associated
+           area  accepts and operates on external informa-
+           tion; if zero, it is a stub area.
+
+           Bit 2, if set, indicates that the system is ca-
+           pable  of routing IP Multicast datagrams; i.e.,
+           that it implements the Multicast Extensions  to
+           OSPF.
+
+           Bit 3, if set, indicates  that  the  associated
+           area  is  an  NSSA.  These areas are capable of
+           carrying type 7 external advertisements,  which
+           are  translated into type 5 external advertise-
+           ments at NSSA borders."
+       REFERENCE
+          "OSPF Version 2, Section 12.1.2 Options"
+      DEFVAL { 0 }
+      ::= { ospfNbrEntry 4 }
+
+
+    ospfNbrPriority OBJECT-TYPE
+        SYNTAX   DesignatedRouterPriority
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The priority of this neighbor in the designat-
+           ed router election algorithm.  The value 0 sig-
+           nifies that the neighbor is not eligible to be-
+           come  the  designated router on this particular
+           network."
+       DEFVAL { 1 }
+       ::= { ospfNbrEntry 5 }
+
+
+    ospfNbrState OBJECT-TYPE
+        SYNTAX   INTEGER    {
+                    down (1),
+                    attempt (2),
+                    init (3),
+                    twoWay (4),
+                    exchangeStart (5),
+                    exchange (6),
+                    loading (7),
+                    full (8)
+                  }
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The State of the relationship with this Neigh-
+           bor."
+       REFERENCE
+          "OSPF Version 2, Section 10.1 Neighbor States"
+      DEFVAL   { down }
+      ::= { ospfNbrEntry 6 }
+
+
+    ospfNbrEvents OBJECT-TYPE
+        SYNTAX   Counter32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The number of times this neighbor relationship
+           has changed state, or an error has occurred."
+       ::= { ospfNbrEntry 7 }
+
+
+    ospfNbrLsRetransQLen OBJECT-TYPE
+        SYNTAX   Gauge32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The  current  length  of  the   retransmission
+           queue."
+       ::= { ospfNbrEntry 8 }
+
+
+    ospfNbmaNbrStatus OBJECT-TYPE
+        SYNTAX   RowStatus
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "This variable displays the status of  the  en-
+           try.  Setting it to 'invalid' has the effect of
+           rendering it inoperative.  The internal  effect
+           (row removal) is implementation dependent."
+       ::= { ospfNbrEntry 9 }
+
+
+    ospfNbmaNbrPermanence OBJECT-TYPE
+        SYNTAX   INTEGER    {
+                    dynamic (1),        -- learned through protocol
+                    permanent (2)       -- configured address
+                  }
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "This variable displays the status of  the  en-
+           try.   'dynamic'  and  'permanent' refer to how
+           the neighbor became known."
+       DEFVAL { permanent }
+       ::= { ospfNbrEntry 10 }
+
+
+    ospfNbrHelloSuppressed OBJECT-TYPE
+        SYNTAX   TruthValue
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "Indicates whether Hellos are being  suppressed
+           to the neighbor"
+       ::= { ospfNbrEntry 11 }
+
+
+--  OSPF Virtual Neighbor Table
+
+--      This table describes all virtual neighbors.
+--      Since Virtual Links are configured in the
+--      virtual interface table, this table is read-only.
+
+    ospfVirtNbrTable OBJECT-TYPE
+        SYNTAX   SEQUENCE OF OspfVirtNbrEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "A table of virtual neighbor information."
+       REFERENCE
+          "OSPF Version 2, Section 15  Virtual Links"
+      ::= { ospf 11 }
+
+
+    ospfVirtNbrEntry OBJECT-TYPE
+        SYNTAX   OspfVirtNbrEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "Virtual neighbor information."
+       INDEX { ospfVirtNbrArea, ospfVirtNbrRtrId }
+       ::= { ospfVirtNbrTable 1 }
+
+OspfVirtNbrEntry ::=
+    SEQUENCE {
+        ospfVirtNbrArea
+            AreaID,
+        ospfVirtNbrRtrId
+            RouterID,
+        ospfVirtNbrIpAddr
+            IpAddress,
+        ospfVirtNbrOptions
+            Integer32,
+        ospfVirtNbrState
+            INTEGER,
+        ospfVirtNbrEvents
+            Counter32,
+        ospfVirtNbrLsRetransQLen
+            Gauge32,
+        ospfVirtNbrHelloSuppressed
+                TruthValue
+              }
+
+    ospfVirtNbrArea OBJECT-TYPE
+        SYNTAX   AreaID
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The Transit Area Identifier."
+       ::= { ospfVirtNbrEntry 1 }
+
+
+    ospfVirtNbrRtrId OBJECT-TYPE
+        SYNTAX   RouterID
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "A  32-bit  integer  uniquely  identifying  the
+           neighboring router in the Autonomous System."
+       ::= { ospfVirtNbrEntry 2 }
+
+
+    ospfVirtNbrIpAddr OBJECT-TYPE
+        SYNTAX   IpAddress
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The IP address this Virtual  Neighbor  is  us-
+           ing."
+       ::= { ospfVirtNbrEntry 3 }
+
+
+    ospfVirtNbrOptions OBJECT-TYPE
+        SYNTAX   Integer32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "A Bit Mask corresponding to the neighbor's op-
+           tions field.
+
+           Bit 1, if set, indicates that the  system  will
+           operate  on  Type of Service metrics other than
+           TOS 0.  If zero, the neighbor will  ignore  all
+           metrics except the TOS 0 metric.
+
+           Bit 2, if set, indicates  that  the  system  is
+           Network  Multicast  capable; ie, that it imple-
+           ments OSPF Multicast Routing."
+       ::= { ospfVirtNbrEntry 4 }
+    ospfVirtNbrState OBJECT-TYPE
+        SYNTAX   INTEGER    {
+                    down (1),
+                    attempt (2),
+                    init (3),
+                    twoWay (4),
+                    exchangeStart (5),
+                    exchange (6),
+                    loading (7),
+                    full (8)
+                  }
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The state of the  Virtual  Neighbor  Relation-
+           ship."
+       ::= { ospfVirtNbrEntry 5 }
+
+
+    ospfVirtNbrEvents OBJECT-TYPE
+        SYNTAX   Counter32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The number of  times  this  virtual  link  has
+           changed its state, or an error has occurred."
+       ::= { ospfVirtNbrEntry 6 }
+
+
+    ospfVirtNbrLsRetransQLen OBJECT-TYPE
+        SYNTAX   Gauge32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The  current  length  of  the   retransmission
+           queue."
+       ::= { ospfVirtNbrEntry 7 }
+
+
+    ospfVirtNbrHelloSuppressed OBJECT-TYPE
+        SYNTAX   TruthValue
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "Indicates whether Hellos are being  suppressed
+           to the neighbor"
+       ::= { ospfVirtNbrEntry 8 }
+
+--  OSPF Link State Database, External
+
+--      The Link State Database contains the Link State
+--      Advertisements from throughout the areas that the
+--      device is attached to.
+
+--             This table is identical to the OSPF LSDB Table in
+--      format, but contains only External Link State
+--             Advertisements.  The purpose is to allow external
+--      LSAs to be displayed once for the router rather
+--      than once in each non-stub area.
+
+    ospfExtLsdbTable OBJECT-TYPE
+        SYNTAX   SEQUENCE OF OspfExtLsdbEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "The OSPF Process's Links State Database."
+       REFERENCE
+          "OSPF Version 2, Section 12  Link  State  Adver-
+          tisements"
+      ::= { ospf 12 }
+
+
+    ospfExtLsdbEntry OBJECT-TYPE
+        SYNTAX   OspfExtLsdbEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "A single Link State Advertisement."
+       INDEX { ospfExtLsdbType, ospfExtLsdbLsid, ospfExtLsdbRouterId }
+       ::= { ospfExtLsdbTable 1 }
+
+OspfExtLsdbEntry ::=
+    SEQUENCE {
+        ospfExtLsdbType
+            INTEGER,
+        ospfExtLsdbLsid
+            IpAddress,
+        ospfExtLsdbRouterId
+            RouterID,
+        ospfExtLsdbSequence
+            Integer32,
+        ospfExtLsdbAge
+            Integer32,
+        ospfExtLsdbChecksum
+            Integer32,
+        ospfExtLsdbAdvertisement
+            OCTET STRING
+              }
+
+    ospfExtLsdbType OBJECT-TYPE
+        SYNTAX   INTEGER    {
+                    asExternalLink (5)
+                  }
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The type  of  the  link  state  advertisement.
+           Each  link state type has a separate advertise-
+           ment format."
+       REFERENCE
+          "OSPF Version 2, Appendix A.4.1 The  Link  State
+          Advertisement header"
+      ::= { ospfExtLsdbEntry 1 }
+
+
+    ospfExtLsdbLsid OBJECT-TYPE
+        SYNTAX   IpAddress
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The Link State ID is an LS Type Specific field
+           containing either a Router ID or an IP Address;
+           it identifies the piece of the  routing  domain
+           that is being described by the advertisement."
+       REFERENCE
+          "OSPF Version 2, Section 12.1.4 Link State ID"
+      ::= { ospfExtLsdbEntry 2 }
+
+
+    ospfExtLsdbRouterId OBJECT-TYPE
+        SYNTAX   RouterID
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The 32 bit number that uniquely identifies the
+           originating router in the Autonomous System."
+       REFERENCE
+          "OSPF Version 2, Appendix C.1 Global parameters"
+      ::= { ospfExtLsdbEntry 3 }
+
+--  Note that the OSPF Sequence Number is a 32 bit signed
+--  integer.  It starts with the value '80000001'h,
+--  or -'7FFFFFFF'h, and increments until '7FFFFFFF'h
+--  Thus, a typical sequence number will be very negative.
+    ospfExtLsdbSequence OBJECT-TYPE
+        SYNTAX   Integer32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The sequence number field is a  signed  32-bit
+           integer.   It  is used to detect old and dupli-
+           cate link state advertisements.  The  space  of
+           sequence  numbers  is  linearly  ordered.   The
+           larger the sequence number the more recent  the
+           advertisement."
+       REFERENCE
+          "OSPF Version  2,  Section  12.1.6  LS  sequence
+          number"
+      ::= { ospfExtLsdbEntry 4 }
+
+
+    ospfExtLsdbAge OBJECT-TYPE
+        SYNTAX   Integer32    -- Should be 0..MaxAge
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "This field is the age of the link state adver-
+           tisement in seconds."
+       REFERENCE
+          "OSPF Version 2, Section 12.1.1 LS age"
+      ::= { ospfExtLsdbEntry 5 }
+
+
+    ospfExtLsdbChecksum OBJECT-TYPE
+        SYNTAX   Integer32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "This field is the  checksum  of  the  complete
+           contents  of  the  advertisement, excepting the
+           age field.  The age field is excepted  so  that
+           an   advertisement's  age  can  be  incremented
+           without updating the  checksum.   The  checksum
+           used  is  the same that is used for ISO connec-
+           tionless datagrams; it is commonly referred  to
+           as the Fletcher checksum."
+       REFERENCE
+          "OSPF Version 2, Section 12.1.7 LS checksum"
+      ::= { ospfExtLsdbEntry 6 }
+
+
+    ospfExtLsdbAdvertisement OBJECT-TYPE
+        SYNTAX   OCTET STRING (SIZE(36))
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The entire Link State Advertisement, including
+           its header."
+       REFERENCE
+          "OSPF Version 2, Section 12  Link  State  Adver-
+          tisements"
+      ::= { ospfExtLsdbEntry 7 }
+
+
+--  OSPF Use of the CIDR Route Table
+
+ospfRouteGroup           OBJECT IDENTIFIER ::= { ospf 13 }
+
+-- The IP Forwarding Table defines a number of objects for use by
+-- the routing protocol to externalize its information.  Most of
+-- the variables (ipForwardDest, ipForwardMask, ipForwardPolicy,
+-- ipForwardNextHop, ipForwardIfIndex, ipForwardType,
+-- ipForwardProto, ipForwardAge, and ipForwardNextHopAS) are
+-- defined there.
+
+-- Those that leave some discretion are defined here.
+
+-- ipCidrRouteProto is, of course, ospf (13).
+
+-- ipCidrRouteAge is the time since the route was first calculated,
+-- as opposed to the time since the last SPF run.
+
+-- ipCidrRouteInfo is an OBJECT IDENTIFIER for use by the routing
+-- protocol.  The following values shall be found there depending
+-- on the way the route was calculated.
+
+ospfIntraArea      OBJECT IDENTIFIER ::= { ospfRouteGroup 1 }
+ospfInterArea      OBJECT IDENTIFIER ::= { ospfRouteGroup 2 }
+ospfExternalType1  OBJECT IDENTIFIER ::= { ospfRouteGroup 3 }
+ospfExternalType2  OBJECT IDENTIFIER ::= { ospfRouteGroup 4 }
+
+-- ipCidrRouteMetric1 is, by definition, the primary routing
+-- metric.  Therefore, it should be the metric that route
+-- selection is based on.  For intra-area and inter-area routes,
+-- it is an OSPF metric.  For External Type 1 (comparable value)
+-- routes, it is an OSPF metric plus the External Metric.  For
+-- external Type 2 (non-comparable value) routes, it is the
+-- external metric.
+
+-- ipCidrRouteMetric2 is, by definition, a secondary routing
+-- metric.  Therefore, it should be the metric that breaks a tie
+-- among routes having equal metric1 values and the same
+-- calculation rule.  For intra-area, inter-area routes, and
+-- External Type 1 (comparable value) routes, it is unused.  For
+-- external Type 2 (non-comparable value) routes, it is the metric
+-- to the AS border router.
+
+-- ipCidrRouteMetric3, ipCidrRouteMetric4, and ipCidrRouteMetric5 are
+-- unused.
+
+--
+--      The OSPF Area Aggregate Table
+--
+--      This table replaces the OSPF Area Summary Table, being an
+--      extension of that for CIDR routers.
+
+    ospfAreaAggregateTable OBJECT-TYPE
+        SYNTAX   SEQUENCE OF OspfAreaAggregateEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "A range of IP addresses  specified  by  an  IP
+           address/IP  network  mask  pair.   For example,
+           class B address range of X.X.X.X with a network
+           mask  of  255.255.0.0 includes all IP addresses
+           from X.X.0.0  to  X.X.255.255.   Note  that  if
+           ranges  are configured such that one range sub-
+           sumes  another  range  (e.g.,   10.0.0.0   mask
+           255.0.0.0  and  10.1.0.0 mask 255.255.0.0), the
+           most specific match is the preferred one."
+       REFERENCE
+          "OSPF Version 2, Appendix C.2  Area parameters"
+      ::= { ospf 14 }
+
+
+    ospfAreaAggregateEntry OBJECT-TYPE
+        SYNTAX   OspfAreaAggregateEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "A range of IP addresses  specified  by  an  IP
+           address/IP  network  mask  pair.   For example,
+           class B address range of X.X.X.X with a network
+           mask  of  255.255.0.0 includes all IP addresses
+           from X.X.0.0  to  X.X.255.255.   Note  that  if
+           ranges are range configured such that one range
+           subsumes another  range  (e.g.,  10.0.0.0  mask
+           255.0.0.0  and  10.1.0.0 mask 255.255.0.0), the
+           most specific match is the preferred one."
+       REFERENCE
+          "OSPF Version 2, Appendix C.2  Area parameters"
+      INDEX { ospfAreaAggregateAreaID, ospfAreaAggregateLsdbType,
+              ospfAreaAggregateNet, ospfAreaAggregateMask }
+      ::= { ospfAreaAggregateTable 1 }
+
+
+OspfAreaAggregateEntry ::=
+    SEQUENCE {
+        ospfAreaAggregateAreaID
+            AreaID,
+        ospfAreaAggregateLsdbType
+            INTEGER,
+        ospfAreaAggregateNet
+            IpAddress,
+        ospfAreaAggregateMask
+            IpAddress,
+        ospfAreaAggregateStatus
+            RowStatus,
+        ospfAreaAggregateEffect
+            INTEGER
+              }
+
+    ospfAreaAggregateAreaID OBJECT-TYPE
+        SYNTAX   AreaID
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The Area the Address Aggregate is to be  found
+           within."
+       REFERENCE
+          "OSPF Version 2, Appendix C.2 Area parameters"
+      ::= { ospfAreaAggregateEntry 1 }
+
+
+    ospfAreaAggregateLsdbType OBJECT-TYPE
+        SYNTAX   INTEGER    {
+                    summaryLink (3),
+                    nssaExternalLink (7)
+                  }
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The type of the Address Aggregate.  This field
+           specifies  the  Lsdb type that this Address Ag-
+           gregate applies to."
+       REFERENCE
+          "OSPF Version 2, Appendix A.4.1 The  Link  State
+          Advertisement header"
+      ::= { ospfAreaAggregateEntry 2 }
+
+
+    ospfAreaAggregateNet OBJECT-TYPE
+        SYNTAX   IpAddress
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The IP Address of the Net or Subnet  indicated
+           by the range."
+       REFERENCE
+          "OSPF Version 2, Appendix C.2 Area parameters"
+      ::= { ospfAreaAggregateEntry 3 }
+
+
+    ospfAreaAggregateMask OBJECT-TYPE
+        SYNTAX   IpAddress
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The Subnet Mask that pertains to  the  Net  or
+           Subnet."
+       REFERENCE
+          "OSPF Version 2, Appendix C.2 Area parameters"
+      ::= { ospfAreaAggregateEntry 4 }
+
+
+    ospfAreaAggregateStatus OBJECT-TYPE
+        SYNTAX   RowStatus
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "This variable displays the status of  the  en-
+           try.  Setting it to 'invalid' has the effect of
+           rendering it inoperative.  The internal  effect
+           (row removal) is implementation dependent."
+       ::= { ospfAreaAggregateEntry 5 }
+
+
+    ospfAreaAggregateEffect OBJECT-TYPE
+        SYNTAX   INTEGER    {
+                    advertiseMatching (1),
+                    doNotAdvertiseMatching (2)
+                  }
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "Subnets subsumed by ranges either trigger  the
+           advertisement  of  the indicated aggregate (ad-
+           vertiseMatching), or result in the subnet's not
+           being advertised at all outside the area."
+       DEFVAL   { advertiseMatching }
+       ::= { ospfAreaAggregateEntry 6 }
+
+
+-- conformance information
+
+ospfConformance OBJECT IDENTIFIER ::= { ospf 15 }
+
+ospfGroups      OBJECT IDENTIFIER ::= { ospfConformance 1 }
+ospfCompliances OBJECT IDENTIFIER ::= { ospfConformance 2 }
+
+-- compliance statements
+
+    ospfCompliance MODULE-COMPLIANCE
+        STATUS  current
+        DESCRIPTION
+           "The compliance statement "
+       MODULE  -- this module
+       MANDATORY-GROUPS {
+                    ospfBasicGroup,
+                    ospfAreaGroup,
+                    ospfStubAreaGroup,
+                    ospfIfGroup,
+                    ospfIfMetricGroup,
+                    ospfVirtIfGroup,
+                    ospfNbrGroup,
+                    ospfVirtNbrGroup,
+                    ospfAreaAggregateGroup
+           }
+       ::= { ospfCompliances 1 }
+
+
+-- units of conformance
+
+    ospfBasicGroup    OBJECT-GROUP
+        OBJECTS {
+                    ospfRouterId,
+                    ospfAdminStat,
+                    ospfVersionNumber,
+                    ospfAreaBdrRtrStatus,
+                    ospfASBdrRtrStatus,
+                    ospfExternLsaCount,
+                    ospfExternLsaCksumSum,
+                    ospfTOSSupport,
+                    ospfOriginateNewLsas,
+                    ospfRxNewLsas,
+                    ospfExtLsdbLimit,
+                    ospfMulticastExtensions,
+                    ospfExitOverflowInterval,
+                    ospfDemandExtensions
+        }
+        STATUS  current
+        DESCRIPTION
+           "These objects are required for OSPF systems."
+       ::= { ospfGroups 1 }
+
+
+    ospfAreaGroup    OBJECT-GROUP
+        OBJECTS {
+                    ospfAreaId,
+                    ospfImportAsExtern,
+                    ospfSpfRuns,
+                    ospfAreaBdrRtrCount,
+                    ospfAsBdrRtrCount,
+                    ospfAreaLsaCount,
+                    ospfAreaLsaCksumSum,
+                    ospfAreaSummary,
+                    ospfAreaStatus
+        }
+        STATUS  current
+        DESCRIPTION
+           "These objects are required  for  OSPF  systems
+           supporting areas."
+       ::= { ospfGroups 2 }
+
+
+    ospfStubAreaGroup    OBJECT-GROUP
+        OBJECTS {
+                    ospfStubAreaId,
+                    ospfStubTOS,
+                    ospfStubMetric,
+                    ospfStubStatus,
+                    ospfStubMetricType
+        }
+        STATUS  current
+        DESCRIPTION
+           "These objects are required  for  OSPF  systems
+           supporting stub areas."
+       ::= { ospfGroups 3 }
+
+
+    ospfLsdbGroup    OBJECT-GROUP
+        OBJECTS {
+                    ospfLsdbAreaId,
+                    ospfLsdbType,
+                    ospfLsdbLsid,
+                    ospfLsdbRouterId,
+                    ospfLsdbSequence,
+                    ospfLsdbAge,
+                    ospfLsdbChecksum,
+                    ospfLsdbAdvertisement
+        }
+        STATUS  current
+        DESCRIPTION
+           "These objects are required  for  OSPF  systems
+           that display their link state database."
+       ::= { ospfGroups 4 }
+
+
+    ospfAreaRangeGroup    OBJECT-GROUP
+        OBJECTS {
+                    ospfAreaRangeAreaId,
+                    ospfAreaRangeNet,
+                    ospfAreaRangeMask,
+                    ospfAreaRangeStatus,
+                    ospfAreaRangeEffect
+        }
+        STATUS  obsolete
+        DESCRIPTION
+           "These objects are required for  non-CIDR  OSPF
+           systems that support multiple areas."
+       ::= { ospfGroups 5 }
+
+
+    ospfHostGroup    OBJECT-GROUP
+        OBJECTS {
+                    ospfHostIpAddress,
+                    ospfHostTOS,
+                    ospfHostMetric,
+                    ospfHostStatus,
+                    ospfHostAreaID
+        }
+        STATUS  current
+        DESCRIPTION
+           "These objects are required  for  OSPF  systems
+           that support attached hosts."
+       ::= { ospfGroups 6 }
+
+
+    ospfIfGroup    OBJECT-GROUP
+        OBJECTS {
+                    ospfIfIpAddress,
+                    ospfAddressLessIf,
+                    ospfIfAreaId,
+                    ospfIfType,
+                    ospfIfAdminStat,
+                    ospfIfRtrPriority,
+                    ospfIfTransitDelay,
+                    ospfIfRetransInterval,
+                    ospfIfHelloInterval,
+                    ospfIfRtrDeadInterval,
+                    ospfIfPollInterval,
+                    ospfIfState,
+                    ospfIfDesignatedRouter,
+                    ospfIfBackupDesignatedRouter,
+                    ospfIfEvents,
+                    ospfIfAuthType,
+                    ospfIfAuthKey,
+                    ospfIfStatus,
+                    ospfIfMulticastForwarding,
+                    ospfIfDemand
+        }
+        STATUS  current
+        DESCRIPTION
+           "These objects are required for OSPF systems."
+       ::= { ospfGroups 7 }
+
+
+    ospfIfMetricGroup    OBJECT-GROUP
+        OBJECTS {
+                    ospfIfMetricIpAddress,
+                    ospfIfMetricAddressLessIf,
+                    ospfIfMetricTOS,
+                    ospfIfMetricValue,
+                    ospfIfMetricStatus
+        }
+        STATUS  current
+        DESCRIPTION
+           "These objects are required for OSPF systems."
+       ::= { ospfGroups 8 }
+
+
+    ospfVirtIfGroup    OBJECT-GROUP
+        OBJECTS {
+                    ospfVirtIfAreaId,
+                    ospfVirtIfNeighbor,
+                    ospfVirtIfTransitDelay,
+                    ospfVirtIfRetransInterval,
+                    ospfVirtIfHelloInterval,
+                    ospfVirtIfRtrDeadInterval,
+                    ospfVirtIfState,
+                    ospfVirtIfEvents,
+                    ospfVirtIfAuthType,
+                    ospfVirtIfAuthKey,
+                    ospfVirtIfStatus
+        }
+        STATUS  current
+        DESCRIPTION
+           "These objects are required for OSPF systems."
+       ::= { ospfGroups 9 }
+
+
+    ospfNbrGroup    OBJECT-GROUP
+        OBJECTS {
+                    ospfNbrIpAddr,
+                    ospfNbrAddressLessIndex,
+                    ospfNbrRtrId,
+                    ospfNbrOptions,
+                    ospfNbrPriority,
+                    ospfNbrState,
+                    ospfNbrEvents,
+                    ospfNbrLsRetransQLen,
+                    ospfNbmaNbrStatus,
+                    ospfNbmaNbrPermanence,
+                    ospfNbrHelloSuppressed
+        }
+        STATUS  current
+        DESCRIPTION
+           "These objects are required for OSPF systems."
+       ::= { ospfGroups 10 }
+
+
+    ospfVirtNbrGroup    OBJECT-GROUP
+        OBJECTS {
+                    ospfVirtNbrArea,
+                    ospfVirtNbrRtrId,
+                    ospfVirtNbrIpAddr,
+                    ospfVirtNbrOptions,
+                    ospfVirtNbrState,
+                    ospfVirtNbrEvents,
+                    ospfVirtNbrLsRetransQLen,
+                    ospfVirtNbrHelloSuppressed
+        }
+        STATUS  current
+        DESCRIPTION
+           "These objects are required for OSPF systems."
+       ::= { ospfGroups 11 }
+
+
+    ospfExtLsdbGroup    OBJECT-GROUP
+        OBJECTS {
+                    ospfExtLsdbType,
+                    ospfExtLsdbLsid,
+                    ospfExtLsdbRouterId,
+                    ospfExtLsdbSequence,
+                    ospfExtLsdbAge,
+                    ospfExtLsdbChecksum,
+                    ospfExtLsdbAdvertisement
+        }
+        STATUS  current
+        DESCRIPTION
+           "These objects are required  for  OSPF  systems
+           that display their link state database."
+       ::= { ospfGroups 12 }
+
+
+    ospfAreaAggregateGroup    OBJECT-GROUP
+        OBJECTS {
+                    ospfAreaAggregateAreaID,
+                    ospfAreaAggregateLsdbType,
+                    ospfAreaAggregateNet,
+                    ospfAreaAggregateMask,
+                    ospfAreaAggregateStatus,
+                    ospfAreaAggregateEffect
+        }
+        STATUS  current
+        DESCRIPTION
+           "These objects are required for OSPF systems."
+       ::= { ospfGroups 13 }
+
+END
--- /dev/null
+++ b/mibs/OSPF-TRAP-MIB.txt
@@ -0,0 +1,443 @@
+OSPF-TRAP-MIB DEFINITIONS ::= BEGIN
+
+    IMPORTS
+            MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE, IpAddress
+                FROM SNMPv2-SMI
+            MODULE-COMPLIANCE, OBJECT-GROUP
+                FROM SNMPv2-CONF
+            ospfRouterId, ospfIfIpAddress, ospfAddressLessIf, ospfIfState,
+            ospfVirtIfAreaId, ospfVirtIfNeighbor, ospfVirtIfState,
+            ospfNbrIpAddr, ospfNbrAddressLessIndex, ospfNbrRtrId,
+            ospfNbrState, ospfVirtNbrArea, ospfVirtNbrRtrId, ospfVirtNbrState,
+            ospfLsdbType, ospfLsdbLsid, ospfLsdbRouterId, ospfLsdbAreaId,
+            ospfExtLsdbLimit, ospf
+                FROM OSPF-MIB;
+
+    ospfTrap MODULE-IDENTITY
+           LAST-UPDATED "9501201225Z" -- Fri Jan 20 12:25:50 PST 1995
+           ORGANIZATION "IETF OSPF Working Group"
+           CONTACT-INFO
+           "                      Fred Baker
+           Postal:                Cisco Systems
+                                  519 Lado Drive
+                                  Santa Barbara, California 93111
+           Tel:                   +1 805 681 0115
+           E-Mail:                fred@cisco.com
+
+                                  Rob Coltun
+           Postal:                RainbowBridge Communications
+           Tel:                   (301) 340-9416
+           E-Mail:                rcoltun@rainbow-bridge.com"
+       DESCRIPTION
+          "The MIB module to describe traps for  the  OSPF
+          Version 2 Protocol."
+      ::= { ospf 16 }
+
+-- Trap Support Objects
+
+--         The following are support objects for the OSPF traps.
+
+ospfTrapControl OBJECT IDENTIFIER ::= { ospfTrap 1 }
+ospfTraps OBJECT IDENTIFIER ::= { ospfTrap 2 }
+
+    ospfSetTrap OBJECT-TYPE
+        SYNTAX   OCTET STRING (SIZE(4))
+        MAX-ACCESS   read-write
+        STATUS   current
+        DESCRIPTION
+           "A four-octet string serving as a bit  map  for
+           the trap events defined by the OSPF traps. This
+           object is used to enable and  disable  specific
+           OSPF   traps   where  a  1  in  the  bit  field
+           represents enabled.  The right-most bit  (least
+           significant) represents trap 0."
+       ::= { ospfTrapControl 1 }
+
+
+    ospfConfigErrorType OBJECT-TYPE
+        SYNTAX   INTEGER   {
+                    badVersion (1),
+                    areaMismatch (2),
+                    unknownNbmaNbr (3), -- Router is Dr eligible
+                    unknownVirtualNbr (4),
+                    authTypeMismatch(5),
+                    authFailure (6),
+                    netMaskMismatch (7),
+                    helloIntervalMismatch (8),
+                    deadIntervalMismatch (9),
+                    optionMismatch (10) }
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "Potential types  of  configuration  conflicts.
+           Used  by the ospfConfigError and ospfConfigVir-
+           tError traps."
+   ::= { ospfTrapControl 2 }
+
+
+    ospfPacketType OBJECT-TYPE
+        SYNTAX   INTEGER   {
+                    hello (1),
+                    dbDescript (2),
+                    lsReq (3),
+                    lsUpdate (4),
+                    lsAck (5) }
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "OSPF packet types."
+   ::= { ospfTrapControl 3 }
+
+
+    ospfPacketSrc OBJECT-TYPE
+        SYNTAX   IpAddress
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The IP address of an inbound packet that  can-
+           not be identified by a neighbor instance."
+       ::= { ospfTrapControl 4 }
+
+
+-- Traps
+
+
+    ospfIfStateChange NOTIFICATION-TYPE
+        OBJECTS {
+                    ospfRouterId, -- The originator of the trap
+                    ospfIfIpAddress,
+                    ospfAddressLessIf,
+                    ospfIfState   -- The new state
+                  }
+        STATUS             current
+        DESCRIPTION
+           "An ospfIfStateChange trap signifies that there
+           has been a change in the state of a non-virtual
+           OSPF interface. This trap should  be  generated
+           when  the interface state regresses (e.g., goes
+           from Dr to Down) or progresses  to  a  terminal
+           state  (i.e.,  Point-to-Point, DR Other, Dr, or
+           Backup)."
+   ::= { ospfTraps 16 }
+
+
+    ospfVirtIfStateChange NOTIFICATION-TYPE
+        OBJECTS {
+                    ospfRouterId, -- The originator of the trap
+                    ospfVirtIfAreaId,
+                    ospfVirtIfNeighbor,
+                    ospfVirtIfState  -- The new state
+                  }
+        STATUS             current
+        DESCRIPTION
+           "An ospfIfStateChange trap signifies that there
+           has  been a change in the state of an OSPF vir-
+           tual interface.
+           This trap should be generated when  the  inter-
+           face  state  regresses  (e.g., goes from Point-
+           to-Point to Down) or progresses to  a  terminal
+           state (i.e., Point-to-Point)."
+   ::= { ospfTraps 1 }
+
+
+    ospfNbrStateChange NOTIFICATION-TYPE
+        OBJECTS {
+                    ospfRouterId, -- The originator of the trap
+                    ospfNbrIpAddr,
+                    ospfNbrAddressLessIndex,
+                    ospfNbrRtrId,
+                    ospfNbrState  -- The new state
+                  }
+        STATUS             current
+        DESCRIPTION
+           "An  ospfNbrStateChange  trap  signifies   that
+           there  has been a change in the state of a non-
+           virtual OSPF neighbor.   This  trap  should  be
+           generated  when  the  neighbor  state regresses
+           (e.g., goes from Attempt or Full  to  1-Way  or
+           Down)  or progresses to a terminal state (e.g.,
+           2-Way or Full).  When an  neighbor  transitions
+           from  or  to Full on non-broadcast multi-access
+           and broadcast networks, the trap should be gen-
+           erated  by the designated router.  A designated
+           router transitioning to Down will be  noted  by
+           ospfIfStateChange."
+   ::= { ospfTraps 2 }
+
+
+    ospfVirtNbrStateChange NOTIFICATION-TYPE
+        OBJECTS {
+                    ospfRouterId, -- The originator of the trap
+                    ospfVirtNbrArea,
+                    ospfVirtNbrRtrId,
+                    ospfVirtNbrState  -- The new state
+                  }
+        STATUS             current
+        DESCRIPTION
+           "An ospfIfStateChange trap signifies that there
+           has  been a change in the state of an OSPF vir-
+           tual neighbor.  This trap should  be  generated
+           when  the  neighbor state regresses (e.g., goes
+           from Attempt or  Full  to  1-Way  or  Down)  or
+           progresses to a terminal state (e.g., Full)."
+   ::= { ospfTraps 3 }
+    ospfIfConfigError NOTIFICATION-TYPE
+        OBJECTS {
+                    ospfRouterId, -- The originator of the trap
+                    ospfIfIpAddress,
+                    ospfAddressLessIf,
+                    ospfPacketSrc,  -- The source IP address
+                    ospfConfigErrorType, -- Type of error
+                    ospfPacketType
+                  }
+        STATUS             current
+        DESCRIPTION
+           "An ospfIfConfigError  trap  signifies  that  a
+           packet  has  been received on a non-virtual in-
+           terface  from  a  router  whose   configuration
+           parameters  conflict  with this router's confi-
+           guration parameters.  Note that the  event  op-
+           tionMismatch  should  cause  a  trap only if it
+           prevents an adjacency from forming."
+                  ::= { ospfTraps 4 }
+
+
+    ospfVirtIfConfigError NOTIFICATION-TYPE
+        OBJECTS {
+                    ospfRouterId, -- The originator of the trap
+                    ospfVirtIfAreaId,
+                    ospfVirtIfNeighbor,
+                    ospfConfigErrorType, -- Type of error
+                    ospfPacketType
+                  }
+        STATUS             current
+        DESCRIPTION
+           "An ospfConfigError trap signifies that a pack-
+           et  has  been  received  on a virtual interface
+           from a router  whose  configuration  parameters
+           conflict   with   this  router's  configuration
+           parameters.  Note that the event optionMismatch
+           should  cause a trap only if it prevents an ad-
+           jacency from forming."
+   ::= { ospfTraps 5 }
+
+
+    ospfIfAuthFailure NOTIFICATION-TYPE
+        OBJECTS {
+                    ospfRouterId, -- The originator of the trap
+                    ospfIfIpAddress,
+                    ospfAddressLessIf,
+                    ospfPacketSrc,  -- The source IP address
+                    ospfConfigErrorType, -- authTypeMismatch or
+                                         -- authFailure
+                    ospfPacketType
+                  }
+        STATUS             current
+        DESCRIPTION
+           "An ospfIfAuthFailure  trap  signifies  that  a
+           packet  has  been received on a non-virtual in-
+           terface from a router whose authentication  key
+           or  authentication  type  conflicts  with  this
+           router's authentication key  or  authentication
+           type."
+   ::= { ospfTraps 6 }
+
+
+    ospfVirtIfAuthFailure NOTIFICATION-TYPE
+        OBJECTS {
+                    ospfRouterId, -- The originator of the trap
+                    ospfVirtIfAreaId,
+                    ospfVirtIfNeighbor,
+                    ospfConfigErrorType, -- authTypeMismatch or
+                                         -- authFailure
+                    ospfPacketType
+                  }
+        STATUS             current
+        DESCRIPTION
+           "An ospfVirtIfAuthFailure trap signifies that a
+           packet has been received on a virtual interface
+           from a router whose authentication key  or  au-
+           thentication  type conflicts with this router's
+           authentication key or authentication type."
+   ::= { ospfTraps 7 }
+
+
+    ospfIfRxBadPacket NOTIFICATION-TYPE
+        OBJECTS {
+                    ospfRouterId, -- The originator of the trap
+                    ospfIfIpAddress,
+                    ospfAddressLessIf,
+                    ospfPacketSrc,  -- The source IP address
+                    ospfPacketType
+                  }
+        STATUS             current
+        DESCRIPTION
+           "An ospfIfRxBadPacket trap  signifies  that  an
+           OSPF  packet has been received on a non-virtual
+           interface that cannot be parsed."
+   ::= { ospfTraps 8 }
+
+    ospfVirtIfRxBadPacket NOTIFICATION-TYPE
+        OBJECTS {
+                    ospfRouterId, -- The originator of the trap
+                    ospfVirtIfAreaId,
+                    ospfVirtIfNeighbor,
+                    ospfPacketType
+                  }
+        STATUS             current
+        DESCRIPTION
+           "An ospfRxBadPacket trap signifies that an OSPF
+           packet has been received on a virtual interface
+           that cannot be parsed."
+   ::= { ospfTraps 9 }
+
+
+    ospfTxRetransmit NOTIFICATION-TYPE
+        OBJECTS {
+                    ospfRouterId, -- The originator of the trap
+                    ospfIfIpAddress,
+                    ospfAddressLessIf,
+                    ospfNbrRtrId, -- Destination
+                    ospfPacketType,
+                    ospfLsdbType,
+                    ospfLsdbLsid,
+                    ospfLsdbRouterId
+                  }
+        STATUS             current
+        DESCRIPTION
+           "An ospfTxRetransmit  trap  signifies  than  an
+           OSPF  packet  has  been retransmitted on a non-
+           virtual interface.  All packets that may be re-
+           transmitted  are associated with an LSDB entry.
+           The LS type, LS ID, and Router ID are  used  to
+           identify the LSDB entry."
+   ::= { ospfTraps 10 }
+
+
+    ospfVirtIfTxRetransmit NOTIFICATION-TYPE
+        OBJECTS {
+                    ospfRouterId, -- The originator of the trap
+                    ospfVirtIfAreaId,
+                    ospfVirtIfNeighbor,
+                    ospfPacketType,
+                    ospfLsdbType,
+                    ospfLsdbLsid,
+                    ospfLsdbRouterId
+                  }
+        STATUS             current
+        DESCRIPTION
+           "An ospfTxRetransmit  trap  signifies  than  an
+           OSPF packet has been retransmitted on a virtual
+           interface.  All packets that may be retransmit-
+           ted  are  associated with an LSDB entry. The LS
+           type, LS ID, and Router ID are used to identify
+           the LSDB entry."
+   ::= { ospfTraps 11 }
+
+
+    ospfOriginateLsa NOTIFICATION-TYPE
+        OBJECTS {
+                    ospfRouterId, -- The originator of the trap
+                    ospfLsdbAreaId,  -- 0.0.0.0 for AS Externals
+                    ospfLsdbType,
+                    ospfLsdbLsid,
+                    ospfLsdbRouterId
+                  }
+        STATUS             current
+        DESCRIPTION
+           "An ospfOriginateLsa trap signifies that a  new
+           LSA  has  been originated by this router.  This
+           trap should not be invoked for simple refreshes
+           of  LSAs  (which happesn every 30 minutes), but
+           instead will only be invoked  when  an  LSA  is
+           (re)originated due to a topology change.  Addi-
+           tionally, this trap does not include LSAs  that
+           are  being  flushed  because  they have reached
+           MaxAge."
+   ::= { ospfTraps 12 }
+
+
+    ospfMaxAgeLsa NOTIFICATION-TYPE
+        OBJECTS {
+                    ospfRouterId, -- The originator of the trap
+                    ospfLsdbAreaId,  -- 0.0.0.0 for AS Externals
+                    ospfLsdbType,
+                    ospfLsdbLsid,
+                    ospfLsdbRouterId
+                  }
+        STATUS             current
+        DESCRIPTION
+           "An ospfMaxAgeLsa trap signifies  that  one  of
+           the LSA in the router's link-state database has
+           aged to MaxAge."
+   ::= { ospfTraps 13 }
+
+
+    ospfLsdbOverflow NOTIFICATION-TYPE
+        OBJECTS {
+                    ospfRouterId, -- The originator of the trap
+                    ospfExtLsdbLimit
+                  }
+        STATUS             current
+        DESCRIPTION
+           "An ospfLsdbOverflow trap  signifies  that  the
+           number of LSAs in the router's link-state data-
+           base has exceeded ospfExtLsdbLimit."
+   ::= { ospfTraps 14 }
+
+
+    ospfLsdbApproachingOverflow NOTIFICATION-TYPE
+        OBJECTS {
+                    ospfRouterId, -- The originator of the trap
+                    ospfExtLsdbLimit
+                  }
+        STATUS             current
+        DESCRIPTION
+           "An ospfLsdbApproachingOverflow trap  signifies
+           that  the  number of LSAs in the router's link-
+           state database has exceeded ninety  percent  of
+           ospfExtLsdbLimit."
+   ::= { ospfTraps 15 }
+
+
+-- conformance information
+
+ospfTrapConformance OBJECT IDENTIFIER ::= { ospfTrap 3 }
+
+ospfTrapGroups      OBJECT IDENTIFIER ::= { ospfTrapConformance 1 }
+ospfTrapCompliances OBJECT IDENTIFIER ::= { ospfTrapConformance 2 }
+
+-- compliance statements
+
+    ospfTrapCompliance MODULE-COMPLIANCE
+        STATUS  current
+        DESCRIPTION
+           "The compliance statement "
+       MODULE  -- this module
+       MANDATORY-GROUPS { ospfTrapControlGroup }
+
+
+        GROUP       ospfTrapControlGroup
+        DESCRIPTION
+           "This group is optional but recommended for all
+           OSPF systems"
+       ::= { ospfTrapCompliances 1 }
+
+
+-- units of conformance
+
+    ospfTrapControlGroup    OBJECT-GROUP
+        OBJECTS {
+                           ospfSetTrap,
+                           ospfConfigErrorType,
+                           ospfPacketType,
+                           ospfPacketSrc
+        }
+        STATUS  current
+        DESCRIPTION
+           "These objects are required  to  control  traps
+           from OSPF systems."
+       ::= { ospfTrapGroups 1 }
+
+
+END
--- /dev/null
+++ b/mibs/RIPv2-MIB.txt
@@ -0,0 +1,530 @@
+   RIPv2-MIB DEFINITIONS ::= BEGIN
+
+   IMPORTS
+       MODULE-IDENTITY, OBJECT-TYPE, Counter32,
+       TimeTicks, IpAddress                     FROM SNMPv2-SMI
+       TEXTUAL-CONVENTION, RowStatus            FROM SNMPv2-TC
+       MODULE-COMPLIANCE, OBJECT-GROUP          FROM SNMPv2-CONF
+       mib-2                                    FROM RFC1213-MIB;
+
+   --  This MIB module uses the extended OBJECT-TYPE macro as
+   --  defined in [9].
+
+   rip2  MODULE-IDENTITY
+           LAST-UPDATED "9407272253Z"      -- Wed Jul 27 22:53:04 PDT 1994
+           ORGANIZATION "IETF RIP-II Working Group"
+           CONTACT-INFO
+          "       Fred Baker
+          Postal: Cisco Systems
+                  519 Lado Drive
+                  Santa Barbara, California 93111
+          Tel:    +1 805 681 0115
+          E-Mail: fbaker@cisco.com
+
+          Postal: Gary Malkin
+                  Xylogics, Inc.
+                  53 Third Avenue
+                  Burlington, MA  01803
+
+          Phone:  (617) 272-8140
+          EMail:  gmalkin@Xylogics.COM"
+      DESCRIPTION
+         "The MIB module to describe the RIP2 Version 2 Protocol"
+     ::= { mib-2 23 }
+
+ --  RIP-2 Management Information Base
+
+ -- the RouteTag type represents the contents of the
+ -- Route Domain field in the packet header or route entry.
+ -- The use of the Route Domain is deprecated.
+
+ RouteTag ::= TEXTUAL-CONVENTION
+     STATUS      current
+     DESCRIPTION
+        "the RouteTag type represents the contents of the Route Domain
+        field in the packet header or route entry"
+    SYNTAX      OCTET STRING (SIZE (2))
+
+--4.1 Global Counters
+
+--      The RIP-2 Globals Group.
+--      Implementation of this group is mandatory for systems
+--      which implement RIP-2.
+
+-- These counters are intended to facilitate debugging quickly
+-- changing routes or failing neighbors
+
+rip2Globals OBJECT IDENTIFIER ::= { rip2 1 }
+
+    rip2GlobalRouteChanges OBJECT-TYPE
+        SYNTAX   Counter32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The number of route changes made to the IP Route
+           Database by RIP.  This does not include the refresh
+           of a route's age."
+       ::= { rip2Globals 1 }
+
+    rip2GlobalQueries OBJECT-TYPE
+        SYNTAX   Counter32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The number of responses sent to RIP queries
+           from other systems."
+       ::= { rip2Globals 2 }
+
+--4.2 RIP Interface Tables
+
+--  RIP Interfaces Groups
+--  Implementation of these Groups is mandatory for systems
+--  which implement RIP-2.
+
+-- The RIP Interface Status Table.
+
+    rip2IfStatTable OBJECT-TYPE
+        SYNTAX   SEQUENCE OF Rip2IfStatEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "A list of subnets which require separate
+           status monitoring in RIP."
+       ::= { rip2 2 }
+
+   rip2IfStatEntry OBJECT-TYPE
+       SYNTAX   Rip2IfStatEntry
+       MAX-ACCESS   not-accessible
+       STATUS   current
+       DESCRIPTION
+          "A Single Routing Domain in a single Subnet."
+      INDEX { rip2IfStatAddress }
+      ::= { rip2IfStatTable 1 }
+
+    Rip2IfStatEntry ::=
+        SEQUENCE {
+            rip2IfStatAddress
+                IpAddress,
+            rip2IfStatRcvBadPackets
+                Counter32,
+            rip2IfStatRcvBadRoutes
+                Counter32,
+            rip2IfStatSentUpdates
+                Counter32,
+            rip2IfStatStatus
+                RowStatus
+    }
+
+    rip2IfStatAddress OBJECT-TYPE
+        SYNTAX   IpAddress
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The IP Address of this system on the indicated
+           subnet. For unnumbered interfaces, the value 0.0.0.N,
+           where the least significant 24 bits (N) is the ifIndex
+           for the IP Interface in network byte order."
+       ::= { rip2IfStatEntry 1 }
+
+    rip2IfStatRcvBadPackets OBJECT-TYPE
+        SYNTAX   Counter32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The number of RIP response packets received by
+           the RIP process which were subsequently discarded
+           for any reason (e.g. a version 0 packet, or an
+           unknown command type)."
+       ::= { rip2IfStatEntry 2 }
+
+    rip2IfStatRcvBadRoutes OBJECT-TYPE
+        SYNTAX   Counter32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The number of routes, in valid RIP packets,
+           which were ignored for any reason (e.g. unknown
+           address family, or invalid metric)."
+       ::= { rip2IfStatEntry 3 }
+
+    rip2IfStatSentUpdates OBJECT-TYPE
+        SYNTAX   Counter32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The number of triggered RIP updates actually
+           sent on this interface.  This explicitly does
+           NOT include full updates sent containing new
+           information."
+       ::= { rip2IfStatEntry 4 }
+
+    rip2IfStatStatus OBJECT-TYPE
+        SYNTAX   RowStatus
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "Writing invalid has the effect of deleting
+           this interface."
+       ::= { rip2IfStatEntry 5 }
+
+-- The RIP Interface Configuration Table.
+
+    rip2IfConfTable OBJECT-TYPE
+        SYNTAX   SEQUENCE OF Rip2IfConfEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "A list of subnets which require separate
+           configuration in RIP."
+       ::= { rip2 3 }
+
+   rip2IfConfEntry OBJECT-TYPE
+       SYNTAX   Rip2IfConfEntry
+       MAX-ACCESS   not-accessible
+       STATUS   current
+       DESCRIPTION
+          "A Single Routing Domain in a single Subnet."
+      INDEX { rip2IfConfAddress }
+      ::= { rip2IfConfTable 1 }
+
+    Rip2IfConfEntry ::=
+        SEQUENCE {
+            rip2IfConfAddress
+                IpAddress,
+            rip2IfConfDomain
+                RouteTag,
+            rip2IfConfAuthType
+                INTEGER,
+            rip2IfConfAuthKey
+                OCTET STRING (SIZE(0..16)),
+            rip2IfConfSend
+                INTEGER,
+            rip2IfConfReceive
+                INTEGER,
+            rip2IfConfDefaultMetric
+                INTEGER,
+            rip2IfConfStatus
+                RowStatus,
+            rip2IfConfSrcAddress
+                IpAddress
+    }
+
+    rip2IfConfAddress OBJECT-TYPE
+        SYNTAX   IpAddress
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The IP Address of this system on the indicated
+           subnet.  For unnumbered interfaces, the value 0.0.0.N,
+           where the least significant 24 bits (N) is the ifIndex
+           for the IP Interface in network byte order."
+       ::= { rip2IfConfEntry 1 }
+
+    rip2IfConfDomain OBJECT-TYPE
+        SYNTAX   RouteTag
+        MAX-ACCESS   read-create
+        STATUS   obsolete
+        DESCRIPTION
+           "Value inserted into the Routing Domain field
+           of all RIP packets sent on this interface."
+       DEFVAL { '0000'h }
+       ::= { rip2IfConfEntry 2 }
+
+    rip2IfConfAuthType OBJECT-TYPE
+        SYNTAX   INTEGER {
+                    noAuthentication (1),
+                    simplePassword (2),
+                    md5 (3)
+                 }
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The type of Authentication used on this
+           interface."
+       DEFVAL { noAuthentication }
+       ::= { rip2IfConfEntry 3 }
+
+    rip2IfConfAuthKey OBJECT-TYPE
+        SYNTAX   OCTET STRING (SIZE(0..16))
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The value to be used as the Authentication Key
+           whenever the corresponding instance of
+           rip2IfConfAuthType has a value other than
+           noAuthentication.  A modification of the corresponding
+           instance of rip2IfConfAuthType does not modify
+           the rip2IfConfAuthKey value.  If a string shorter
+           than 16 octets is supplied, it will be left-
+           justified and padded to 16 octets, on the right,
+           with nulls (0x00).
+
+           Reading this object always results in an  OCTET
+           STRING of length zero; authentication may not
+           be bypassed by reading the MIB object."
+       DEFVAL { ''h }
+       ::= { rip2IfConfEntry 4 }
+
+    rip2IfConfSend OBJECT-TYPE
+        SYNTAX   INTEGER {
+                    doNotSend (1),
+                    ripVersion1 (2),
+                    rip1Compatible (3),
+                    ripVersion2 (4),
+                    ripV1Demand (5),
+                    ripV2Demand (6)
+                 }
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "What the router sends on this interface.
+           ripVersion1 implies sending RIP updates compliant
+           with  RFC  1058.   rip1Compatible implies
+           broadcasting RIP-2 updates using RFC 1058 route
+           subsumption rules.  ripVersion2 implies
+           multicasting RIP-2 updates.  ripV1Demand indicates
+           the use of Demand RIP on a WAN interface under RIP
+           Version 1 rules.  ripV2Demand indicates the use of
+           Demand RIP on a WAN interface under Version 2 rules."
+       DEFVAL { rip1Compatible }
+       ::= { rip2IfConfEntry 5 }
+
+    rip2IfConfReceive OBJECT-TYPE
+        SYNTAX   INTEGER {
+                    rip1 (1),
+                    rip2 (2),
+                    rip1OrRip2 (3),
+                    doNotRecieve (4)
+                 }
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "This indicates which version of RIP updates
+           are to be accepted.  Note that rip2 and
+           rip1OrRip2 implies reception of multicast
+           packets."
+       DEFVAL { rip1OrRip2 }
+       ::= { rip2IfConfEntry 6 }
+
+    rip2IfConfDefaultMetric OBJECT-TYPE
+        SYNTAX   INTEGER ( 0..15 )
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "This variable indicates the metric that is to
+           be used for the default route entry in RIP updates
+           originated on this interface.  A value of zero
+           indicates that no default route should be
+           originated; in this case, a default route via
+           another router may be propagated."
+       ::= { rip2IfConfEntry 7 }
+
+    rip2IfConfStatus OBJECT-TYPE
+        SYNTAX   RowStatus
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "Writing invalid has  the  effect  of  deleting
+           this interface."
+       ::= { rip2IfConfEntry 8 }
+
+    rip2IfConfSrcAddress OBJECT-TYPE
+        SYNTAX   IpAddress
+        MAX-ACCESS   read-create
+        STATUS   current
+        DESCRIPTION
+           "The IP Address this system will use as a source
+            address on this interface.  If it is a numbered
+            interface, this MUST be the same value as
+            rip2IfConfAddress.  On unnumbered interfaces,
+            it must be the value of rip2IfConfAddress for
+            some interface on the system."
+       ::= { rip2IfConfEntry 9 }
+
+--4.3 Peer Table
+
+--  Peer Table
+
+--      The RIP Peer Group
+--      Implementation of this Group is Optional
+
+--      This group provides information about active peer
+--      relationships intended to assist in debugging.  An
+--      active peer is a router from which a valid RIP
+--      updated has been heard in the last 180 seconds.
+
+    rip2PeerTable OBJECT-TYPE
+        SYNTAX   SEQUENCE OF Rip2PeerEntry
+        MAX-ACCESS   not-accessible
+        STATUS   current
+        DESCRIPTION
+           "A list of RIP Peers."
+       ::= { rip2 4 }
+
+   rip2PeerEntry OBJECT-TYPE
+       SYNTAX   Rip2PeerEntry
+       MAX-ACCESS   not-accessible
+       STATUS   current
+       DESCRIPTION
+          "Information regarding a single routing peer."
+      INDEX { rip2PeerAddress, rip2PeerDomain }
+      ::= { rip2PeerTable 1 }
+
+    Rip2PeerEntry ::=
+        SEQUENCE {
+            rip2PeerAddress
+                IpAddress,
+            rip2PeerDomain
+                RouteTag,
+            rip2PeerLastUpdate
+                TimeTicks,
+            rip2PeerVersion
+                INTEGER,
+            rip2PeerRcvBadPackets
+                Counter32,
+            rip2PeerRcvBadRoutes
+                Counter32
+            }
+
+    rip2PeerAddress OBJECT-TYPE
+        SYNTAX   IpAddress
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The IP Address that the peer is using as its source
+            address.  Note that on an unnumbered link, this may
+            not be a member of any subnet on the system."
+       ::= { rip2PeerEntry 1 }
+
+    rip2PeerDomain OBJECT-TYPE
+        SYNTAX   RouteTag
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The value in the Routing Domain field  in  RIP
+           packets received from the peer.  As domain suuport
+           is deprecated, this must be zero."
+       ::= { rip2PeerEntry 2 }
+
+    rip2PeerLastUpdate OBJECT-TYPE
+        SYNTAX   TimeTicks
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The value of sysUpTime when the most recent
+           RIP update was received from this system."
+       ::= { rip2PeerEntry 3 }
+
+    rip2PeerVersion OBJECT-TYPE
+        SYNTAX   INTEGER ( 0..255 )
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The RIP version number in the header of the
+           last RIP packet received."
+       ::= { rip2PeerEntry 4 }
+
+    rip2PeerRcvBadPackets OBJECT-TYPE
+        SYNTAX   Counter32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The number of RIP response packets from this
+           peer discarded as invalid."
+       ::= { rip2PeerEntry 5 }
+
+
+    rip2PeerRcvBadRoutes OBJECT-TYPE
+        SYNTAX   Counter32
+        MAX-ACCESS   read-only
+        STATUS   current
+        DESCRIPTION
+           "The number of routes from this peer that were
+           ignored because the entry format was invalid."
+       ::= { rip2PeerEntry 6 }
+
+-- conformance information
+
+rip2Conformance OBJECT IDENTIFIER ::= { rip2 5 }
+
+rip2Groups      OBJECT IDENTIFIER ::= { rip2Conformance 1 }
+rip2Compliances OBJECT IDENTIFIER ::= { rip2Conformance 2 }
+
+-- compliance statements
+rip2Compliance MODULE-COMPLIANCE
+    STATUS  current
+    DESCRIPTION
+       "The compliance statement "
+    MODULE  -- this module
+    MANDATORY-GROUPS {
+                 rip2GlobalGroup,
+                 rip2IfStatGroup,
+                 rip2IfConfGroup,
+                 rip2PeerGroup
+        }
+    GROUP       rip2GlobalGroup
+    DESCRIPTION
+       "This group defines global controls for RIP-II systems."
+    GROUP       rip2IfStatGroup
+    DESCRIPTION
+       "This group defines interface statistics for RIP-II systems."
+    GROUP       rip2IfConfGroup
+    DESCRIPTION
+       "This group defines interface configuration for RIP-II systems."
+    GROUP       rip2PeerGroup
+    DESCRIPTION
+       "This group defines peer information for RIP-II systems."
+    ::= { rip2Compliances 1 }
+
+-- units of conformance
+
+rip2GlobalGroup    OBJECT-GROUP
+    OBJECTS {
+                rip2GlobalRouteChanges,
+                rip2GlobalQueries
+    }
+    STATUS  current
+    DESCRIPTION
+       "This group defines global controls for RIP-II systems."
+    ::= { rip2Groups 1 }
+rip2IfStatGroup    OBJECT-GROUP
+    OBJECTS {
+            rip2IfStatAddress,
+            rip2IfStatRcvBadPackets,
+            rip2IfStatRcvBadRoutes,
+            rip2IfStatSentUpdates,
+            rip2IfStatStatus
+    }
+    STATUS  current
+    DESCRIPTION
+       "This group defines interface statistics for RIP-II systems."
+    ::= { rip2Groups 2 }
+rip2IfConfGroup    OBJECT-GROUP
+    OBJECTS {
+            rip2IfConfAddress,
+            rip2IfConfAuthType,
+            rip2IfConfAuthKey,
+            rip2IfConfSend,
+            rip2IfConfReceive,
+            rip2IfConfDefaultMetric,
+            rip2IfConfStatus,
+            rip2IfConfSrcAddress
+    }
+    STATUS  current
+    DESCRIPTION
+       "This group defines interface configuration for RIP-II systems."
+    ::= { rip2Groups 3 }
+rip2PeerGroup    OBJECT-GROUP
+    OBJECTS {
+            rip2PeerAddress,
+            rip2PeerDomain,
+            rip2PeerLastUpdate,
+            rip2PeerVersion,
+            rip2PeerRcvBadPackets,
+            rip2PeerRcvBadRoutes
+    }
+    STATUS  current
+    DESCRIPTION
+       "This group defines peer information for RIP-II systems."
+    ::= { rip2Groups 4 }
+END
--- /dev/null
+++ b/mibs/SOURCE-ROUTING-MIB.txt
@@ -0,0 +1,452 @@
+SOURCE-ROUTING-MIB DEFINITIONS ::= BEGIN
+
+IMPORTS
+        Counter, Gauge
+                FROM RFC1155-SMI
+        dot1dBridge, dot1dSr
+                FROM BRIDGE-MIB
+        OBJECT-TYPE
+                FROM RFC-1212;
+
+-- groups in the SR MIB
+
+-- dot1dSr is imported from the Bridge MIB
+
+dot1dPortPair   OBJECT IDENTIFIER ::= { dot1dBridge 10 }
+
+-- the dot1dSr group
+
+-- this group is implemented by those bridges that
+-- support the source route bridging mode, including Source
+-- Routing and SRT bridges.
+
+dot1dSrPortTable OBJECT-TYPE
+    SYNTAX  SEQUENCE OF Dot1dSrPortEntry
+    ACCESS  not-accessible
+    STATUS  mandatory
+    DESCRIPTION
+            "A table that contains information about every
+            port that is associated with this source route
+            bridge."
+    ::= { dot1dSr 1 }
+
+dot1dSrPortEntry OBJECT-TYPE
+    SYNTAX  Dot1dSrPortEntry
+    ACCESS  not-accessible
+    STATUS  mandatory
+    DESCRIPTION
+            "A list of information for each port of a source
+            route bridge."
+    INDEX   { dot1dSrPort }
+
+    ::= { dot1dSrPortTable 1 }
+
+Dot1dSrPortEntry ::=
+    SEQUENCE {
+        dot1dSrPort
+            INTEGER,
+        dot1dSrPortHopCount
+            INTEGER,
+        dot1dSrPortLocalSegment
+            INTEGER,
+        dot1dSrPortBridgeNum
+            INTEGER,
+        dot1dSrPortTargetSegment
+            INTEGER,
+        dot1dSrPortLargestFrame
+            INTEGER,
+        dot1dSrPortSTESpanMode
+            INTEGER,
+        dot1dSrPortSpecInFrames
+            Counter,
+        dot1dSrPortSpecOutFrames
+            Counter,
+        dot1dSrPortApeInFrames
+            Counter,
+        dot1dSrPortApeOutFrames
+            Counter,
+        dot1dSrPortSteInFrames
+            Counter,
+        dot1dSrPortSteOutFrames
+            Counter,
+        dot1dSrPortSegmentMismatchDiscards
+            Counter,
+        dot1dSrPortDuplicateSegmentDiscards
+            Counter,
+        dot1dSrPortHopCountExceededDiscards
+            Counter,
+        dot1dSrPortDupLanIdOrTreeErrors
+            Counter,
+        dot1dSrPortLanIdMismatches
+            Counter
+    }
+
+dot1dSrPort OBJECT-TYPE
+    SYNTAX  INTEGER (1..65535)
+    ACCESS  read-only
+    STATUS  mandatory
+    DESCRIPTION
+            "The port number of the port for which this entry
+
+            contains Source Route management information."
+    ::= { dot1dSrPortEntry 1 }
+
+dot1dSrPortHopCount OBJECT-TYPE
+    SYNTAX  INTEGER
+    ACCESS  read-write
+    STATUS  mandatory
+    DESCRIPTION
+            "The maximum number of routing descriptors allowed
+            in an All Paths or Spanning Tree Explorer frames."
+    ::= { dot1dSrPortEntry 2 }
+
+dot1dSrPortLocalSegment OBJECT-TYPE
+    SYNTAX  INTEGER
+    ACCESS  read-write
+    STATUS  mandatory
+    DESCRIPTION
+            "The segment number that uniquely identifies the
+            segment to which this port is connected. Current
+            source routing protocols limit this value to the
+            range: 0 through 4095. (The value 0 is used by
+            some management applications for special test
+            cases.) A value of 65535 signifies that no segment
+            number is assigned to this port."
+    ::= { dot1dSrPortEntry 3 }
+
+dot1dSrPortBridgeNum OBJECT-TYPE
+    SYNTAX  INTEGER
+    ACCESS  read-write
+    STATUS  mandatory
+    DESCRIPTION
+            "A bridge number uniquely identifies a bridge when
+            more than one bridge is used to span the same two
+            segments.  Current source routing protocols limit
+            this value to the range: 0 through 15. A value of
+            65535 signifies that no bridge number is assigned
+            to this bridge."
+    ::= { dot1dSrPortEntry 4 }
+
+dot1dSrPortTargetSegment OBJECT-TYPE
+    SYNTAX  INTEGER
+    ACCESS  read-write
+    STATUS  mandatory
+    DESCRIPTION
+            "The segment number that corresponds to the target
+            segment this port is considered to be connected to
+            by the bridge.  Current source routing protocols
+            limit this value to the range: 0 through 4095.
+
+            (The value 0 is used by some management
+            applications for special test cases.) A value of
+            65535 signifies that no target segment is assigned
+            to this port."
+    ::= { dot1dSrPortEntry 5 }
+
+-- It would be nice if we could use ifMtu as the size of the
+-- largest frame, but we can't because ifMtu is defined to be
+-- the size that the (inter-)network layer can use which can
+-- differ from the MAC layer (especially if several layers of
+-- encapsulation are used).
+
+dot1dSrPortLargestFrame OBJECT-TYPE
+    SYNTAX  INTEGER
+    ACCESS  read-write
+    STATUS  mandatory
+    DESCRIPTION
+            "The maximum size of the INFO field (LLC and
+            above) that this port can send/receive.  It does
+            not include any MAC level (framing) octets.  The
+            value of this object is used by this bridge to
+            determine whether a modification of the
+            LargestFrame (LF, see [14]) field of the Routing
+            Control field of the Routing Information Field is
+            necessary.
+
+            64 valid values are defined by the IEEE 802.5M SRT
+            Addendum: 516, 635, 754, 873, 993, 1112, 1231,
+            1350, 1470, 1542, 1615, 1688, 1761, 1833, 1906,
+            1979, 2052, 2345, 2638, 2932, 3225, 3518, 3812,
+            4105, 4399, 4865, 5331, 5798, 6264, 6730, 7197,
+            7663, 8130, 8539, 8949, 9358, 9768, 10178, 10587,
+            10997, 11407, 12199, 12992, 13785, 14578, 15370,
+            16163, 16956, 17749, 20730, 23711, 26693, 29674,
+            32655, 35637, 38618, 41600, 44591, 47583, 50575,
+            53567, 56559, 59551, and 65535.
+
+            An illegal value will not be accepted by the
+            bridge."
+    ::= { dot1dSrPortEntry 6 }
+
+dot1dSrPortSTESpanMode OBJECT-TYPE
+    SYNTAX  INTEGER {
+                auto-span(1),
+                disabled(2),
+                forced(3)
+            }
+    ACCESS  read-write
+    STATUS  mandatory
+    DESCRIPTION
+            "Determines how this port behaves when presented
+            with a Spanning Tree Explorer frame.  The value
+            'disabled(2)' indicates that the port will not
+            accept or send Spanning Tree Explorer packets; any
+            STE packets received will be silently discarded.
+            The value 'forced(3)' indicates the port will
+            always accept and propagate Spanning Tree Explorer
+            frames.  This allows a manually configured
+            Spanning Tree for this class of packet to be
+            configured.  Note that unlike transparent
+            bridging, this is not catastrophic to the network
+            if there are loops.  The value 'auto-span(1)' can
+            only be returned by a bridge that both implements
+            the Spanning Tree Protocol and has use of the
+            protocol enabled on this port. The behavior of the
+            port for Spanning Tree Explorer frames is
+            determined by the state of dot1dStpPortState.  If
+            the port is in the 'forwarding' state, the frame
+            will be accepted or propagated.  Otherwise, it
+            will be silently discarded."
+    ::= { dot1dSrPortEntry 7 }
+
+dot1dSrPortSpecInFrames OBJECT-TYPE
+    SYNTAX  Counter
+    ACCESS  read-only
+    STATUS  mandatory
+    DESCRIPTION
+            "The number of Specifically Routed frames, also
+            referred to as Source Routed Frames, that have
+            been received from this port's segment."
+    ::= { dot1dSrPortEntry 8 }
+
+dot1dSrPortSpecOutFrames OBJECT-TYPE
+    SYNTAX  Counter
+    ACCESS  read-only
+    STATUS  mandatory
+    DESCRIPTION
+            "The number of Specifically Routed frames, also
+            referred to as Source Routed Frames, that this
+            port has transmitted on its segment."
+    ::= { dot1dSrPortEntry 9 }
+
+dot1dSrPortApeInFrames OBJECT-TYPE
+    SYNTAX  Counter
+    ACCESS  read-only
+    STATUS  mandatory
+    DESCRIPTION
+            "The number of All Paths Explorer frames, also
+            referred to as All Routes Explorer frames, that
+            have been received by this port from its segment."
+    ::= { dot1dSrPortEntry 10 }
+
+dot1dSrPortApeOutFrames OBJECT-TYPE
+    SYNTAX  Counter
+    ACCESS  read-only
+    STATUS  mandatory
+    DESCRIPTION
+            "The number of all Paths Explorer Frames, also
+            referred to as All Routes Explorer frames, that
+            have been transmitted by this port on its
+            segment."
+    ::= { dot1dSrPortEntry 11 }
+
+dot1dSrPortSteInFrames OBJECT-TYPE
+    SYNTAX  Counter
+    ACCESS  read-only
+    STATUS  mandatory
+    DESCRIPTION
+            "The number of spanning tree explorer frames that
+            have been received by this port from its segment."
+    ::= { dot1dSrPortEntry 12 }
+
+dot1dSrPortSteOutFrames OBJECT-TYPE
+    SYNTAX  Counter
+    ACCESS  read-only
+    STATUS  mandatory
+    DESCRIPTION
+            "The number of spanning tree explorer frames that
+            have been transmitted by this port on its
+            segment."
+    ::= { dot1dSrPortEntry 13 }
+
+dot1dSrPortSegmentMismatchDiscards OBJECT-TYPE
+    SYNTAX  Counter
+    ACCESS  read-only
+    STATUS  mandatory
+    DESCRIPTION
+            "The number of explorer frames that have been
+            discarded by this port because the routing
+            descriptor field contained an invalid adjacent
+            segment value."
+    ::= { dot1dSrPortEntry 14 }
+
+dot1dSrPortDuplicateSegmentDiscards OBJECT-TYPE
+    SYNTAX  Counter
+    ACCESS  read-only
+    STATUS  mandatory
+    DESCRIPTION
+            "The number of frames that have been discarded by
+            this port because the routing descriptor field
+            contained a duplicate segment identifier."
+    ::= { dot1dSrPortEntry 15 }
+
+dot1dSrPortHopCountExceededDiscards OBJECT-TYPE
+    SYNTAX  Counter
+    ACCESS  read-only
+    STATUS  mandatory
+    DESCRIPTION
+            "The number of explorer frames that have been
+            discarded by this port because the Routing
+            Information Field has exceeded the maximum route
+            descriptor length."
+    ::= { dot1dSrPortEntry 16 }
+
+dot1dSrPortDupLanIdOrTreeErrors OBJECT-TYPE
+    SYNTAX  Counter
+    ACCESS  read-only
+    STATUS  mandatory
+    DESCRIPTION
+            "The number of duplicate LAN IDs or Tree errors.
+            This helps in detection of problems in networks
+            containing older IBM Source Routing Bridges."
+    ::= { dot1dSrPortEntry 17 }
+
+dot1dSrPortLanIdMismatches OBJECT-TYPE
+    SYNTAX  Counter
+    ACCESS  read-only
+    STATUS  mandatory
+    DESCRIPTION
+            "The number of ARE and STE frames that were
+            discarded because the last LAN ID in the routing
+            information field did not equal the LAN-in ID.
+            This error can occur in implementations which do
+            only a LAN-in ID and Bridge Number check instead
+            of a LAN-in ID, Bridge Number, and LAN-out ID
+            check before they forward broadcast frames."
+    ::= { dot1dSrPortEntry 18 }
+
+-- scalar object in dot1dSr
+
+dot1dSrBridgeLfMode OBJECT-TYPE
+    SYNTAX  INTEGER {
+                mode3(1),
+                mode6(2)
+            }
+    ACCESS  read-write
+    STATUS  mandatory
+    DESCRIPTION
+            "Indicates whether the bridge operates using older
+            3 bit length negotiation fields or the newer 6 bit
+            length field in its RIF."
+    ::= { dot1dSr 2 }
+
+-- The Port-Pair Database
+
+-- Implementation of this group is optional.
+
+-- This group is implemented by those bridges that support
+-- the direct multiport model of the source route bridging
+-- mode as defined in the IEEE 802.5 SRT Addendum to
+-- 802.1d.
+
+-- Bridges implementing this group may report 65535 for
+-- dot1dSrPortBridgeNumber and dot1dSrPortTargetSegment,
+-- indicating that those objects are not applicable.
+
+dot1dPortPairTableSize OBJECT-TYPE
+    SYNTAX  Gauge
+    ACCESS  read-only
+    STATUS  mandatory
+    DESCRIPTION
+            "The total number of entries in the Bridge Port
+            Pair Database."
+    ::= { dot1dPortPair 1 }
+
+-- the Bridge Port-Pair table
+
+-- this table represents port pairs within a bridge forming
+-- a unique bridge path, as defined in the IEEE 802.5M SRT
+-- Addendum.
+
+dot1dPortPairTable OBJECT-TYPE
+    SYNTAX  SEQUENCE OF Dot1dPortPairEntry
+    ACCESS  not-accessible
+    STATUS  mandatory
+    DESCRIPTION
+            "A table that contains information about every
+
+            port pair database entity associated with this
+            source routing bridge."
+    ::= { dot1dPortPair 2 }
+
+dot1dPortPairEntry OBJECT-TYPE
+    SYNTAX  Dot1dPortPairEntry
+    ACCESS  not-accessible
+    STATUS  mandatory
+    DESCRIPTION
+            "A list of information for each port pair entity
+            of a bridge."
+    INDEX   { dot1dPortPairLowPort, dot1dPortPairHighPort }
+    ::= { dot1dPortPairTable 1 }
+
+Dot1dPortPairEntry ::=
+    SEQUENCE {
+        dot1dPortPairLowPort
+            INTEGER,
+        dot1dPortPairHighPort
+            INTEGER,
+        dot1dPortPairBridgeNum
+            INTEGER,
+        dot1dPortPairBridgeState
+            INTEGER
+    }
+
+dot1dPortPairLowPort OBJECT-TYPE
+    SYNTAX  INTEGER (1..65535)
+    ACCESS  read-write
+    STATUS  mandatory
+    DESCRIPTION
+            "The port number of the lower numbered port for
+            which this entry contains port pair database
+            information."
+    ::= { dot1dPortPairEntry 1 }
+
+dot1dPortPairHighPort OBJECT-TYPE
+    SYNTAX  INTEGER (1..65535)
+    ACCESS  read-write
+    STATUS  mandatory
+    DESCRIPTION
+            "The port number of the higher numbered port for
+            which this entry contains port pair database
+            information."
+    ::= { dot1dPortPairEntry 2 }
+
+dot1dPortPairBridgeNum OBJECT-TYPE
+    SYNTAX  INTEGER
+
+    ACCESS  read-write
+    STATUS  mandatory
+    DESCRIPTION
+            "A bridge number that uniquely identifies the path
+            provided by this source routing bridge between the
+            segments connected to dot1dPortPairLowPort and
+            dot1dPortPairHighPort.  The purpose of bridge
+            number is to disambiguate between multiple paths
+            connecting the same two LANs."
+    ::= { dot1dPortPairEntry 3 }
+
+dot1dPortPairBridgeState OBJECT-TYPE
+    SYNTAX  INTEGER {
+                enabled(1),
+                disabled(2),
+                invalid(3)
+            }
+    ACCESS  read-write
+    STATUS  mandatory
+    DESCRIPTION
+            "The state of dot1dPortPairBridgeNum.  Writing
+            'invalid(3)' to this object removes the
+            corresponding entry."
+    ::= { dot1dPortPairEntry 4 }
+
+END
