// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca956x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "tplink,eap245-v3", "qca,qca9563";
	model = "TP-Link EAP245 v3";

	aliases {
		led-boot = &led_status_green;
		led-failsafe = &led_status_amber;
		led-running = &led_status_green;
		led-upgrade = &led_status_amber;
		label-mac-device = &eth0;
	};

	leds {
		compatible = "gpio-leds";

		led_status_green: status_green {
			label = "green:status";
			gpios = <&gpio 7 GPIO_ACTIVE_HIGH>;
			default-state = "on";
		};

		led_status_amber: status_amber {
			label = "amber:status";
			gpios = <&gpio 9 GPIO_ACTIVE_HIGH>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};
};

&pcie {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "factory-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot";
				reg = <0x040000 0x040000>;
				read-only;
			};

			partition@80000 {
				label = "partition-table";
				reg = <0x080000 0x010000>;
				read-only;
			};

			info: partition@90000 {
				label = "info";
				reg = <0x090000 0x010000>;
				read-only;
			};

			art: partition@a0000 {
				label = "art";
				reg = <0x0a0000 0x010000>;
				read-only;
			};

			partition@b0000 {
				label = "extra-para";
				reg = <0x0b0000 0x010000>;
				read-only;
			};

			partition@c0000 {
				compatible = "openwrt,elf";
				label = "firmware";
				reg = <0x0c0000 0xe40000>;
			};

			partition@f00000 {
				label = "config";
				reg = <0xf00000 0x030000>;
				read-only;
			};

			partition@f30000 {
				label = "mutil-log";
				reg = <0xf30000 0x080000>;
				read-only;
			};

			partition@fb0000 {
				label = "oops";
				reg = <0xfb0000 0x040000>;
				read-only;
			};
		};
	};
};

&mdio0 {
	status = "okay";

	phy-mask = <0x1>;

	phy0: ethernet-phy@0 {
		reg = <0>;
		phy-mode = "sgmii";
		qca,ar8327-initvals = <
			0x04 0x00080080 /* PAD0 */
			0x7c 0x0000007e /* PORT0_STATUS */
			0xe0 0xc74164de /* SGMII_CTRL */
			>;
	};
};

&eth0 {
	status = "okay";

	phy-handle = <&phy0>;
	phy-mode = "sgmii";

	mtd-mac-address = <&info 0x8>;
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
	mtd-mac-address = <&info 0x8>;
};
