From: Johannes Berg <johannes.berg@intel.com>
Date: Fri, 9 Apr 2021 12:40:24 +0300
Subject: [PATCH] wireless: fix spelling of A-MSDU in HE capabilities

In the HE capabilities, spell A-MSDU correctly, not "A-MDSU".

Signed-off-by: Luca Coelho <luciano.coelho@intel.com>
Link: https://lore.kernel.org/r/iwlwifi.20210409123755.9e6ff1af1181.If6868bc6902ccd9a95c74c78f716c4b41473ef14@changeid
Signed-off-by: Johannes Berg <johannes.berg@intel.com>
---

--- a/drivers/net/wireless/intel/iwlwifi/iwl-nvm-parse.c
+++ b/drivers/net/wireless/intel/iwlwifi/iwl-nvm-parse.c
@@ -597,7 +597,7 @@ static struct ieee80211_sband_iftype_dat
 					IEEE80211_HE_MAC_CAP3_OMI_CONTROL |
 					IEEE80211_HE_MAC_CAP3_MAX_AMPDU_LEN_EXP_VHT_2,
 				.mac_cap_info[4] =
-					IEEE80211_HE_MAC_CAP4_AMDSU_IN_AMPDU |
+					IEEE80211_HE_MAC_CAP4_AMSDU_IN_AMPDU |
 					IEEE80211_HE_MAC_CAP4_MULTI_TID_AGG_TX_QOS_B39,
 				.mac_cap_info[5] =
 					IEEE80211_HE_MAC_CAP5_MULTI_TID_AGG_TX_QOS_B40 |
@@ -681,7 +681,7 @@ static struct ieee80211_sband_iftype_dat
 					IEEE80211_HE_MAC_CAP3_OMI_CONTROL |
 					IEEE80211_HE_MAC_CAP3_MAX_AMPDU_LEN_EXP_VHT_2,
 				.mac_cap_info[4] =
-					IEEE80211_HE_MAC_CAP4_AMDSU_IN_AMPDU,
+					IEEE80211_HE_MAC_CAP4_AMSDU_IN_AMPDU,
 				.mac_cap_info[5] =
 					IEEE80211_HE_MAC_CAP5_UL_2x996_TONE_RU,
 				.phy_cap_info[0] =
--- a/drivers/net/wireless/mediatek/mt76/mt7915/init.c
+++ b/drivers/net/wireless/mediatek/mt76/mt7915/init.c
@@ -427,7 +427,7 @@ mt7915_init_he_caps(struct mt7915_phy *p
 			IEEE80211_HE_MAC_CAP3_OMI_CONTROL |
 			IEEE80211_HE_MAC_CAP3_MAX_AMPDU_LEN_EXP_RESERVED;
 		he_cap_elem->mac_cap_info[4] =
-			IEEE80211_HE_MAC_CAP4_AMDSU_IN_AMPDU;
+			IEEE80211_HE_MAC_CAP4_AMSDU_IN_AMPDU;
 
 		if (band == NL80211_BAND_2GHZ)
 			he_cap_elem->phy_cap_info[0] =
--- a/drivers/net/wireless/mediatek/mt76/mt7915/mcu.c
+++ b/drivers/net/wireless/mediatek/mt76/mt7915/mcu.c
@@ -1358,7 +1358,7 @@ mt7915_mcu_sta_he_tlv(struct sk_buff *sk
 	if (elem->mac_cap_info[3] & IEEE80211_HE_MAC_CAP3_OMI_CONTROL)
 		cap |= STA_REC_HE_CAP_OM;
 
-	if (elem->mac_cap_info[4] & IEEE80211_HE_MAC_CAP4_AMDSU_IN_AMPDU)
+	if (elem->mac_cap_info[4] & IEEE80211_HE_MAC_CAP4_AMSDU_IN_AMPDU)
 		cap |= STA_REC_HE_CAP_AMSDU_IN_AMPDU;
 
 	if (elem->mac_cap_info[4] & IEEE80211_HE_MAC_CAP4_BQR)
--- a/include/linux/ieee80211.h
+++ b/include/linux/ieee80211.h
@@ -2068,7 +2068,7 @@ int ieee80211_get_vht_max_nss(struct iee
 #define IEEE80211_HE_MAC_CAP4_PSR_RESP				0x08
 #define IEEE80211_HE_MAC_CAP4_NDP_FB_REP			0x10
 #define IEEE80211_HE_MAC_CAP4_OPS				0x20
-#define IEEE80211_HE_MAC_CAP4_AMDSU_IN_AMPDU			0x40
+#define IEEE80211_HE_MAC_CAP4_AMSDU_IN_AMPDU			0x40
 /* Multi TID agg TX is split between byte #4 and #5
  * The value is a combination of B39,B40,B41
  */
--- a/net/mac80211/debugfs_sta.c
+++ b/net/mac80211/debugfs_sta.c
@@ -735,7 +735,7 @@ static ssize_t sta_he_capa_read(struct f
 	PFLAG(MAC, 4, PSR_RESP, "PSR-RESP");
 	PFLAG(MAC, 4, NDP_FB_REP, "NDP-FB-REP");
 	PFLAG(MAC, 4, OPS, "OPS");
-	PFLAG(MAC, 4, AMDSU_IN_AMPDU, "AMSDU-IN-AMPDU");
+	PFLAG(MAC, 4, AMSDU_IN_AMPDU, "AMSDU-IN-AMPDU");
 
 	PRINT("MULTI-TID-AGG-TX-QOS-%d", ((cap[5] << 1) | (cap[4] >> 7)) & 0x7);
 
--- a/drivers/net/wireless/mac80211_hwsim.c
+++ b/drivers/net/wireless/mac80211_hwsim.c
@@ -2764,7 +2764,7 @@ static const struct ieee80211_sband_ifty
 				.mac_cap_info[3] =
 					IEEE80211_HE_MAC_CAP3_OMI_CONTROL |
 					IEEE80211_HE_MAC_CAP3_MAX_AMPDU_LEN_EXP_VHT_2,
-				.mac_cap_info[4] = IEEE80211_HE_MAC_CAP4_AMDSU_IN_AMPDU,
+				.mac_cap_info[4] = IEEE80211_HE_MAC_CAP4_AMSDU_IN_AMPDU,
 				.phy_cap_info[1] =
 					IEEE80211_HE_PHY_CAP1_PREAMBLE_PUNC_RX_MASK |
 					IEEE80211_HE_PHY_CAP1_DEVICE_CLASS_A |
@@ -2808,7 +2808,7 @@ static const struct ieee80211_sband_ifty
 				.mac_cap_info[3] =
 					IEEE80211_HE_MAC_CAP3_OMI_CONTROL |
 					IEEE80211_HE_MAC_CAP3_MAX_AMPDU_LEN_EXP_VHT_2,
-				.mac_cap_info[4] = IEEE80211_HE_MAC_CAP4_AMDSU_IN_AMPDU,
+				.mac_cap_info[4] = IEEE80211_HE_MAC_CAP4_AMSDU_IN_AMPDU,
 				.phy_cap_info[1] =
 					IEEE80211_HE_PHY_CAP1_PREAMBLE_PUNC_RX_MASK |
 					IEEE80211_HE_PHY_CAP1_DEVICE_CLASS_A |
@@ -2854,7 +2854,7 @@ static const struct ieee80211_sband_ifty
 				.mac_cap_info[3] =
 					IEEE80211_HE_MAC_CAP3_OMI_CONTROL |
 					IEEE80211_HE_MAC_CAP3_MAX_AMPDU_LEN_EXP_VHT_2,
-				.mac_cap_info[4] = IEEE80211_HE_MAC_CAP4_AMDSU_IN_AMPDU,
+				.mac_cap_info[4] = IEEE80211_HE_MAC_CAP4_AMSDU_IN_AMPDU,
 				.phy_cap_info[0] =
 					IEEE80211_HE_PHY_CAP0_CHANNEL_WIDTH_SET_40MHZ_80MHZ_IN_5G |
 					IEEE80211_HE_PHY_CAP0_CHANNEL_WIDTH_SET_160MHZ_IN_5G |
@@ -2902,7 +2902,7 @@ static const struct ieee80211_sband_ifty
 				.mac_cap_info[3] =
 					IEEE80211_HE_MAC_CAP3_OMI_CONTROL |
 					IEEE80211_HE_MAC_CAP3_MAX_AMPDU_LEN_EXP_VHT_2,
-				.mac_cap_info[4] = IEEE80211_HE_MAC_CAP4_AMDSU_IN_AMPDU,
+				.mac_cap_info[4] = IEEE80211_HE_MAC_CAP4_AMSDU_IN_AMPDU,
 				.phy_cap_info[0] =
 					IEEE80211_HE_PHY_CAP0_CHANNEL_WIDTH_SET_40MHZ_80MHZ_IN_5G |
 					IEEE80211_HE_PHY_CAP0_CHANNEL_WIDTH_SET_160MHZ_IN_5G |
