From dbc2f62061c6bfba0aee93161ee3194dcee84bd0 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Fri, 29 Apr 2022 17:26:46 +0100
Subject: [PATCH] nvmem: core: support passing DT node in cell info
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Some hardware may have NVMEM cells described in Device Tree using
individual nodes. Let drivers pass such nodes to the NVMEM subsystem so
they can be later used by NVMEM consumers.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: Srinivas Kandagatla <srinivas.kandagatla@linaro.org>
Link: https://lore.kernel.org/r/20220429162701.2222-2-srinivas.kandagatla@linaro.org
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/nvmem/core.c           | 1 +
 include/linux/nvmem-consumer.h | 1 +
 2 files changed, 2 insertions(+)

--- a/drivers/nvmem/core.c
+++ b/drivers/nvmem/core.c
@@ -141,6 +141,7 @@ static int nvmem_cell_info_to_nvmem_cell
 
 	cell->bit_offset = info->bit_offset;
 	cell->nbits = info->nbits;
+	cell->np = info->np;
 
 	if (cell->nbits)
 		cell->bytes = DIV_ROUND_UP(cell->nbits + cell->bit_offset,
--- a/include/linux/nvmem-consumer.h
+++ b/include/linux/nvmem-consumer.h
@@ -25,6 +25,7 @@ struct nvmem_cell_info {
 	unsigned int		bytes;
 	unsigned int		bit_offset;
 	unsigned int		nbits;
+	struct device_node	*np;
 };
 
 /**
