From 38f8111369f318a538e9d4d89d8e48030c22fb40 Mon Sep 17 00:00:00 2001
From: Matthew Hagan <mnhagan88@gmail.com>
Date: Sun, 29 Aug 2021 22:37:49 +0000
Subject: [PATCH] ARM: dts: NSP: Fix MDIO mux node names

While functional, the mdio-mux-mmioreg binding does not conform to
Documentation/devicetree/bindings/net/mdio-mux-mmioreg.yaml in that an
mdio-mux compatible is also required. Without this the following output
is observed when running dtbs_check:

mdio-mux@32000: compatible: ['mdio-mux-mmioreg'] is too short

This change brings conformance to this requirement and corresponds
likewise to Rafal Milecki's change to the BCM5301x platform[1].

[1] https://lore.kernel.org/linux-arm-kernel/20210822191256.3715003-1-f.fainelli@gmail.com/T/

Signed-off-by: Matthew Hagan <mnhagan88@gmail.com>
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/bcm-nsp.dtsi                | 2 +-
 arch/arm/boot/dts/bcm958625-meraki-alamo.dtsi | 2 +-
 2 files changed, 2 insertions(+), 2 deletions(-)

--- a/arch/arm/boot/dts/bcm-nsp.dtsi
+++ b/arch/arm/boot/dts/bcm-nsp.dtsi
@@ -369,7 +369,7 @@
 		};
 
 		mdio-mux@32000 {
-			compatible = "mdio-mux-mmioreg";
+			compatible = "mdio-mux-mmioreg", "mdio-mux";
 			reg = <0x32000 0x4>;
 			mux-mask = <0x200>;
 			#address-cells = <1>;
--- a/arch/arm/boot/dts/bcm958625-meraki-alamo.dtsi
+++ b/arch/arm/boot/dts/bcm958625-meraki-alamo.dtsi
@@ -72,7 +72,7 @@
 	};
 
 	mdio-mii-mux {
-		compatible = "mdio-mux-mmioreg";
+		compatible = "mdio-mux-mmioreg", "mdio-mux";
 		reg = <0x1803f1c0 0x4>;
 		mux-mask = <0x2000>;
 		mdio-parent-bus = <&mdio_ext>;
