From 510fccc1a7533aa9f46d97ad500fe45ab7f91010 Mon Sep 17 00:00:00 2001
From: Jonathan Bell <jonathan@raspberrypi.org>
Date: Mon, 26 Oct 2020 14:03:35 +0000
Subject: [PATCH] xhci: quirks: add link TRB quirk for VL805

The VL805 controller can't cope with the TR Dequeue Pointer for an endpoint
being set to a Link TRB. The hardware-maintained endpoint context ends up
stuck at the address of the Link TRB, leading to erroneous ring expansion
events whenever the enqueue pointer wraps to the dequeue position.

If the search for the end of the current TD and ring cycle state lands on
a Link TRB, move to the next segment.

See: https://github.com/raspberrypi/linux/issues/3919

Signed-off-by: Jonathan Bell <jonathan@raspberrypi.com>
---
 drivers/usb/host/xhci-pci.c  |  1 +
 drivers/usb/host/xhci-ring.c | 10 ++++++++++
 drivers/usb/host/xhci.h      |  1 +
 3 files changed, 12 insertions(+)

--- a/drivers/usb/host/xhci-pci.c
+++ b/drivers/usb/host/xhci-pci.c
@@ -278,6 +278,7 @@ static void xhci_pci_quirks(struct devic
 			pdev->device == 0x3483) {
 		xhci->quirks |= XHCI_LPM_SUPPORT;
 		xhci->quirks |= XHCI_EP_CTX_BROKEN_DCS;
+		xhci->quirks |= XHCI_AVOID_DQ_ON_LINK;
 	}
 
 	if (pdev->vendor == PCI_VENDOR_ID_ASMEDIA &&
--- a/drivers/usb/host/xhci-ring.c
+++ b/drivers/usb/host/xhci-ring.c
@@ -660,6 +660,16 @@ void xhci_find_new_dequeue_state(struct
 
 	} while (!cycle_found || !td_last_trb_found);
 
+	/*
+	 * Quirk: the xHC does not correctly parse link TRBs if the HW Dequeue
+	 * pointer is set to one. Advance to the next TRB (and next segment).
+	 */
+	if (xhci->quirks & XHCI_AVOID_DQ_ON_LINK && trb_is_link(new_deq)) {
+		if (link_trb_toggles_cycle(new_deq))
+			state->new_cycle_state ^= 0x1;
+		next_trb(xhci, ep_ring, &new_seg, &new_deq);
+	}
+
 	state->new_deq_seg = new_seg;
 	state->new_deq_ptr = new_deq;
 
--- a/drivers/usb/host/xhci.h
+++ b/drivers/usb/host/xhci.h
@@ -1884,6 +1884,7 @@ struct xhci_hcd {
 #define XHCI_EP_CTX_BROKEN_DCS	BIT_ULL(36)
 #define XHCI_SKIP_PHY_INIT	BIT_ULL(37)
 #define XHCI_DISABLE_SPARSE	BIT_ULL(38)
+#define XHCI_AVOID_DQ_ON_LINK	BIT_ULL(39)
 #define XHCI_NO_SOFT_RETRY	BIT_ULL(40)
 
 	unsigned int		num_active_eps;
