#!/bin/sh

. /lib/functions/uci-defaults.sh

board_config_update

case "$(board_name)" in
dlink,dir-685)
	# These are all connected to eth0 thru RTL8366RB
	ucidef_set_interface "eth" device "eth0" protocol "none"
	ucidef_set_interfaces_lan_wan "lan0 lan1 lan2 lan3" "wan"
	;;
itian,sq201)
	# These are all connected to eth1 thru VSC7395
	ucidef_set_interface "eth" device "eth1" protocol "none"
	ucidef_set_interfaces_lan_wan "lan1 lan2 lan3 lan4" "eth0"
	;;
storlink,gemini324)
	# These are all connected to eth1 thru VSC7385
	ucidef_set_interface "eth" device "eth1" protocol "none"
	ucidef_set_interfaces_lan_wan "lan1 lan2 lan3 lan4" "eth0"
	;;
esac

board_config_flush

exit 0
