From 668ed11b1e8fbbe7ad9a63abbfece67d44b0aa85 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Thu, 25 Jun 2020 18:03:47 +0100
Subject: [PATCH] media: bcm2835-unicam: Add support for 14bit mono
 sources

Now that V4L2_PIX_FMT_Y14 and V4L2_PIX_FMT_Y14P are defined,
allow passing 14bit mono data through the peripheral.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/media/platform/bcm2835/bcm2835-unicam.c | 6 ++++++
 1 file changed, 6 insertions(+)

--- a/drivers/media/platform/bcm2835/bcm2835-unicam.c
+++ b/drivers/media/platform/bcm2835/bcm2835-unicam.c
@@ -341,6 +341,12 @@ static const struct unicam_fmt formats[]
 		.code		= MEDIA_BUS_FMT_Y12_1X12,
 		.depth		= 12,
 		.csi_dt		= 0x2c,
+	}, {
+		.fourcc		= V4L2_PIX_FMT_Y14P,
+		.repacked_fourcc = V4L2_PIX_FMT_Y14,
+		.code		= MEDIA_BUS_FMT_Y14_1X14,
+		.depth		= 14,
+		.csi_dt		= 0x2d,
 	},
 	/* Embedded data format */
 	{
