#include "mt7621_xiaomi_nand_128m.dtsi"

/ {
	compatible = "xiaomi,mi-router-3g", "mediatek,mt7621-soc";
	model = "Xiaomi Mi Router 3G";

	aliases {
		led-boot = &led_status_yellow;
		led-failsafe = &led_status_red;
		led-running = &led_status_blue;
		led-upgrade = &led_status_yellow;
		label-mac-device = &gmac0;
	};

	leds {
		compatible = "gpio-leds";

		led_status_red: status_red {
			label = "red:status";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};

		led_status_blue: status_blue {
			label = "blue:status";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};

		led_status_yellow: status_yellow {
			label = "yellow:status";
			gpios = <&gpio 10 GPIO_ACTIVE_LOW>;
		};

		wan_amber {
			label = "amber:wan";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "dsa-0.0:01:1Gbps";
		};

		lan1_amber {
			label = "amber:lan1";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "dsa-0.0:03:1Gbps";
		};

		lan2_amber {
			label = "amber:lan2";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "dsa-0.0:02:1Gbps";
		};
	};

	reg_usb_vbus: regulator {
		compatible = "regulator-fixed";
		regulator-name = "usb_vbus";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio 12 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};
};

&xhci {
	vbus-supply = <&reg_usb_vbus>;
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "pci14c3,7603";
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x0000>;
		ieee80211-freq-limit = <2400000 2500000>;
	};
};

&pcie1 {
	wifi@0,0 {
		compatible = "pci14c3,7662";
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x8000>;
		ieee80211-freq-limit = <5000000 6000000>;
	};
};

&gmac0 {
	mtd-mac-address = <&factory 0xe006>;
};

&switch0 {
	ports {
		port@1 {
			status = "okay";
			label = "wan";
			mtd-mac-address = <&factory 0xe000>;
		};

		port@2 {
			status = "okay";
			label = "lan2";
		};

		port@3 {
			status = "okay";
			label = "lan1";
		};
	};
};

&state_default {
	gpio {
		groups = "jtag", "uart2", "uart3", "wdt";
		function = "gpio";
	};
};
