--- a/arch/mips/bcm63xx/boards/board_bcm963xx.c
+++ b/arch/mips/bcm63xx/boards/board_bcm963xx.c
@@ -12,6 +12,7 @@
 #include <linux/init.h>
 #include <linux/kernel.h>
 #include <linux/string.h>
+#include <linux/pci_ids.h>
 #include <asm/addrspace.h>
 #include <bcm63xx_board.h>
 #include <bcm63xx_cpu.h>
@@ -1614,6 +1615,88 @@ static struct board_info __initdata boar
 	.has_ehci0 = 1,
 };
 
+static struct board_info __initdata board_CPVA642 = {
+	.name = "CPVA642",
+	.expected_cpu_id = 0x6358,
+
+	.has_pci = 1,
+	.has_ohci0 = 1,
+	.has_ehci0 = 1,
+
+	.has_enet1 = 1,
+	.enet1 = {
+		.has_phy = 1,
+		.phy_id = 0,
+		.force_speed_100 = 1,
+		.force_duplex_full = 1,
+ 	},
+};
+
+static struct board_info __initdata board_ct6373_1 = {
+	.name = "CT6373-1",
+	.expected_cpu_id = 0x6358,
+
+	.has_pci = 1,
+	.has_ohci0 = 1,
+	.has_ehci0 = 1,
+
+	.has_enet1 = 1,
+	.enet1 = {
+		.has_phy = 1,
+		.phy_id = 0,
+		.force_speed_100 = 1,
+		.force_duplex_full = 1,
+	},
+
+	.use_fallback_sprom = 1,
+	.fallback_sprom = {
+		.type = SPROM_BCM4318,
+		.pci_bus = 0,
+		.pci_dev = 1,
+	},
+};
+
+/* D-Link DSL-274xB revison C2/C3 */
+static struct board_info __initdata board_dsl_274xb_rev_c = {
+	.name = "AW4139",
+	.expected_cpu_id = 0x6358,
+
+	.has_pci = 1,
+
+	.has_enet1 = 1,
+	.enet1 = {
+		.has_phy = 1,
+		.phy_id = 0,
+		.force_speed_100 = 1,
+		.force_duplex_full = 1,
+	},
+};
+
+/* D-Link DVA-G3810BN/TL */
+static struct board_info __initdata board_DVAG3810BN = {
+	.name = "DVAG3810BN",
+	.expected_cpu_id = 0x6358,
+
+	.has_pccard = 1,
+	.has_pci = 1,
+	.has_ohci0 = 1,
+	.has_ehci0 = 1,
+
+	.has_enet0 = 1,
+	.enet0 = {
+		.has_phy = 1,
+		.use_internal_phy = 1,
+	},
+
+	.has_enet1 = 1,
+	.enet1 = {
+		.has_phy = 1,
+		.phy_id = 0,
+		.force_speed_100 = 1,
+		.force_duplex_full = 1,
+	},
+};
+
 static struct board_info __initdata board_DWVS0 = {
 	.name				= "DWV-S0",
 	.expected_cpu_id		= 0x6358,
@@ -1638,6 +1721,238 @@ static struct board_info __initdata boar
 	.has_ohci0			= 1,
 	.has_ehci0			= 1,
 };
+
+static struct board_info __initdata board_homehub2a = {
+	.name = "HOMEHUB2A",
+	.expected_cpu_id = 0x6358,
+
+	.has_pci = 1,
+	.has_ohci0 = 1,
+	.has_ehci0 = 1,
+	.num_usbh_ports = 2,
+
+	.has_enet1 = 1,
+	.enet1 = {
+		.has_phy = 1,
+		.phy_id = 0,
+		.force_speed_100 = 1,
+		.force_duplex_full = 1,
+	},
+
+	.use_fallback_sprom = 1,
+	.fallback_sprom = {
+		.type = SPROM_BCM4322,
+		.pci_bus = 0,
+		.pci_dev = 1,
+	},
+};
+
+static struct board_info __initdata board_HW520 = {
+	.name = "HW6358GW_B",
+	.expected_cpu_id = 0x6358,
+
+	.has_pci = 1,
+	.has_ohci0 = 1,
+	.has_ehci0 = 1,
+
+	.has_enet0 = 1,
+	.enet0 = {
+		.has_phy = 1,
+		.use_internal_phy = 1,
+	},
+
+	.has_enet1 = 1,
+	.enet1 = {
+		.has_phy = 1,
+		.phy_id = 0,
+		.force_speed_100 = 1,
+		.force_duplex_full = 1,
+	},
+
+	.use_fallback_sprom = 1,
+	.fallback_sprom = {
+		.type = SPROM_BCM4318,
+		.pci_bus = 0,
+		.pci_dev = 1,
+	},
+};
+
+static struct board_info __initdata board_HW553 = {
+	.name = "HW553",
+	.expected_cpu_id = 0x6358,
+
+	.has_pci = 1,
+	.has_ohci0 = 1,
+	.has_ehci0 = 1,
+	.num_usbh_ports = 2,
+
+	.has_enet1 = 1,
+	.enet1 = {
+		.has_phy = 1,
+		.phy_id = 0,
+		.force_speed_100 = 1,
+		.force_duplex_full = 1,
+	},
+
+	.use_fallback_sprom = 1,
+	.fallback_sprom = {
+		.type = SPROM_BCM4318,
+		.pci_bus = 0,
+		.pci_dev = 1,
+	},
+};
+
+static struct board_info __initdata board_HW556_A = {
+	.name = "HW556_A",
+	.expected_cpu_id = 0x6358,
+
+	.has_pci = 1,
+	.has_ohci0 = 1,
+	.has_ehci0 = 1,
+	.num_usbh_ports = 2,
+
+	.has_caldata = 1,
+	.caldata = {
+		{
+			.vendor = PCI_VENDOR_ID_ATHEROS,
+			.caldata_offset = 0xf7e000,
+			.slot = 1,
+			.endian_check = 1,
+			.led_pin = 2,
+			.led_active_high = 1,
+		},
+	},
+
+	.has_enet1 = 1,
+	.enet1 = {
+		.has_phy = 1,
+		.phy_id = 0,
+		.force_speed_100 = 1,
+		.force_duplex_full = 1,
+	},
+};
+
+static struct board_info __initdata board_HW556_B = {
+	.name = "HW556_B",
+	.expected_cpu_id = 0x6358,
+
+	.has_pci = 1,
+	.has_ohci0 = 1,
+	.has_ehci0 = 1,
+	.num_usbh_ports = 2,
+
+	.has_caldata = 1,
+	.caldata = {
+		{
+			.vendor = PCI_VENDOR_ID_ATHEROS,
+			.caldata_offset = 0xefe000,
+			.slot = 1,
+			.endian_check = 1,
+			.led_pin = 2,
+			.led_active_high = 1,
+		},
+	},
+
+	.has_enet1 = 1,
+	.enet1 = {
+		.has_phy = 1,
+		.phy_id = 0,
+		.force_speed_100 = 1,
+		.force_duplex_full = 1,
+	},
+};
+
+static struct board_info __initdata board_HW556_C = {
+	.name = "HW556_C",
+	.expected_cpu_id = 0x6358,
+
+	.has_pci = 1,
+	.has_ohci0 = 1,
+	.has_ehci0 = 1,
+	.num_usbh_ports = 2,
+
+	.has_caldata = 1,
+	.caldata = {
+		{
+			.vendor = PCI_VENDOR_ID_RALINK,
+			.caldata_offset = 0xeffe00,
+			.slot = 1,
+			.eeprom = "rt2x00.eeprom",
+		},
+	},
+
+	.has_enet1 = 1,
+	.enet1 = {
+		.has_phy = 1,
+		.phy_id = 0,
+		.force_speed_100 = 1,
+		.force_duplex_full = 1,
+	},
+};
+
+static struct board_info __initdata board_nb4_ser_r0 = {
+	.name = "NB4-SER-r0",
+	.expected_cpu_id = 0x6358,
+
+	.has_pccard = 1,
+	.has_pci = 1,
+	.has_ohci0 = 1,
+	.has_ehci0 = 1,
+	.num_usbh_ports = 2,
+
+	.has_enet0 = 1,
+	.enet0 = {
+		.has_phy = 1,
+		.use_internal_phy = 1,
+	},
+
+	.has_enet1 = 1,
+	.enet1 = {
+		.has_phy = 1,
+		.phy_id = 0,
+		.force_speed_100 = 1,
+		.force_duplex_full = 1,
+	},
+};
+
+static struct board_info __initdata board_nb4_fxc_r1 = {
+	.name = "NB4-FXC-r1",
+	.expected_cpu_id = 0x6358,
+
+	.has_pccard = 1,
+	.has_pci = 1,
+	.has_ohci0 = 1,
+	.has_ehci0 = 1,
+	.num_usbh_ports = 2,
+
+	.has_enet0 = 1,
+	.enet0 = {
+		.has_phy = 1,
+		.use_internal_phy = 1,
+	},
+
+	.has_enet1 = 1,
+	.enet1 = {
+		.has_phy = 1,
+		.phy_id = 0,
+		.force_speed_100 = 1,
+		.force_duplex_full = 1,
+	},
+};
+
+ /* T-Home Speedport W 303V Typ B */
+static struct board_info __initdata board_spw303v = {
+	.name = "96358-502V",
+	.expected_cpu_id = 0x6358,
+
+	.has_pci = 1,
+
+	.has_enet0 = 1,
+	.enet0 = {
+		.has_phy = 1,
+		.use_internal_phy = 1,
+	},
+};
 #endif /* CONFIG_BCM63XX_CPU_6358 */
 
 /*
@@ -1708,7 +2023,20 @@ static const struct board_info __initcon
 	&board_96358vw,
 	&board_96358vw2,
 	&board_AGPFS0,
+	&board_CPVA642,
+	&board_ct6373_1,
+	&board_dsl_274xb_rev_c,
+	&board_DVAG3810BN,
 	&board_DWVS0,
+	&board_homehub2a,
+	&board_HW520,
+	&board_HW553,
+	&board_HW556_A,
+	&board_HW556_B,
+	&board_HW556_C,
+	&board_nb4_ser_r0,
+	&board_nb4_fxc_r1,
+	&board_spw303v,
 #endif /* CONFIG_BCM63XX_CPU_6358 */
 };
 
@@ -1785,11 +2113,24 @@ static struct of_device_id const bcm963x
 	{ .compatible = "alcatel,rg100a", .data = &board_96358vw2, },
 	{ .compatible = "brcm,bcm96358vw", .data = &board_96358vw, },
 	{ .compatible = "brcm,bcm96358vw2", .data = &board_96358vw2, },
+	{ .compatible = "bt,home-hub-2-a", .data = &board_homehub2a, },
+	{ .compatible = "comtrend,ct-6373", .data = &board_ct6373_1, },
 	{ .compatible = "d-link,dsl-2650u", .data = &board_96358vw2, },
+	{ .compatible = "d-link,dsl-274xb-c2", .data = &board_dsl_274xb_rev_c, },
+	{ .compatible = "d-link,dva-g3810bn-tl", .data = &board_DVAG3810BN, },
+	{ .compatible = "huawei,echolife-hg520v", .data = &board_HW520, },
+	{ .compatible = "huawei,echolife-hg553", .data = &board_HW553, },
+	{ .compatible = "huawei,echolife-hg556a-a", .data = &board_HW556_A, },
+	{ .compatible = "huawei,echolife-hg556a-b", .data = &board_HW556_B, },
+	{ .compatible = "huawei,echolife-hg556a-c", .data = &board_HW556_C, },
 	{ .compatible = "pirelli,a226g", .data = &board_DWVS0, },
 	{ .compatible = "pirelli,a226m", .data = &board_DWVS0, },
 	{ .compatible = "pirelli,a226m-fwb", .data = &board_DWVS0, },
 	{ .compatible = "pirelli,agpf-s0", .data = &board_AGPFS0, },
+	{ .compatible = "sfr,neufbox-4-sercomm-r0", .data = &board_nb4_ser_r0, },
+	{ .compatible = "sfr,neufbox-4-foxconn-r1", .data = &board_nb4_fxc_r1, },
+	{ .compatible = "t-com,speedport-w-303v", .data = &board_spw303v, },
+	{ .compatible = "telsey,cpva642", .data = &board_CPVA642, },
 #endif /* CONFIG_BCM63XX_CPU_6358 */
 #ifdef CONFIG_BCM63XX_CPU_6362
 #endif /* CONFIG_BCM63XX_CPU_6362 */
