From b7c3fda0df5da90e87b037348c6d27f669c38388 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Mon, 13 Feb 2017 17:20:08 +0000
Subject: [PATCH] clk-bcm2835: Add claim-clocks property

The claim-clocks property can be used to prevent PLLs and dividers
from being marked as critical. It contains a vector of clock IDs,
as defined by dt-bindings/clock/bcm2835.h.

Use this mechanism to claim PLLD_DSI0, PLLD_DSI1, PLLH_AUX and
PLLH_PIX for the vc4_kms_v3d driver.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 drivers/clk/bcm/clk-bcm2835.c | 34 ++++++++++++++++++++++++++++++++--
 1 file changed, 32 insertions(+), 2 deletions(-)

--- a/drivers/clk/bcm/clk-bcm2835.c
+++ b/drivers/clk/bcm/clk-bcm2835.c
@@ -1311,6 +1311,8 @@ static const struct clk_ops bcm2835_vpu_
 	.debug_init = bcm2835_clock_debug_init,
 };
 
+static bool bcm2835_clk_is_claimed(const char *name);
+
 static struct clk_hw *bcm2835_register_pll(struct bcm2835_cprman *cprman,
 					   const struct bcm2835_pll_data *data)
 {
@@ -1327,6 +1329,9 @@ static struct clk_hw *bcm2835_register_p
 	init.ops = &bcm2835_pll_clk_ops;
 	init.flags = CLK_IGNORE_UNUSED;
 
+	if (!bcm2835_clk_is_claimed(data->name))
+		init.flags |= CLK_IS_CRITICAL;
+
 	pll = kzalloc(sizeof(*pll), GFP_KERNEL);
 	if (!pll)
 		return NULL;
@@ -1382,8 +1387,10 @@ bcm2835_register_pll_divider(struct bcm2
 	divider->div.table = NULL;
 
 	if (!(cprman_read(cprman, data->cm_reg) & data->hold_mask)) {
-		init.flags |= CLK_IS_CRITICAL;
-		divider->div.flags |= CLK_IS_CRITICAL;
+		if (!bcm2835_clk_is_claimed(data->source_pll))
+			init.flags |= CLK_IS_CRITICAL;
+		if (!bcm2835_clk_is_claimed(data->name))
+			divider->div.flags |= CLK_IS_CRITICAL;
 	}
 
 	divider->cprman = cprman;
@@ -2191,6 +2198,8 @@ static const struct bcm2835_clk_desc clk
 		.ctl_reg = CM_PERIICTL),
 };
 
+static bool bcm2835_clk_claimed[ARRAY_SIZE(clk_desc_array)];
+
 /*
  * Permanently take a reference on the parent of the SDRAM clock.
  *
@@ -2210,6 +2219,19 @@ static int bcm2835_mark_sdc_parent_criti
 	return clk_prepare_enable(parent);
 }
 
+static bool bcm2835_clk_is_claimed(const char *name)
+{
+	int i;
+
+	for (i = 0; i < ARRAY_SIZE(clk_desc_array); i++) {
+		const char *clk_name = *(const char **)(clk_desc_array[i].data);
+		if (!strcmp(name, clk_name))
+		    return bcm2835_clk_claimed[i];
+	}
+
+	return false;
+}
+
 static int bcm2835_clk_probe(struct platform_device *pdev)
 {
 	struct device *dev = &pdev->dev;
@@ -2220,6 +2242,7 @@ static int bcm2835_clk_probe(struct plat
 	const size_t asize = ARRAY_SIZE(clk_desc_array);
 	const struct cprman_plat_data *pdata;
 	size_t i;
+	u32 clk_id;
 	int ret;
 
 	pdata = of_device_get_match_data(&pdev->dev);
@@ -2239,6 +2262,13 @@ static int bcm2835_clk_probe(struct plat
 	if (IS_ERR(cprman->regs))
 		return PTR_ERR(cprman->regs);
 
+	memset(bcm2835_clk_claimed, 0, sizeof(bcm2835_clk_claimed));
+	for (i = 0;
+	     !of_property_read_u32_index(pdev->dev.of_node, "claim-clocks",
+					 i, &clk_id);
+	     i++)
+		bcm2835_clk_claimed[clk_id]= true;
+
 	memcpy(cprman->real_parent_names, cprman_parent_names,
 	       sizeof(cprman_parent_names));
 	of_clk_parent_fill(dev->of_node, cprman->real_parent_names,
