From b1a4a23406727f112b9a296b0231ec4d1b99d6e0 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.org>
Date: Wed, 31 Oct 2018 14:57:56 +0000
Subject: [PATCH] media: adv7180: Add YPrPb support for ADV7282M

The ADV7282M can support YPbPr on AIN1-3, but this was
not selectable from the driver. Add it to the list of
supported input modes.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.org>
---
 drivers/media/i2c/adv7180.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/media/i2c/adv7180.c
+++ b/drivers/media/i2c/adv7180.c
@@ -1235,6 +1235,7 @@ static const struct adv7180_chip_info ad
 		BIT(ADV7182_INPUT_SVIDEO_AIN1_AIN2) |
 		BIT(ADV7182_INPUT_SVIDEO_AIN3_AIN4) |
 		BIT(ADV7182_INPUT_SVIDEO_AIN7_AIN8) |
+		BIT(ADV7182_INPUT_YPRPB_AIN1_AIN2_AIN3) |
 		BIT(ADV7182_INPUT_DIFF_CVBS_AIN1_AIN2) |
 		BIT(ADV7182_INPUT_DIFF_CVBS_AIN3_AIN4) |
 		BIT(ADV7182_INPUT_DIFF_CVBS_AIN7_AIN8),
