// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar9344.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	model = "Western Digital My Net Wi-Fi Range Extender";
	compatible = "wd,mynet-wifi-rangeextender", "qca,ar9344";

	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "blue:power";
			gpios = <&gpio 11 GPIO_ACTIVE_HIGH>;
			/* LED has no off state. It's either on or it blinks */
		};

		lan {
			label = "green:lan";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};

		wifi {
			label = "blue:wifi";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wifi-rssi-low {
			label = "blue:rssi-low";
			gpios = <&gpio 20 GPIO_ACTIVE_LOW>;
		};

		wifi-rssi-med {
			label = "blue:rssi-med";
			gpios = <&gpio 21 GPIO_ACTIVE_LOW>;
		};

		wifi-rssi-max {
			label = "blue:rssi-max";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};

		band-switch {
			linux,code = <BTN_1>;
			gpios = <&gpio 14 GPIO_ACTIVE_HIGH>;
			linux,input-type = <EV_SW>;
		};

		wps {
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};
	};
};

&ref {
	clock-frequency = <25000000>;
};

&uart {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = /* "s25fl064k", */ "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot: partition@0 {
				label = "u-boot";
				reg = <0x0 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "firmware";
				reg = <0x40000 0x7a0000>;
				compatible = "cybertan,trx";
			};

			nvram: partition@7e0000 {
				label = "nvram";
				reg = <0x7e0000 0x10000>;
			};

			art: partition@7f0000 {
				label = "art";
				reg = <0x7f0000 0x10000>;
				read-only;
			};
		};
	};
};

&pcie {
	status = "okay";

	ath9k: wifi@0,0 {
		compatible = "pci168c,0030";
		reg = <0x0000 0 0 0 0>;
		qca,no-eeprom;
		/* wifi MAC is stored in nvram */
	};
};

&mdio0 {
	status = "okay";

	phy-mask = <0x10>;

	phy4: ethernet-phy@4 {
		reg = <4>;
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x0e000000 0x3c000101 0x3c001313>;

	/* ethernet MAC is stored in nvram */
	phy-mode = "rgmii";
	phy-handle = <&phy4>;

	gmac-config {
		device = <&gmac>;
		rgmii-gmac0 = <1>;
		rxd-delay = <3>;
		rxdv-delay = <3>;
	};
};

&mdio1 {
	status = "disabled";
};
