// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar9331.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	model = "Hak5 WiFi Pineapple NANO";
	compatible = "hak5,wifi-pineapple-nano", "qca,ar9331";

	aliases {
		label-mac-device = &wmac;
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-upgrade = &led_system;
		serial0 = &uart;
	};

	gpio-export {
		compatible = "gpio-export";
		#size-cells = <0>;

		microsd-detect {
			gpio-export,name = "microsd-detect";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
		};

		usb-alarm {
			gpio-export,name = "usb-alarm";
			gpios = <&gpio 20 GPIO_ACTIVE_LOW>;
		};

		usb-power {
			gpio-export,name = "usb-power";
			gpio-export,output = <0>;
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_system: system {
			label = "blue:system";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};
};

&eth0 {
	status = "okay";

	mtd-mac-address = <&art 0x6>;
};

&eth1 {
	status = "okay";

	compatible = "syscon", "simple-mfd";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;
		m25p,fast-read;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x020000>;
				read-only;
			};

			partition@20000 {
				label = "firmware";
				reg = <0x020000 0xfd0000>;
				compatible = "tplink,firmware";
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;
			};
		};
	};
};

&uart {
	status = "okay";
};

&usb {
	status = "okay";
};

&usb_phy {
	status = "okay";
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
};
