#include "mt7628an.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "d-team,pbr-d1", "mediatek,mt7628an-soc";
	model = "PBR-D1";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	aliases {
		serial0 = &uart2;
	};

	leds {
		compatible = "gpio-leds";

		usb {
			label = "orange:usb";
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
			trigger-sources = <&ohci_port1>, <&ehci_port1>;
			linux,default-trigger = "usbport";
		};

		led_power: power {
			label = "orange:power";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 70 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	wgpio: gpio-wifi {
		compatible = "mediatek,gpio-wifi";
		#address-cells = <1>;
		#size-cells = <0>;
		gpio-controller;
		#gpio-cells = <2>;
	};
};

&state_default {
	gpio {
		groups = "gpio";
		function = "gpio";
	};

	i2c {
		groups = "i2c";
		function = "gpio";
	};

	i2s {
		groups = "i2s";
		function = "gpio";
	};

	spis {
		groups = "spis";
		function = "gpio";
	};

	wdt {
		groups = "wdt";
		function = "gpio";
	};
};

&spi0 {
	status = "okay";

	pinctrl-names = "default";
	pinctrl-0 = <&spi_pins>, <&spi_cs1_pins>;

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <40000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x0fb0000>;
			};
		};
	};

	spidev@1 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "linux,spidev";
		reg = <1>;
		spi-max-frequency = <40000000>;
	};
};

&i2c {
	status = "okay";
};

&uart1 {
	status = "okay";
};

&uart2 {
	status = "okay";
};

&pwm {
	status = "okay";
};

&ethernet {
	mtd-mac-address = <&factory 0x28>;
};

&sdhci {
	status = "okay";
	mediatek,cd-high;
};
