From: MarkLee <Mark-MC.Lee@mediatek.com>
Date: Wed, 13 Nov 2019 10:38:42 +0800
Subject: [PATCH] net: ethernet: mediatek: Integrate GDM/PSE setup operations

Integrate GDM/PSE setup operations into single function "mtk_gdm_config"

Signed-off-by: MarkLee <Mark-MC.Lee@mediatek.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -2211,6 +2211,28 @@ static int mtk_start_dma(struct mtk_eth
 	return 0;
 }
 
+static void mtk_gdm_config(struct mtk_eth *eth, u32 config)
+{
+	int i;
+
+	for (i = 0; i < MTK_MAC_COUNT; i++) {
+		u32 val = mtk_r32(eth, MTK_GDMA_FWD_CFG(i));
+
+		/* default setup the forward port to send frame to PDMA */
+		val &= ~0xffff;
+
+		/* Enable RX checksum */
+		val |= MTK_GDMA_ICS_EN | MTK_GDMA_TCS_EN | MTK_GDMA_UCS_EN;
+
+		val |= config;
+
+		mtk_w32(eth, val, MTK_GDMA_FWD_CFG(i));
+	}
+	/* Reset and enable PSE */
+	mtk_w32(eth, RST_GL_PSE, MTK_RST_GL);
+	mtk_w32(eth, 0, MTK_RST_GL);
+}
+
 static int mtk_open(struct net_device *dev)
 {
 	struct mtk_mac *mac = netdev_priv(dev);
@@ -2406,8 +2428,6 @@ static int mtk_hw_init(struct mtk_eth *e
 	mtk_w32(eth, 0, MTK_QDMA_DELAY_INT);
 	mtk_tx_irq_disable(eth, ~0);
 	mtk_rx_irq_disable(eth, ~0);
-	mtk_w32(eth, RST_GL_PSE, MTK_RST_GL);
-	mtk_w32(eth, 0, MTK_RST_GL);
 
 	/* FE int grouping */
 	mtk_w32(eth, MTK_TX_DONE_INT, MTK_PDMA_INT_GRP1);
@@ -2416,18 +2436,7 @@ static int mtk_hw_init(struct mtk_eth *e
 	mtk_w32(eth, MTK_RX_DONE_INT, MTK_QDMA_INT_GRP2);
 	mtk_w32(eth, 0x21021000, MTK_FE_INT_GRP);
 
-	for (i = 0; i < MTK_MAC_COUNT; i++) {
-		u32 val = mtk_r32(eth, MTK_GDMA_FWD_CFG(i));
-
-		/* setup the forward port to send frame to PDMA */
-		val &= ~0xffff;
-
-		/* Enable RX checksum */
-		val |= MTK_GDMA_ICS_EN | MTK_GDMA_TCS_EN | MTK_GDMA_UCS_EN;
-
-		/* setup the mac dma */
-		mtk_w32(eth, val, MTK_GDMA_FWD_CFG(i));
-	}
+	mtk_gdm_config(eth, MTK_GDMA_TO_PDMA);
 
 	return 0;
 
--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.h
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.h
@@ -84,6 +84,7 @@
 #define MTK_GDMA_ICS_EN		BIT(22)
 #define MTK_GDMA_TCS_EN		BIT(21)
 #define MTK_GDMA_UCS_EN		BIT(20)
+#define MTK_GDMA_TO_PDMA	0x0
 
 /* Unicast Filter MAC Address Register - Low */
 #define MTK_GDMA_MAC_ADRL(x)	(0x508 + (x * 0x1000))
