#include "rt2880.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "airlink101,ar670w", "ralink,rt2880-soc";
	model = "Airlink101 AR670W";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	flash@bdc00000 {
		compatible = "cfi-flash";
		reg = <0xbc400000 0x800000>;
		bank-width = <2>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				reg = <0x0 0x30000>;
				label = "u-boot";
				read-only;
			};

			factory: partition@30000 {
				reg = <0x30000 0x10000>;
				label = "factory";
				read-only;
			};

			partition@40000 {
				compatible = "lzma";
				reg = <0x40000 0x3c0000>;
				label = "firmware";
			};
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "green:power";
			gpios = <&gpio0 7 GPIO_ACTIVE_LOW>;
		};

		wpsblue {
			label = "blue:wps";
			gpios = <&gpio0 13 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		wps {
			label = "wps";
			gpios = <&gpio0 0 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		reset {
			label = "reset";
			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};
};

&state_default {
	gpio {
		groups = "i2c", "spi", "uartlite";
		function = "gpio";
	};
};

&ethernet {
	status = "okay";
	mtd-mac-address = <&factory 0x2004>;

	port@0 {
		phy-handle = <&phy0>;
		phy-mode = "mii";
	};

	mdio-bus {
		status = "okay";

		phy0: ethernet-phy@0 {
			phy-mode = "mii";
			reg = <0>;
		};
	};
};

&wmac {
	status = "okay";
	ralink,mtd-eeprom = <&factory 0x2000>;
};
