From 65318cd76f4523acf8ffe8fe7448fb7d913f8c66 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Tue, 3 Mar 2020 09:43:41 +0000
Subject: [PATCH] overlays: sc16ic750-i2c: Fix xtal parameter

The xtal parameter is targetting the wrong node - fix it.

See: https://github.com/raspberrypi/linux/issues/3156

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 arch/arm/boot/dts/overlays/sc16is750-i2c-overlay.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/overlays/sc16is750-i2c-overlay.dts
+++ b/arch/arm/boot/dts/overlays/sc16is750-i2c-overlay.dts
@@ -32,7 +32,7 @@
 	__overrides__ {
 		int_pin = <&sc16is750>,"interrupts:0";
 		addr = <&sc16is750>,"reg:0",<&sc16is750_clk>,"name";
-		xtal = <&sc16is750>,"clock-frequency:0";
+		xtal = <&sc16is750_clk>,"clock-frequency:0";
 	};
 
 };
