From bed63eea982ba6d59995288a5deab94510a51994 Mon Sep 17 00:00:00 2001
From: Shengjiu Wang <shengjiu.wang@nxp.com>
Date: Tue, 6 Mar 2018 11:45:30 +0800
Subject: [PATCH] MLK-17156-1: ASoC: fsl_sai: update register offset for ULP B0

ULP B0 integrate the latest SAI IP, there is version id and
parameter id register in the beginning, so update the offset
for ULP B0

Signed-off-by: Shengjiu Wang <shengjiu.wang@nxp.com>
Reviewed-by: Daniel Baluta <daniel.baluta@nxp.com>
---
 sound/soc/fsl/fsl_sai.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/sound/soc/fsl/fsl_sai.c
+++ b/sound/soc/fsl/fsl_sai.c
@@ -64,7 +64,7 @@ static struct fsl_sai_soc_data fsl_sai_i
 	.fifos = 2,
 	.fifo_depth = 16,
 	.flags = SAI_FLAG_PMQOS,
-	.reg_offset = 0,
+	.reg_offset = 8,
 	.constrain_period_size = false,
 };
 
