From: Christian Marangi <ansuelsmth@gmail.com>
Subject: kernel/mtd: add support for EON EN25QX128A

Add support for EON EN25QX128A with no flags as it does
support SFDP parsing.

Signed-off-by: Christian Marangi <ansuelsmth@gmail.com>
---
 drivers/mtd/spi-nor/spi-nor.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/mtd/spi-nor/spi-nor.c
+++ b/drivers/mtd/spi-nor/spi-nor.c
@@ -2180,6 +2180,7 @@ static const struct flash_info spi_nor_i
 	{ "en25p64",    INFO(0x1c2017, 0, 64 * 1024,  128, 0) },
 	{ "en25q64",    INFO(0x1c3017, 0, 64 * 1024,  128, SECT_4K) },
 	{ "en25q128",   INFO(0x1c3018, 0, 64 * 1024,  256, SECT_4K) },
+	{ "en25qx128a", INFO(0x1c7118, 0, 64 * 1024, 256, 0) },
 	{ "en25q80a",   INFO(0x1c3014, 0, 64 * 1024,   16,
 			SECT_4K | SPI_NOR_DUAL_READ) },
 	{ "en25qh32",   INFO(0x1c7016, 0, 64 * 1024,   64, 0) },
