From 0cbec9aef5a86194117a956546dc1aec95031f37 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?=C3=81lvaro=20Fern=C3=A1ndez=20Rojas?= <noltari@gmail.com>
Date: Sat, 14 Jun 2025 09:59:50 +0200
Subject: [PATCH] net: dsa: b53: detect BCM5325 variants
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

We need to be able to differentiate the BCM5325 variants because:
- BCM5325M switches lack the ARLIO_PAGE->VLAN_ID_IDX register.
- BCM5325E have less 512 ARL buckets instead of 1024.

Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
Reviewed-by: Florian Fainelli <florian.fainelli@broadcom.com>
Link: https://patch.msgid.link/20250614080000.1884236-5-noltari@gmail.com
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/dsa/b53/b53_common.c | 24 +++++++++++++++++++++---
 drivers/net/dsa/b53/b53_priv.h   | 19 +++++++++++++++++++
 2 files changed, 40 insertions(+), 3 deletions(-)

--- a/drivers/net/dsa/b53/b53_common.c
+++ b/drivers/net/dsa/b53/b53_common.c
@@ -1835,7 +1835,8 @@ static int b53_arl_op(struct b53_device
 
 	/* Perform a read for the given MAC and VID */
 	b53_write48(dev, B53_ARLIO_PAGE, B53_MAC_ADDR_IDX, mac);
-	b53_write16(dev, B53_ARLIO_PAGE, B53_VLAN_ID_IDX, vid);
+	if (!is5325m(dev))
+		b53_write16(dev, B53_ARLIO_PAGE, B53_VLAN_ID_IDX, vid);
 
 	/* Issue a read operation for this MAC */
 	ret = b53_arl_rw_op(dev, 1);
@@ -2906,6 +2907,9 @@ static int b53_switch_init(struct b53_de
 		}
 	}
 
+	if (is5325e(dev))
+		dev->num_arl_buckets = 512;
+
 	dev->num_ports = fls(dev->enabled_ports);
 
 	dev->ds->num_ports = min_t(unsigned int, dev->num_ports, DSA_MAX_PORTS);
@@ -3007,10 +3011,24 @@ int b53_switch_detect(struct b53_device
 		b53_write16(dev, B53_VLAN_PAGE, B53_VLAN_TABLE_ACCESS_25, 0xf);
 		b53_read16(dev, B53_VLAN_PAGE, B53_VLAN_TABLE_ACCESS_25, &tmp);
 
-		if (tmp == 0xf)
+		if (tmp == 0xf) {
+			u32 phy_id;
+			int val;
+
 			dev->chip_id = BCM5325_DEVICE_ID;
-		else
+
+			val = b53_phy_read16(dev->ds, 0, MII_PHYSID1);
+			phy_id = (val & 0xffff) << 16;
+			val = b53_phy_read16(dev->ds, 0, MII_PHYSID2);
+			phy_id |= (val & 0xfff0);
+
+			if (phy_id == 0x00406330)
+				dev->variant_id = B53_VARIANT_5325M;
+			else if (phy_id == 0x0143bc30)
+				dev->variant_id = B53_VARIANT_5325E;
+		} else {
 			dev->chip_id = BCM5365_DEVICE_ID;
+		}
 		break;
 	case BCM5389_DEVICE_ID:
 	case BCM5395_DEVICE_ID:
--- a/drivers/net/dsa/b53/b53_priv.h
+++ b/drivers/net/dsa/b53/b53_priv.h
@@ -84,6 +84,12 @@ enum {
 	BCM53134_DEVICE_ID = 0x5075,
 };
 
+enum b53_variant_id {
+	B53_VARIANT_NONE = 0,
+	B53_VARIANT_5325E,
+	B53_VARIANT_5325M,
+};
+
 struct b53_pcs {
 	struct phylink_pcs pcs;
 	struct b53_device *dev;
@@ -118,6 +124,7 @@ struct b53_device {
 
 	/* chip specific data */
 	u32 chip_id;
+	enum b53_variant_id variant_id;
 	u8 core_rev;
 	u8 vta_regs[3];
 	u8 duplex_reg;
@@ -165,6 +172,18 @@ static inline int is5325(struct b53_devi
 	return dev->chip_id == BCM5325_DEVICE_ID;
 }
 
+static inline int is5325e(struct b53_device *dev)
+{
+	return is5325(dev) &&
+		dev->variant_id == B53_VARIANT_5325E;
+}
+
+static inline int is5325m(struct b53_device *dev)
+{
+	return is5325(dev) &&
+		dev->variant_id == B53_VARIANT_5325M;
+}
+
 static inline int is5365(struct b53_device *dev)
 {
 #ifdef CONFIG_BCM47XX
