From 0bea93fdbaf8675b7e8124bdcaf51497dcc8bcfa Mon Sep 17 00:00:00 2001
From: Heiner Kallweit <hkallweit1@gmail.com>
Date: Mon, 3 Feb 2025 21:41:36 +0100
Subject: [PATCH] net: phy: realtek: use string choices helpers

Use string choices helpers to simplify the code.

Reported-by: kernel test robot <lkp@intel.com>
Closes: https://lore.kernel.org/oe-kbuild-all/202501190707.qQS8PGHW-lkp@intel.com/
Signed-off-by: Heiner Kallweit <hkallweit1@gmail.com>
Reviewed-by: Simon Horman <horms@kernel.org>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/phy/realtek/realtek_main.c | 9 +++++----
 1 file changed, 5 insertions(+), 4 deletions(-)

--- a/drivers/net/phy/realtek/realtek_main.c
+++ b/drivers/net/phy/realtek/realtek_main.c
@@ -13,6 +13,7 @@
 #include <linux/module.h>
 #include <linux/delay.h>
 #include <linux/clk.h>
+#include <linux/string_choices.h>
 
 #include "realtek.h"
 
@@ -422,11 +423,11 @@ static int rtl8211f_config_init(struct p
 	} else if (ret) {
 		dev_dbg(dev,
 			"%s 2ns TX delay (and changing the value from pin-strapping RXD1 or the bootloader)\n",
-			val_txdly ? "Enabling" : "Disabling");
+			str_enable_disable(val_txdly));
 	} else {
 		dev_dbg(dev,
 			"2ns TX delay was already %s (by pin-strapping RXD1 or bootloader configuration)\n",
-			val_txdly ? "enabled" : "disabled");
+			str_enabled_disabled(val_txdly));
 	}
 
 	ret = phy_modify_paged_changed(phydev, 0xd08, 0x15, RTL8211F_RX_DELAY,
@@ -437,11 +438,11 @@ static int rtl8211f_config_init(struct p
 	} else if (ret) {
 		dev_dbg(dev,
 			"%s 2ns RX delay (and changing the value from pin-strapping RXD0 or the bootloader)\n",
-			val_rxdly ? "Enabling" : "Disabling");
+			str_enable_disable(val_rxdly));
 	} else {
 		dev_dbg(dev,
 			"2ns RX delay was already %s (by pin-strapping RXD0 or bootloader configuration)\n",
-			val_rxdly ? "enabled" : "disabled");
+			str_enabled_disabled(val_rxdly));
 	}
 
 	if (priv->has_phycr2) {
