From 34e5ededf4b8ad4c9e58f0cab8596e26c8fa59a2 Mon Sep 17 00:00:00 2001
From: Heiner Kallweit <hkallweit1@gmail.com>
Date: Wed, 12 Mar 2025 20:21:42 +0100
Subject: [PATCH] r8169: switch away from deprecated pcim_iomap_table

Avoid using deprecated pcim_iomap_table by switching to
pcim_iomap_region.

Signed-off-by: Heiner Kallweit <hkallweit1@gmail.com>
Reviewed-by: Jacob Keller <jacob.e.keller@intel.com>
Reviewed-by: Simon Horman <horms@kernel.org>
Link: https://patch.msgid.link/a36b4cf3-c792-40fa-8164-5dc9d5f14dd0@gmail.com
Signed-off-by: Paolo Abeni <pabeni@redhat.com>
---
 drivers/net/ethernet/realtek/r8169_main.c | 9 ++++-----
 1 file changed, 4 insertions(+), 5 deletions(-)

--- a/drivers/net/ethernet/realtek/r8169_main.c
+++ b/drivers/net/ethernet/realtek/r8169_main.c
@@ -5471,11 +5471,10 @@ static int rtl_init_one(struct pci_dev *
 	if (region < 0)
 		return dev_err_probe(&pdev->dev, -ENODEV, "no MMIO resource found\n");
 
-	rc = pcim_iomap_regions(pdev, BIT(region), KBUILD_MODNAME);
-	if (rc < 0)
-		return dev_err_probe(&pdev->dev, rc, "cannot remap MMIO, aborting\n");
-
-	tp->mmio_addr = pcim_iomap_table(pdev)[region];
+	tp->mmio_addr = pcim_iomap_region(pdev, region, KBUILD_MODNAME);
+	if (IS_ERR(tp->mmio_addr))
+		return dev_err_probe(&pdev->dev, PTR_ERR(tp->mmio_addr),
+				     "cannot remap MMIO, aborting\n");
 
 	txconfig = RTL_R32(tp, TxConfig);
 	if (txconfig == ~0U)
