From: Felix Fietkau <nbd@nbd.name>
Date: Mon, 21 Mar 2022 20:39:59 +0100
Subject: [PATCH] net: ethernet: mtk_eth_soc: enable threaded NAPI

This can improve performance under load by ensuring that NAPI processing is
not pinned on CPU 0.

Signed-off-by: Felix Fietkau <nbd@nbd.name>
---

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -5148,6 +5148,8 @@ static int mtk_probe(struct platform_dev
 		dev_err(eth->dev, "failed to allocated dummy device\n");
 		goto err_unreg_netdev;
 	}
+	eth->dummy_dev->threaded = 1;
+	strcpy(eth->dummy_dev->name, "mtk_eth");
 	netif_napi_add(eth->dummy_dev, &eth->tx_napi, mtk_napi_tx);
 	netif_napi_add(eth->dummy_dev, &eth->rx_napi, mtk_napi_rx);
 
