From 12a3ccb90a3e88ac60ccb06ea3e5aa1eabe565ac Mon Sep 17 00:00:00 2001
From: Daniel Golle <daniel@makrotopia.org>
Date: Wed, 4 Mar 2026 01:32:35 +0000
Subject: [PATCH 7/8] mediatek: mt7988: add RNG node

Add node representing the hardware random number generator
found in the MediaTek MT7988 SoC family to the corresponding
device tree.

Signed-off-by: Daniel Golle <daniel@makrotopia.org>
---
 arch/arm/dts/mt7988.dtsi | 4 ++++
 1 file changed, 4 insertions(+)

--- a/arch/arm/dts/mt7988.dtsi
+++ b/arch/arm/dts/mt7988.dtsi
@@ -92,6 +92,10 @@
 		reg = <0 0x8000000 0 0x1000>;
 	};
 
+	rng {
+		compatible = "mediatek,mt7988-rng";
+	};
+
 	timer {
 		compatible = "arm,armv8-timer";
 		interrupt-parent = <&gic>;
