From 42ffd5ad8caf672035084c054a707fff9fbc83cd Mon Sep 17 00:00:00 2001
From: Christian Marangi <ansuelsmth@gmail.com>
Date: Tue, 30 Sep 2025 22:15:15 +0200
Subject: [PATCH 15/29] dt-bindings: clock: airoha: Document support for AN7583
 clock

Document support for Airoha AN7583 clock. This is based on the EN7523
clock schema with the new requirement of the "airoha,chip-scu"
(previously optional for EN7581).

Add additional binding for additional clock and reset lines.

Signed-off-by: Christian Marangi <ansuelsmth@gmail.com>
---
 dts/upstream/include/dt-bindings/clock/en7523-clk.h | 3 +++
 1 file changed, 3 insertions(+)

diff --git a/dts/upstream/include/dt-bindings/clock/en7523-clk.h b/dts/upstream/include/dt-bindings/clock/en7523-clk.h
index edfa64045f5..0fbbcb7b1b2 100644
--- a/dts/upstream/include/dt-bindings/clock/en7523-clk.h
+++ b/dts/upstream/include/dt-bindings/clock/en7523-clk.h
@@ -14,4 +14,7 @@
 
 #define EN7581_CLK_EMMC		8
 
+#define AN7583_CLK_MDIO0	9
+#define AN7583_CLK_MDIO1	10
+
 #endif /* _DT_BINDINGS_CLOCK_AIROHA_EN7523_H_ */
-- 
2.53.0

