From c721a0c1076d30958ab96f3dd209f7d92c10f750 Mon Sep 17 00:00:00 2001
From: Mikhail Kshevetskiy <mikhail.kshevetskiy@iopsys.eu>
Date: Mon, 27 Apr 2026 15:30:41 +0300
Subject: [PATCH 09/29] configs: airoha: an7581: enable pinctrl/gpio support

This enables AN7581 pin controller and gpio driver.
Defconfig was minimized with 'make savedefconfig'.

Signed-off-by: Mikhail Kshevetskiy <mikhail.kshevetskiy@iopsys.eu>
Reviewed-by: David Lechner <dlechner@baylibre.com>
---
 configs/an7581_evb_defconfig | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/configs/an7581_evb_defconfig b/configs/an7581_evb_defconfig
index 07569fa0a4e..a615994cc76 100644
--- a/configs/an7581_evb_defconfig
+++ b/configs/an7581_evb_defconfig
@@ -72,7 +72,7 @@ CONFIG_PCS_AIROHA_AN7581=y
 CONFIG_AIROHA_ETH=y
 CONFIG_PHY=y
 CONFIG_PINCTRL=y
-CONFIG_PINCONF=y
+CONFIG_PINCTRL_AIROHA_AN7581=y
 CONFIG_POWER_DOMAIN=y
 CONFIG_DM_REGULATOR=y
 CONFIG_DM_REGULATOR_FIXED=y
-- 
2.53.0

