From caac69565748349a3e532130a891e18dd5c36c5e Mon Sep 17 00:00:00 2001
From: Daniel Golle <daniel@makrotopia.org>
Date: Thu, 20 Jul 2023 17:36:44 +0100
Subject: [PATCH 8/8] mmc: block: set GENHD_FL_NVMEM

Set flag to consider MMC block devices as NVMEM providers.

Signed-off-by: Daniel Golle <daniel@makrotopia.org>
---
 drivers/mmc/core/block.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/mmc/core/block.c
+++ b/drivers/mmc/core/block.c
@@ -2607,6 +2607,7 @@ static struct mmc_blk_data *mmc_blk_allo
 	md->disk->major	= MMC_BLOCK_MAJOR;
 	md->disk->minors = perdev_minors;
 	md->disk->first_minor = devidx * perdev_minors;
+	md->disk->flags = GENHD_FL_NVMEM;
 	md->disk->fops = &mmc_bdops;
 	md->disk->private_data = md;
 	md->parent = parent;
