From c0898e6881f964ca831c407c7019cd7f307d4368 Mon Sep 17 00:00:00 2001
From: Marcin Juszkiewicz <mjuszkiewicz@redhat.com>
Date: Tue, 25 Mar 2025 20:51:47 +0100
Subject: [PATCH] arm64: dts: rockchip: enable HDMI sound on FriendlyElec
 NanoPC-T6

We have both video outputs showing pixels, time to play some noise.

Signed-off-by: Marcin Juszkiewicz <mjuszkiewicz@redhat.com>
Link: https://lore.kernel.org/r/20250325-nanopc-t6-hdmi-v1-2-299a2ed45878@redhat.com
Signed-off-by: Heiko Stuebner <heiko@sntech.de>
---
 .../arm64/boot/dts/rockchip/rk3588-nanopc-t6.dtsi | 15 +++++++++++++++
 1 file changed, 15 insertions(+)

--- a/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dtsi
@@ -371,6 +371,9 @@
 	};
 };
 
+&hdmi0_sound {
+	status = "okay";
+};
 
 &hdmi1 {
 	status = "okay";
@@ -388,6 +391,10 @@
 	};
 };
 
+&hdmi1_sound {
+	status = "okay";
+};
+
 &hdptxphy0 {
 	status = "okay";
 };
@@ -563,6 +570,14 @@
 	};
 };
 
+&i2s5_8ch {
+	status = "okay";
+};
+
+&i2s6_8ch {
+	status = "okay";
+};
+
 &pcie2x1l0 {
 	reset-gpios = <&gpio4 RK_PB3 GPIO_ACTIVE_HIGH>;
 	vpcie3v3-supply = <&vcc_3v3_pcie20>;
