From 8f0aecf2957e7dba78603544368846133bf6d22e Mon Sep 17 00:00:00 2001
From: Rustam Adilov <adilov@disroot.org>
Date: Thu, 5 Mar 2026 21:11:06 +0500
Subject: gpio: realtek-otto: add rtl9607 support

The RTL9607C SoC has support for 3 GPIO banks with 32 GPIOs each and
the port order is reversed just like in RTL930x.

Signed-off-by: Rustam Adilov <adilov@disroot.org>
Reviewed-by: Sander Vanheule <sander@svanheule.net>
Link: https://patch.msgid.link/20260305161106.15999-3-adilov@disroot.org
Signed-off-by: Bartosz Golaszewski <bartosz.golaszewski@oss.qualcomm.com>
---
 drivers/gpio/gpio-realtek-otto.c | 4 ++++
 1 file changed, 4 insertions(+)

--- a/drivers/gpio/gpio-realtek-otto.c
+++ b/drivers/gpio/gpio-realtek-otto.c
@@ -351,6 +351,10 @@ static const struct of_device_id realtek
 	{
 		.compatible = "realtek,rtl9310-gpio",
 	},
+	{
+		.compatible = "realtek,rtl9607-gpio",
+		.data = (void *)GPIO_PORTS_REVERSED,
+	},
 	{}
 };
 MODULE_DEVICE_TABLE(of, realtek_gpio_of_match);
