From b60c86d305f46483d3ed0743e9ec97a76addcabc Mon Sep 17 00:00:00 2001
From: Nickey Yang <nickey.yang@rock-chips.com>
Date: Sun, 8 Sep 2024 14:55:00 +0000
Subject: [PATCH] drm/rockchip: dw_hdmi: Add phy_config for 594Mhz pixel clock

Add phy_config for 594Mhz pixel clock used for HDMI2.0 display modes.

Signed-off-by: Nickey Yang <nickey.yang@rock-chips.com>
Signed-off-by: Jonas Karlman <jonas@kwiboo.se>
Signed-off-by: Heiko Stuebner <heiko@sntech.de>
Link: https://patchwork.freedesktop.org/patch/msgid/20240908145511.3331451-4-jonas@kwiboo.se
---
 drivers/gpu/drm/rockchip/dw_hdmi-rockchip.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/gpu/drm/rockchip/dw_hdmi-rockchip.c
+++ b/drivers/gpu/drm/rockchip/dw_hdmi-rockchip.c
@@ -204,6 +204,7 @@ static const struct dw_hdmi_phy_config r
 	{ 74250000,  0x8009, 0x0004, 0x0272},
 	{ 165000000, 0x802b, 0x0004, 0x0209},
 	{ 297000000, 0x8039, 0x0005, 0x028d},
+	{ 594000000, 0x8039, 0x0000, 0x019d},
 	{ ~0UL,	     0x0000, 0x0000, 0x0000}
 };
 
