#config driver_global 'driver_global'
#	option user nut

#config driver 'upsname'
#	option driver usbhid-ups
#	option port auto
#	option enable_usb_serial 0

#config user
#	option username upsuser
#	option password upspassword
#	option actions optional-action
#	list instcmd optional-instant-command
#	option upsmon secondary|primary

#config listen_address
#	option address ::1
#	option port 3493

#config upsd 'upsd'
#	option maxage 15
#	option statepath /var/run/nut
#	option maxconn 1024
#	option runas nut
# NB: certificates only apply to SSL-enabled version
#       option certfile /usr/local/etc/upsd.pem
