From e8355c6b60adb6704c9fb863f380f2d7b457d82c Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Mon, 23 Mar 2020 18:34:01 +0000
Subject: [PATCH] media: hevc_ctrls: Add slice param dependent slice
 segment

Adds V4L2_HEVC_SLICE_PARAMS_FLAG_DEPENDENT_SLICE_SEGMENT define.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 include/media/hevc-ctrls.h | 1 +
 1 file changed, 1 insertion(+)

--- a/include/media/hevc-ctrls.h
+++ b/include/media/hevc-ctrls.h
@@ -162,6 +162,7 @@ struct v4l2_hevc_pred_weight_table {
 #define V4L2_HEVC_SLICE_PARAMS_FLAG_USE_INTEGER_MV		(1ULL << 6)
 #define V4L2_HEVC_SLICE_PARAMS_FLAG_SLICE_DEBLOCKING_FILTER_DISABLED (1ULL << 7)
 #define V4L2_HEVC_SLICE_PARAMS_FLAG_SLICE_LOOP_FILTER_ACROSS_SLICES_ENABLED (1ULL << 8)
+#define V4L2_HEVC_SLICE_PARAMS_FLAG_DEPENDENT_SLICE_SEGMENT	(1ULL << 9)
 
 struct v4l2_ctrl_hevc_slice_params {
 	__u32	bit_size;
